(kicad_pcb (version 20171130) (host pcbnew 5.0.2+dfsg1-1)
  (general
    (thickness 1.6)
    (drawings 138)
    (tracks 1389)
    (zones 0)
    (modules 234)
    (nets 203)
  )
  (page A4)
  (title_block
    (title "Igsoi board")
    (date 2019-12-31)
    (company "Ivan Shmakov")
  )
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.9)
    (trace_clearance 0.6805)
    (zone_clearance 0)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.9)
    (via_drill 0.5)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5.6 5.6)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010ec_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber-final"))
  )
  (net 0 "")
  (net 1 "/Attenuator A/RFin")
  (net 2 "/Low-pass A/FilterB")
  (net 3 "/Low-pass B/FilterB")
  (net 4 "/Attenuator B/RFin")
  (net 5 "Net-(C103-Pad1)")
  (net 6 "/Attenuator A/RFout")
  (net 7 "/Attenuator B/RFout")
  (net 8 "Net-(C104-Pad1)")
  (net 9 "Net-(C201-Pad1)")
  (net 10 "Net-(C201-Pad2)")
  (net 11 "Net-(C202-Pad1)")
  (net 12 "Net-(C204-Pad2)")
  (net 13 "Net-(C204-Pad1)")
  (net 14 "Net-(C205-Pad1)")
  (net 15 "Net-(C207-Pad2)")
  (net 16 "Net-(C207-Pad1)")
  (net 17 "Net-(C208-Pad1)")
  (net 18 GND)
  (net 19 "Net-(C301-Pad2)")
  (net 20 "Net-(C302-Pad2)")
  (net 21 "Net-(C302-Pad1)")
  (net 22 "Net-(C303-Pad2)")
  (net 23 "Net-(C304-Pad2)")
  (net 24 "Net-(C304-Pad1)")
  (net 25 "Net-(C305-Pad2)")
  (net 26 "Net-(C306-Pad2)")
  (net 27 "Net-(C306-Pad1)")
  (net 28 "Net-(C307-Pad2)")
  (net 29 "Net-(C308-Pad1)")
  (net 30 "Net-(C308-Pad2)")
  (net 31 "Net-(C309-Pad2)")
  (net 32 "Net-(C401-Pad1)")
  (net 33 "Net-(C401-Pad2)")
  (net 34 "Net-(C402-Pad1)")
  (net 35 "Net-(C404-Pad2)")
  (net 36 "Net-(C404-Pad1)")
  (net 37 "Net-(C405-Pad1)")
  (net 38 "Net-(C407-Pad2)")
  (net 39 "Net-(C407-Pad1)")
  (net 40 "Net-(C408-Pad1)")
  (net 41 "Net-(C501-Pad2)")
  (net 42 "Net-(C502-Pad2)")
  (net 43 "Net-(C502-Pad1)")
  (net 44 "Net-(C503-Pad2)")
  (net 45 "Net-(C504-Pad2)")
  (net 46 "Net-(C504-Pad1)")
  (net 47 "Net-(C505-Pad2)")
  (net 48 "Net-(C506-Pad2)")
  (net 49 "Net-(C506-Pad1)")
  (net 50 "Net-(C507-Pad2)")
  (net 51 "Net-(C508-Pad1)")
  (net 52 "Net-(C508-Pad2)")
  (net 53 "Net-(C509-Pad2)")
  (net 54 +12V)
  (net 55 "Net-(C604-Pad1)")
  (net 56 "Net-(C901-Pad2)")
  (net 57 "/Amplifier A/IN+")
  (net 58 "Net-(C902-Pad2)")
  (net 59 "/Amplifier A/IN-")
  (net 60 "Net-(C903-Pad2)")
  (net 61 "/Amplifier A/OUT+")
  (net 62 "Net-(C904-Pad1)")
  (net 63 "Net-(C905-Pad1)")
  (net 64 "/Amplifier A/OUT-")
  (net 65 "/Amplifier A/Vocm")
  (net 66 "/Amplifier B/IN+")
  (net 67 "Net-(C1101-Pad2)")
  (net 68 "Net-(C1102-Pad2)")
  (net 69 "Net-(C1103-Pad2)")
  (net 70 "/Amplifier B/IN-")
  (net 71 "Net-(C1104-Pad1)")
  (net 72 "/Amplifier B/OUT+")
  (net 73 "/Amplifier B/OUT-")
  (net 74 "Net-(C1105-Pad1)")
  (net 75 "/Amplifier B/Vocm")
  (net 76 "Net-(DA602-Pad4)")
  (net 77 "Net-(DA602-Pad5)")
  (net 78 "Net-(DA701-Pad20)")
  (net 79 "Net-(DA701-Pad19)")
  (net 80 "Net-(DA701-Pad17)")
  (net 81 "Net-(DA701-Pad16)")
  (net 82 "Net-(DA701-Pad8)")
  (net 83 "Net-(DA701-Pad7)")
  (net 84 "Net-(DA701-Pad15)")
  (net 85 /LE0)
  (net 86 /YSCK)
  (net 87 /YMOSI)
  (net 88 "Net-(DA701-Pad1)")
  (net 89 "/Control circuit/DO0")
  (net 90 "Net-(DA901-Pad7)")
  (net 91 "Net-(DA901-Pad6)")
  (net 92 "Net-(DA902-Pad6)")
  (net 93 "Net-(DA902-Pad7)")
  (net 94 "/Control circuit/DO1")
  (net 95 "Net-(DA1101-Pad7)")
  (net 96 "Net-(DA1101-Pad6)")
  (net 97 "Net-(DA1102-Pad6)")
  (net 98 "Net-(DA1102-Pad7)")
  (net 99 "Net-(DA1401-Pad1)")
  (net 100 /LE1)
  (net 101 "Net-(DA1401-Pad15)")
  (net 102 "Net-(DA1401-Pad7)")
  (net 103 "Net-(DA1401-Pad8)")
  (net 104 "Net-(DA1401-Pad16)")
  (net 105 "Net-(DA1401-Pad17)")
  (net 106 "Net-(DA1401-Pad19)")
  (net 107 "Net-(DA1401-Pad20)")
  (net 108 "Net-(DD701-Pad1)")
  (net 109 "Net-(DD701-Pad2)")
  (net 110 "Net-(DD701-Pad7)")
  (net 111 "Net-(DD701-Pad8)")
  (net 112 "Net-(DD701-Pad9)")
  (net 113 "Net-(DD701-Pad10)")
  (net 114 "Net-(DD701-Pad11)")
  (net 115 "Net-(DD701-Pad12)")
  (net 116 "Net-(DD701-Pad13)")
  (net 117 "Net-(DD701-Pad14)")
  (net 118 "Net-(DD701-Pad15)")
  (net 119 "Net-(DD701-Pad16)")
  (net 120 "Net-(DD701-Pad17)")
  (net 121 "Net-(DD701-Pad19)")
  (net 122 "Net-(DD701-Pad20)")
  (net 123 "Net-(DD701-Pad22)")
  (net 124 "Net-(DD701-Pad23)")
  (net 125 "Net-(DD701-Pad24)")
  (net 126 "Net-(DD701-Pad25)")
  (net 127 "Net-(DD701-Pad26)")
  (net 128 "Net-(DD701-Pad27)")
  (net 129 "Net-(DD701-Pad28)")
  (net 130 "/Control circuit/~RST")
  (net 131 "Net-(DD701-Pad30)")
  (net 132 "Net-(DD701-Pad31)")
  (net 133 "Net-(DD701-Pad32)")
  (net 134 "Net-(DD1301-Pad1)")
  (net 135 "Net-(DD1301-Pad2)")
  (net 136 "Net-(DD1301-Pad3)")
  (net 137 "Net-(DD1301-Pad4)")
  (net 138 "Net-(DD1301-Pad5)")
  (net 139 "Net-(DD1301-Pad6)")
  (net 140 "Net-(DD1301-Pad7)")
  (net 141 "/Face display/MISO")
  (net 142 "Net-(DD1301-Pad10)")
  (net 143 /LED)
  (net 144 "Net-(DD1301-Pad15)")
  (net 145 "/Amplifier A/+12V")
  (net 146 "/Amplifier A/RFin")
  (net 147 "Net-(K901-Pad3)")
  (net 148 "Net-(K901-Pad4)")
  (net 149 "/Amplifier A/AMPBYPASS")
  (net 150 "Net-(K901-Pad7)")
  (net 151 "/Coil cur. amps/O0A")
  (net 152 "/Coil cur. amps/O0B")
  (net 153 "Net-(K902-Pad7)")
  (net 154 "/Amplifier A/RFout")
  (net 155 "Net-(K902-Pad4)")
  (net 156 "Net-(K902-Pad3)")
  (net 157 "/Coil cur. amps/O1A")
  (net 158 "Net-(K1101-Pad7)")
  (net 159 "/Amplifier B/AMPBYPASS")
  (net 160 "/Amplifier B/RFin")
  (net 161 "Net-(K1101-Pad4)")
  (net 162 "Net-(K1101-Pad3)")
  (net 163 "/Amplifier B/RFout")
  (net 164 "Net-(K1102-Pad3)")
  (net 165 "Net-(K1102-Pad4)")
  (net 166 "Net-(K1102-Pad7)")
  (net 167 "/Coil cur. amps/O1B")
  (net 168 /SCK)
  (net 169 /MISO)
  (net 170 /MOSI)
  (net 171 /~CS)
  (net 172 "Net-(R1301-Pad1)")
  (net 173 "Net-(R1301-Pad2)")
  (net 174 "Net-(R1302-Pad2)")
  (net 175 "Net-(R1302-Pad1)")
  (net 176 "Net-(T902-Pad5)")
  (net 177 "Net-(T1102-Pad5)")
  (net 178 "Net-(R1301-Pad4)")
  (net 179 "Net-(R1301-Pad3)")
  (net 180 "Net-(R1302-Pad4)")
  (net 181 "Net-(R1302-Pad3)")
  (net 182 /~CS0)
  (net 183 /~CS1)
  (net 184 /~CS2)
  (net 185 /~CS3)
  (net 186 "Net-(X106-Pad2)")
  (net 187 "Net-(X107-Pad2)")
  (net 188 "/High-pass A/FilterA")
  (net 189 "Net-(X202-Pad2)")
  (net 190 "Net-(X203-Pad2)")
  (net 191 "/Low-pass A/FilterA")
  (net 192 "/High-pass B/FilterA")
  (net 193 "/Low-pass B/FilterA")
  (net 194 "Net-(XP103-Pad3)")
  (net 195 "Net-(X402-Pad2)")
  (net 196 "Net-(X403-Pad2)")
  (net 197 +3V3)
  (net 198 +3.3VA)
  (net 199 V+)
  (net 200 VDD)
  (net 201 +12VA)
  (net 202 "/Control circuit/RDY")
  (net_class Default "This is the default net class."
    (clearance 0.6805)
    (trace_width 0.9)
    (via_dia 0.9)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "/Amplifier A/AMPBYPASS")
    (add_net "/Amplifier A/RFin")
    (add_net "/Amplifier A/RFout")
    (add_net "/Amplifier B/AMPBYPASS")
    (add_net "/Amplifier B/RFin")
    (add_net "/Amplifier B/RFout")
    (add_net "/High-pass A/FilterA")
    (add_net "/High-pass B/FilterA")
    (add_net "/Low-pass A/FilterA")
    (add_net "/Low-pass A/FilterB")
    (add_net "/Low-pass B/FilterA")
    (add_net "/Low-pass B/FilterB")
    (add_net "Net-(C103-Pad1)")
    (add_net "Net-(C104-Pad1)")
    (add_net "Net-(C1101-Pad2)")
    (add_net "Net-(C1102-Pad2)")
    (add_net "Net-(C1103-Pad2)")
    (add_net "Net-(C1104-Pad1)")
    (add_net "Net-(C1105-Pad1)")
    (add_net "Net-(C201-Pad1)")
    (add_net "Net-(C201-Pad2)")
    (add_net "Net-(C202-Pad1)")
    (add_net "Net-(C204-Pad1)")
    (add_net "Net-(C204-Pad2)")
    (add_net "Net-(C205-Pad1)")
    (add_net "Net-(C207-Pad1)")
    (add_net "Net-(C207-Pad2)")
    (add_net "Net-(C208-Pad1)")
    (add_net "Net-(C301-Pad2)")
    (add_net "Net-(C302-Pad1)")
    (add_net "Net-(C302-Pad2)")
    (add_net "Net-(C303-Pad2)")
    (add_net "Net-(C304-Pad1)")
    (add_net "Net-(C304-Pad2)")
    (add_net "Net-(C305-Pad2)")
    (add_net "Net-(C306-Pad1)")
    (add_net "Net-(C306-Pad2)")
    (add_net "Net-(C307-Pad2)")
    (add_net "Net-(C308-Pad1)")
    (add_net "Net-(C308-Pad2)")
    (add_net "Net-(C309-Pad2)")
    (add_net "Net-(C401-Pad1)")
    (add_net "Net-(C401-Pad2)")
    (add_net "Net-(C402-Pad1)")
    (add_net "Net-(C404-Pad1)")
    (add_net "Net-(C404-Pad2)")
    (add_net "Net-(C405-Pad1)")
    (add_net "Net-(C407-Pad1)")
    (add_net "Net-(C407-Pad2)")
    (add_net "Net-(C408-Pad1)")
    (add_net "Net-(C501-Pad2)")
    (add_net "Net-(C502-Pad1)")
    (add_net "Net-(C502-Pad2)")
    (add_net "Net-(C503-Pad2)")
    (add_net "Net-(C504-Pad1)")
    (add_net "Net-(C504-Pad2)")
    (add_net "Net-(C505-Pad2)")
    (add_net "Net-(C506-Pad1)")
    (add_net "Net-(C506-Pad2)")
    (add_net "Net-(C507-Pad2)")
    (add_net "Net-(C508-Pad1)")
    (add_net "Net-(C508-Pad2)")
    (add_net "Net-(C509-Pad2)")
    (add_net "Net-(C901-Pad2)")
    (add_net "Net-(C902-Pad2)")
    (add_net "Net-(C903-Pad2)")
    (add_net "Net-(C904-Pad1)")
    (add_net "Net-(C905-Pad1)")
    (add_net "Net-(DA901-Pad6)")
    (add_net "Net-(DA901-Pad7)")
    (add_net "Net-(DA902-Pad6)")
    (add_net "Net-(DA902-Pad7)")
    (add_net "Net-(K1101-Pad3)")
    (add_net "Net-(K1101-Pad4)")
    (add_net "Net-(K1101-Pad7)")
    (add_net "Net-(K1102-Pad3)")
    (add_net "Net-(K1102-Pad4)")
    (add_net "Net-(K1102-Pad7)")
    (add_net "Net-(K901-Pad3)")
    (add_net "Net-(K901-Pad4)")
    (add_net "Net-(K901-Pad7)")
    (add_net "Net-(K902-Pad3)")
    (add_net "Net-(K902-Pad4)")
    (add_net "Net-(K902-Pad7)")
    (add_net "Net-(T1102-Pad5)")
    (add_net "Net-(T902-Pad5)")
    (add_net "Net-(X106-Pad2)")
    (add_net "Net-(X107-Pad2)")
    (add_net "Net-(X202-Pad2)")
    (add_net "Net-(X203-Pad2)")
    (add_net "Net-(X402-Pad2)")
    (add_net "Net-(X403-Pad2)")
    (add_net "Net-(XP103-Pad3)")
  )
  (net_class ComGnd ""
    (clearance 0.2)
    (trace_width 0.9)
    (via_dia 0.9)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (net_class ConThin ""
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12VA)
    (add_net "/Amplifier A/IN+")
    (add_net "/Amplifier A/IN-")
    (add_net "/Amplifier A/OUT+")
    (add_net "/Amplifier A/OUT-")
    (add_net "/Amplifier A/Vocm")
    (add_net "/Amplifier B/IN+")
    (add_net "/Amplifier B/IN-")
    (add_net "/Amplifier B/OUT+")
    (add_net "/Amplifier B/OUT-")
    (add_net "/Amplifier B/Vocm")
    (add_net "/Attenuator A/RFin")
    (add_net "/Attenuator A/RFout")
    (add_net "/Attenuator B/RFin")
    (add_net "/Attenuator B/RFout")
    (add_net "/Control circuit/DO0")
    (add_net "/Control circuit/DO1")
    (add_net "/Control circuit/RDY")
    (add_net /LE0)
    (add_net /LE1)
    (add_net /YMOSI)
    (add_net /YSCK)
    (add_net "Net-(C604-Pad1)")
    (add_net "Net-(DA1101-Pad6)")
    (add_net "Net-(DA1101-Pad7)")
    (add_net "Net-(DA1102-Pad6)")
    (add_net "Net-(DA1102-Pad7)")
    (add_net "Net-(DA1401-Pad1)")
    (add_net "Net-(DA1401-Pad15)")
    (add_net "Net-(DA1401-Pad16)")
    (add_net "Net-(DA1401-Pad17)")
    (add_net "Net-(DA1401-Pad19)")
    (add_net "Net-(DA1401-Pad20)")
    (add_net "Net-(DA1401-Pad7)")
    (add_net "Net-(DA1401-Pad8)")
    (add_net "Net-(DA602-Pad4)")
    (add_net "Net-(DA602-Pad5)")
    (add_net "Net-(DA701-Pad1)")
    (add_net "Net-(DA701-Pad15)")
    (add_net "Net-(DA701-Pad16)")
    (add_net "Net-(DA701-Pad17)")
    (add_net "Net-(DA701-Pad19)")
    (add_net "Net-(DA701-Pad20)")
    (add_net "Net-(DA701-Pad7)")
    (add_net "Net-(DA701-Pad8)")
    (add_net V+)
    (add_net VDD)
  )
  (net_class Control ""
    (clearance 0.25)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net "/Control circuit/~RST")
    (add_net "/Face display/MISO")
    (add_net /LED)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /SCK)
    (add_net /~CS)
    (add_net /~CS0)
    (add_net /~CS1)
    (add_net /~CS2)
    (add_net /~CS3)
    (add_net "Net-(DD1301-Pad1)")
    (add_net "Net-(DD1301-Pad10)")
    (add_net "Net-(DD1301-Pad15)")
    (add_net "Net-(DD1301-Pad2)")
    (add_net "Net-(DD1301-Pad3)")
    (add_net "Net-(DD1301-Pad4)")
    (add_net "Net-(DD1301-Pad5)")
    (add_net "Net-(DD1301-Pad6)")
    (add_net "Net-(DD1301-Pad7)")
    (add_net "Net-(DD701-Pad1)")
    (add_net "Net-(DD701-Pad10)")
    (add_net "Net-(DD701-Pad11)")
    (add_net "Net-(DD701-Pad12)")
    (add_net "Net-(DD701-Pad13)")
    (add_net "Net-(DD701-Pad14)")
    (add_net "Net-(DD701-Pad15)")
    (add_net "Net-(DD701-Pad16)")
    (add_net "Net-(DD701-Pad17)")
    (add_net "Net-(DD701-Pad19)")
    (add_net "Net-(DD701-Pad2)")
    (add_net "Net-(DD701-Pad20)")
    (add_net "Net-(DD701-Pad22)")
    (add_net "Net-(DD701-Pad23)")
    (add_net "Net-(DD701-Pad24)")
    (add_net "Net-(DD701-Pad25)")
    (add_net "Net-(DD701-Pad26)")
    (add_net "Net-(DD701-Pad27)")
    (add_net "Net-(DD701-Pad28)")
    (add_net "Net-(DD701-Pad30)")
    (add_net "Net-(DD701-Pad31)")
    (add_net "Net-(DD701-Pad32)")
    (add_net "Net-(DD701-Pad7)")
    (add_net "Net-(DD701-Pad8)")
    (add_net "Net-(DD701-Pad9)")
    (add_net "Net-(R1301-Pad1)")
    (add_net "Net-(R1301-Pad2)")
    (add_net "Net-(R1301-Pad3)")
    (add_net "Net-(R1301-Pad4)")
    (add_net "Net-(R1302-Pad1)")
    (add_net "Net-(R1302-Pad2)")
    (add_net "Net-(R1302-Pad3)")
    (add_net "Net-(R1302-Pad4)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.7)
    (via_dia 1)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +3.3VA)
    (add_net "/Amplifier A/+12V")
    (add_net "/Coil cur. amps/O0A")
    (add_net "/Coil cur. amps/O0B")
    (add_net "/Coil cur. amps/O1A")
    (add_net "/Coil cur. amps/O1B")
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 5E8EEFF8)
    (at 245 60)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965_Pad (at 0 3.8) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 18 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 5E8EF001)
    (at 245 140)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965_Pad (at 0 3.8) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 18 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 5E8EEFED)
    (at 75 60)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965_Pad (at 0 3.8) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 18 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965 (layer F.Cu) (tedit 5E8EEB4E)
    (at 64 107.5)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965 (at 0 3.8) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module custom-devices:Schroff-60807-181reversed (layer F.Cu) (tedit 5E26BA0D)
    (at 53.57 144.45)
    (fp_text reference X113 (at 0 3.7) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 -5.4) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module custom-devices:0.9w-5r-angle90 (layer F.Cu) (tedit 5E8C8800)
    (at 201.25 55 270)
    (fp_text reference REF** (at 0 0.5 270) (layer F.SilkS) hide)
    (fp_text value 0.9w-5r-angle90 (at 0 -0.5 270) (layer F.Fab))
    (pad 1 smd circle (at 5 -5 270) (size 0.9 0.9) (layers F.Cu)
      (net 160 "/Amplifier B/RFin"))
    (pad 1 smd custom (at 0 0 270) (size 0.9 0.9) (layers F.Cu)
      (net 160 "/Amplifier B/RFin") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_line (start 0 0) (end 0.00685 -0.26168) (width 0.9))
        (gr_line (start 0.00685 -0.26168) (end 0.02739 -0.52264) (width 0.9))
        (gr_line (start 0.02739 -0.52264) (end 0.06156 -0.78217) (width 0.9))
        (gr_line (start 0.06156 -0.78217) (end 0.10926 -1.03956) (width 0.9))
        (gr_line (start 0.10926 -1.03956) (end 0.17037 -1.2941) (width 0.9))
        (gr_line (start 0.17037 -1.2941) (end 0.24472 -1.54508) (width 0.9))
        (gr_line (start 0.24472 -1.54508) (end 0.3321 -1.79184) (width 0.9))
        (gr_line (start 0.3321 -1.79184) (end 0.43227 -2.03368) (width 0.9))
        (gr_line (start 0.43227 -2.03368) (end 0.54497 -2.26995) (width 0.9))
        (gr_line (start 0.54497 -2.26995) (end 0.66987 -2.5) (width 0.9))
        (gr_line (start 0.66987 -2.5) (end 0.80665 -2.7232) (width 0.9))
        (gr_line (start 0.80665 -2.7232) (end 0.95492 -2.93893) (width 0.9))
        (gr_line (start 0.95492 -2.93893) (end 1.11427 -3.1466) (width 0.9))
        (gr_line (start 1.11427 -3.1466) (end 1.28428 -3.34565) (width 0.9))
        (gr_line (start 1.28428 -3.34565) (end 1.46447 -3.53553) (width 0.9))
        (gr_line (start 1.46447 -3.53553) (end 1.65435 -3.71572) (width 0.9))
        (gr_line (start 1.65435 -3.71572) (end 1.8534 -3.88573) (width 0.9))
        (gr_line (start 1.8534 -3.88573) (end 2.06107 -4.04508) (width 0.9))
        (gr_line (start 2.06107 -4.04508) (end 2.2768 -4.19335) (width 0.9))
        (gr_line (start 2.2768 -4.19335) (end 2.5 -4.33013) (width 0.9))
        (gr_line (start 2.5 -4.33013) (end 2.73005 -4.45503) (width 0.9))
        (gr_line (start 2.73005 -4.45503) (end 2.96632 -4.56773) (width 0.9))
        (gr_line (start 2.96632 -4.56773) (end 3.20816 -4.6679) (width 0.9))
        (gr_line (start 3.20816 -4.6679) (end 3.45492 -4.75528) (width 0.9))
        (gr_line (start 3.45492 -4.75528) (end 3.7059 -4.82963) (width 0.9))
        (gr_line (start 3.7059 -4.82963) (end 3.96044 -4.89074) (width 0.9))
        (gr_line (start 3.96044 -4.89074) (end 4.21783 -4.93844) (width 0.9))
        (gr_line (start 4.21783 -4.93844) (end 4.47736 -4.97261) (width 0.9))
        (gr_line (start 4.47736 -4.97261) (end 4.73832 -4.99315) (width 0.9))
        (gr_line (start 4.73832 -4.99315) (end 5 -5) (width 0.9))
      ))
  )
  (module custom-devices:0.9w-5r-angle90 (layer F.Cu) (tedit 5E8C8800)
    (at 211.25 65 90)
    (fp_text reference REF** (at 0 0.5 90) (layer F.SilkS) hide)
    (fp_text value 0.9w-5r-angle90 (at 0 -0.5 90) (layer F.Fab))
    (pad 1 smd custom (at 0 0 90) (size 0.9 0.9) (layers F.Cu)
      (net 160 "/Amplifier B/RFin") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_line (start 0 0) (end 0.00685 -0.26168) (width 0.9))
        (gr_line (start 0.00685 -0.26168) (end 0.02739 -0.52264) (width 0.9))
        (gr_line (start 0.02739 -0.52264) (end 0.06156 -0.78217) (width 0.9))
        (gr_line (start 0.06156 -0.78217) (end 0.10926 -1.03956) (width 0.9))
        (gr_line (start 0.10926 -1.03956) (end 0.17037 -1.2941) (width 0.9))
        (gr_line (start 0.17037 -1.2941) (end 0.24472 -1.54508) (width 0.9))
        (gr_line (start 0.24472 -1.54508) (end 0.3321 -1.79184) (width 0.9))
        (gr_line (start 0.3321 -1.79184) (end 0.43227 -2.03368) (width 0.9))
        (gr_line (start 0.43227 -2.03368) (end 0.54497 -2.26995) (width 0.9))
        (gr_line (start 0.54497 -2.26995) (end 0.66987 -2.5) (width 0.9))
        (gr_line (start 0.66987 -2.5) (end 0.80665 -2.7232) (width 0.9))
        (gr_line (start 0.80665 -2.7232) (end 0.95492 -2.93893) (width 0.9))
        (gr_line (start 0.95492 -2.93893) (end 1.11427 -3.1466) (width 0.9))
        (gr_line (start 1.11427 -3.1466) (end 1.28428 -3.34565) (width 0.9))
        (gr_line (start 1.28428 -3.34565) (end 1.46447 -3.53553) (width 0.9))
        (gr_line (start 1.46447 -3.53553) (end 1.65435 -3.71572) (width 0.9))
        (gr_line (start 1.65435 -3.71572) (end 1.8534 -3.88573) (width 0.9))
        (gr_line (start 1.8534 -3.88573) (end 2.06107 -4.04508) (width 0.9))
        (gr_line (start 2.06107 -4.04508) (end 2.2768 -4.19335) (width 0.9))
        (gr_line (start 2.2768 -4.19335) (end 2.5 -4.33013) (width 0.9))
        (gr_line (start 2.5 -4.33013) (end 2.73005 -4.45503) (width 0.9))
        (gr_line (start 2.73005 -4.45503) (end 2.96632 -4.56773) (width 0.9))
        (gr_line (start 2.96632 -4.56773) (end 3.20816 -4.6679) (width 0.9))
        (gr_line (start 3.20816 -4.6679) (end 3.45492 -4.75528) (width 0.9))
        (gr_line (start 3.45492 -4.75528) (end 3.7059 -4.82963) (width 0.9))
        (gr_line (start 3.7059 -4.82963) (end 3.96044 -4.89074) (width 0.9))
        (gr_line (start 3.96044 -4.89074) (end 4.21783 -4.93844) (width 0.9))
        (gr_line (start 4.21783 -4.93844) (end 4.47736 -4.97261) (width 0.9))
        (gr_line (start 4.47736 -4.97261) (end 4.73832 -4.99315) (width 0.9))
        (gr_line (start 4.73832 -4.99315) (end 5 -5) (width 0.9))
      ))
    (pad 1 smd circle (at 5 -5 90) (size 0.9 0.9) (layers F.Cu)
      (net 160 "/Amplifier B/RFin"))
  )
  (module custom-devices:0.9w-5r-angle90 (layer F.Cu) (tedit 5E8C87C8)
    (at 230 65 270)
    (fp_text reference REF** (at 0 0.5 270) (layer F.SilkS) hide)
    (fp_text value 0.9w-5r-angle90 (at 0 -0.5 270) (layer F.Fab))
    (pad 1 smd circle (at 5 -5 270) (size 0.9 0.9) (layers F.Cu)
      (net 3 "/Low-pass B/FilterB"))
    (pad 1 smd custom (at 0 0 270) (size 0.9 0.9) (layers F.Cu)
      (net 3 "/Low-pass B/FilterB") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_line (start 0 0) (end 0.00685 -0.26168) (width 0.9))
        (gr_line (start 0.00685 -0.26168) (end 0.02739 -0.52264) (width 0.9))
        (gr_line (start 0.02739 -0.52264) (end 0.06156 -0.78217) (width 0.9))
        (gr_line (start 0.06156 -0.78217) (end 0.10926 -1.03956) (width 0.9))
        (gr_line (start 0.10926 -1.03956) (end 0.17037 -1.2941) (width 0.9))
        (gr_line (start 0.17037 -1.2941) (end 0.24472 -1.54508) (width 0.9))
        (gr_line (start 0.24472 -1.54508) (end 0.3321 -1.79184) (width 0.9))
        (gr_line (start 0.3321 -1.79184) (end 0.43227 -2.03368) (width 0.9))
        (gr_line (start 0.43227 -2.03368) (end 0.54497 -2.26995) (width 0.9))
        (gr_line (start 0.54497 -2.26995) (end 0.66987 -2.5) (width 0.9))
        (gr_line (start 0.66987 -2.5) (end 0.80665 -2.7232) (width 0.9))
        (gr_line (start 0.80665 -2.7232) (end 0.95492 -2.93893) (width 0.9))
        (gr_line (start 0.95492 -2.93893) (end 1.11427 -3.1466) (width 0.9))
        (gr_line (start 1.11427 -3.1466) (end 1.28428 -3.34565) (width 0.9))
        (gr_line (start 1.28428 -3.34565) (end 1.46447 -3.53553) (width 0.9))
        (gr_line (start 1.46447 -3.53553) (end 1.65435 -3.71572) (width 0.9))
        (gr_line (start 1.65435 -3.71572) (end 1.8534 -3.88573) (width 0.9))
        (gr_line (start 1.8534 -3.88573) (end 2.06107 -4.04508) (width 0.9))
        (gr_line (start 2.06107 -4.04508) (end 2.2768 -4.19335) (width 0.9))
        (gr_line (start 2.2768 -4.19335) (end 2.5 -4.33013) (width 0.9))
        (gr_line (start 2.5 -4.33013) (end 2.73005 -4.45503) (width 0.9))
        (gr_line (start 2.73005 -4.45503) (end 2.96632 -4.56773) (width 0.9))
        (gr_line (start 2.96632 -4.56773) (end 3.20816 -4.6679) (width 0.9))
        (gr_line (start 3.20816 -4.6679) (end 3.45492 -4.75528) (width 0.9))
        (gr_line (start 3.45492 -4.75528) (end 3.7059 -4.82963) (width 0.9))
        (gr_line (start 3.7059 -4.82963) (end 3.96044 -4.89074) (width 0.9))
        (gr_line (start 3.96044 -4.89074) (end 4.21783 -4.93844) (width 0.9))
        (gr_line (start 4.21783 -4.93844) (end 4.47736 -4.97261) (width 0.9))
        (gr_line (start 4.47736 -4.97261) (end 4.73832 -4.99315) (width 0.9))
        (gr_line (start 4.73832 -4.99315) (end 5 -5) (width 0.9))
      ))
  )
  (module custom-devices:0.9w-5r-angle90 (layer F.Cu) (tedit 5E8C87C8)
    (at 235 88 180)
    (fp_text reference REF** (at 0 0.5 180) (layer F.SilkS) hide)
    (fp_text value 0.9w-5r-angle90 (at 0 -0.5 180) (layer F.Fab))
    (pad 1 smd custom (at 0 0 180) (size 0.9 0.9) (layers F.Cu)
      (net 3 "/Low-pass B/FilterB") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_line (start 0 0) (end 0.00685 -0.26168) (width 0.9))
        (gr_line (start 0.00685 -0.26168) (end 0.02739 -0.52264) (width 0.9))
        (gr_line (start 0.02739 -0.52264) (end 0.06156 -0.78217) (width 0.9))
        (gr_line (start 0.06156 -0.78217) (end 0.10926 -1.03956) (width 0.9))
        (gr_line (start 0.10926 -1.03956) (end 0.17037 -1.2941) (width 0.9))
        (gr_line (start 0.17037 -1.2941) (end 0.24472 -1.54508) (width 0.9))
        (gr_line (start 0.24472 -1.54508) (end 0.3321 -1.79184) (width 0.9))
        (gr_line (start 0.3321 -1.79184) (end 0.43227 -2.03368) (width 0.9))
        (gr_line (start 0.43227 -2.03368) (end 0.54497 -2.26995) (width 0.9))
        (gr_line (start 0.54497 -2.26995) (end 0.66987 -2.5) (width 0.9))
        (gr_line (start 0.66987 -2.5) (end 0.80665 -2.7232) (width 0.9))
        (gr_line (start 0.80665 -2.7232) (end 0.95492 -2.93893) (width 0.9))
        (gr_line (start 0.95492 -2.93893) (end 1.11427 -3.1466) (width 0.9))
        (gr_line (start 1.11427 -3.1466) (end 1.28428 -3.34565) (width 0.9))
        (gr_line (start 1.28428 -3.34565) (end 1.46447 -3.53553) (width 0.9))
        (gr_line (start 1.46447 -3.53553) (end 1.65435 -3.71572) (width 0.9))
        (gr_line (start 1.65435 -3.71572) (end 1.8534 -3.88573) (width 0.9))
        (gr_line (start 1.8534 -3.88573) (end 2.06107 -4.04508) (width 0.9))
        (gr_line (start 2.06107 -4.04508) (end 2.2768 -4.19335) (width 0.9))
        (gr_line (start 2.2768 -4.19335) (end 2.5 -4.33013) (width 0.9))
        (gr_line (start 2.5 -4.33013) (end 2.73005 -4.45503) (width 0.9))
        (gr_line (start 2.73005 -4.45503) (end 2.96632 -4.56773) (width 0.9))
        (gr_line (start 2.96632 -4.56773) (end 3.20816 -4.6679) (width 0.9))
        (gr_line (start 3.20816 -4.6679) (end 3.45492 -4.75528) (width 0.9))
        (gr_line (start 3.45492 -4.75528) (end 3.7059 -4.82963) (width 0.9))
        (gr_line (start 3.7059 -4.82963) (end 3.96044 -4.89074) (width 0.9))
        (gr_line (start 3.96044 -4.89074) (end 4.21783 -4.93844) (width 0.9))
        (gr_line (start 4.21783 -4.93844) (end 4.47736 -4.97261) (width 0.9))
        (gr_line (start 4.47736 -4.97261) (end 4.73832 -4.99315) (width 0.9))
        (gr_line (start 4.73832 -4.99315) (end 5 -5) (width 0.9))
      ))
    (pad 1 smd circle (at 5 -5 180) (size 0.9 0.9) (layers F.Cu)
      (net 3 "/Low-pass B/FilterB"))
  )
  (module custom-devices:0.9w-5r-angle90 (layer F.Cu) (tedit 5E8C86AF)
    (at 211.5 135 90)
    (fp_text reference REF** (at 0 0.5 90) (layer F.SilkS) hide)
    (fp_text value 0.9w-5r-angle90 (at 0 -0.5 90) (layer F.Fab))
    (pad 1 smd custom (at 0 0 90) (size 0.9 0.9) (layers F.Cu)
      (net 146 "/Amplifier A/RFin") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_line (start 0 0) (end 0.00685 -0.26168) (width 0.9))
        (gr_line (start 0.00685 -0.26168) (end 0.02739 -0.52264) (width 0.9))
        (gr_line (start 0.02739 -0.52264) (end 0.06156 -0.78217) (width 0.9))
        (gr_line (start 0.06156 -0.78217) (end 0.10926 -1.03956) (width 0.9))
        (gr_line (start 0.10926 -1.03956) (end 0.17037 -1.2941) (width 0.9))
        (gr_line (start 0.17037 -1.2941) (end 0.24472 -1.54508) (width 0.9))
        (gr_line (start 0.24472 -1.54508) (end 0.3321 -1.79184) (width 0.9))
        (gr_line (start 0.3321 -1.79184) (end 0.43227 -2.03368) (width 0.9))
        (gr_line (start 0.43227 -2.03368) (end 0.54497 -2.26995) (width 0.9))
        (gr_line (start 0.54497 -2.26995) (end 0.66987 -2.5) (width 0.9))
        (gr_line (start 0.66987 -2.5) (end 0.80665 -2.7232) (width 0.9))
        (gr_line (start 0.80665 -2.7232) (end 0.95492 -2.93893) (width 0.9))
        (gr_line (start 0.95492 -2.93893) (end 1.11427 -3.1466) (width 0.9))
        (gr_line (start 1.11427 -3.1466) (end 1.28428 -3.34565) (width 0.9))
        (gr_line (start 1.28428 -3.34565) (end 1.46447 -3.53553) (width 0.9))
        (gr_line (start 1.46447 -3.53553) (end 1.65435 -3.71572) (width 0.9))
        (gr_line (start 1.65435 -3.71572) (end 1.8534 -3.88573) (width 0.9))
        (gr_line (start 1.8534 -3.88573) (end 2.06107 -4.04508) (width 0.9))
        (gr_line (start 2.06107 -4.04508) (end 2.2768 -4.19335) (width 0.9))
        (gr_line (start 2.2768 -4.19335) (end 2.5 -4.33013) (width 0.9))
        (gr_line (start 2.5 -4.33013) (end 2.73005 -4.45503) (width 0.9))
        (gr_line (start 2.73005 -4.45503) (end 2.96632 -4.56773) (width 0.9))
        (gr_line (start 2.96632 -4.56773) (end 3.20816 -4.6679) (width 0.9))
        (gr_line (start 3.20816 -4.6679) (end 3.45492 -4.75528) (width 0.9))
        (gr_line (start 3.45492 -4.75528) (end 3.7059 -4.82963) (width 0.9))
        (gr_line (start 3.7059 -4.82963) (end 3.96044 -4.89074) (width 0.9))
        (gr_line (start 3.96044 -4.89074) (end 4.21783 -4.93844) (width 0.9))
        (gr_line (start 4.21783 -4.93844) (end 4.47736 -4.97261) (width 0.9))
        (gr_line (start 4.47736 -4.97261) (end 4.73832 -4.99315) (width 0.9))
        (gr_line (start 4.73832 -4.99315) (end 5 -5) (width 0.9))
      ))
    (pad 1 smd circle (at 5 -5 90) (size 0.9 0.9) (layers F.Cu)
      (net 146 "/Amplifier A/RFin"))
  )
  (module custom-devices:0.9w-5r-angle90 (layer F.Cu) (tedit 5E8C867B)
    (at 230 108 270)
    (fp_text reference REF** (at 0 0.5 270) (layer F.SilkS) hide)
    (fp_text value 0.9w-5r-angle90 (at 0 -0.5 270) (layer F.Fab))
    (pad 1 smd circle (at 5 -5 270) (size 0.9 0.9) (layers F.Cu)
      (net 2 "/Low-pass A/FilterB"))
    (pad 1 smd custom (at 0 0 270) (size 0.9 0.9) (layers F.Cu)
      (net 2 "/Low-pass A/FilterB") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_line (start 0 0) (end 0.00685 -0.26168) (width 0.9))
        (gr_line (start 0.00685 -0.26168) (end 0.02739 -0.52264) (width 0.9))
        (gr_line (start 0.02739 -0.52264) (end 0.06156 -0.78217) (width 0.9))
        (gr_line (start 0.06156 -0.78217) (end 0.10926 -1.03956) (width 0.9))
        (gr_line (start 0.10926 -1.03956) (end 0.17037 -1.2941) (width 0.9))
        (gr_line (start 0.17037 -1.2941) (end 0.24472 -1.54508) (width 0.9))
        (gr_line (start 0.24472 -1.54508) (end 0.3321 -1.79184) (width 0.9))
        (gr_line (start 0.3321 -1.79184) (end 0.43227 -2.03368) (width 0.9))
        (gr_line (start 0.43227 -2.03368) (end 0.54497 -2.26995) (width 0.9))
        (gr_line (start 0.54497 -2.26995) (end 0.66987 -2.5) (width 0.9))
        (gr_line (start 0.66987 -2.5) (end 0.80665 -2.7232) (width 0.9))
        (gr_line (start 0.80665 -2.7232) (end 0.95492 -2.93893) (width 0.9))
        (gr_line (start 0.95492 -2.93893) (end 1.11427 -3.1466) (width 0.9))
        (gr_line (start 1.11427 -3.1466) (end 1.28428 -3.34565) (width 0.9))
        (gr_line (start 1.28428 -3.34565) (end 1.46447 -3.53553) (width 0.9))
        (gr_line (start 1.46447 -3.53553) (end 1.65435 -3.71572) (width 0.9))
        (gr_line (start 1.65435 -3.71572) (end 1.8534 -3.88573) (width 0.9))
        (gr_line (start 1.8534 -3.88573) (end 2.06107 -4.04508) (width 0.9))
        (gr_line (start 2.06107 -4.04508) (end 2.2768 -4.19335) (width 0.9))
        (gr_line (start 2.2768 -4.19335) (end 2.5 -4.33013) (width 0.9))
        (gr_line (start 2.5 -4.33013) (end 2.73005 -4.45503) (width 0.9))
        (gr_line (start 2.73005 -4.45503) (end 2.96632 -4.56773) (width 0.9))
        (gr_line (start 2.96632 -4.56773) (end 3.20816 -4.6679) (width 0.9))
        (gr_line (start 3.20816 -4.6679) (end 3.45492 -4.75528) (width 0.9))
        (gr_line (start 3.45492 -4.75528) (end 3.7059 -4.82963) (width 0.9))
        (gr_line (start 3.7059 -4.82963) (end 3.96044 -4.89074) (width 0.9))
        (gr_line (start 3.96044 -4.89074) (end 4.21783 -4.93844) (width 0.9))
        (gr_line (start 4.21783 -4.93844) (end 4.47736 -4.97261) (width 0.9))
        (gr_line (start 4.47736 -4.97261) (end 4.73832 -4.99315) (width 0.9))
        (gr_line (start 4.73832 -4.99315) (end 5 -5) (width 0.9))
      ))
  )
  (module custom-devices:L_12_same_45 (layer F.Cu) (tedit 5E859728)
    (at 213 118 270)
    (fp_text reference L304 (at 1.7 2.35 270) (layer F.SilkS))
    (fp_text value L (at 0 12.75 270) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 270) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad 1 smd rect (at -5 4 270) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C308-Pad2)"))
    (pad 2 smd rect (at -5 -4 270) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C308-Pad1)"))
  )
  (module custom-devices:L_12_same_45 (layer F.Cu) (tedit 5E859728)
    (at 194 118 270)
    (fp_text reference L303 (at 1.7 2.35 270) (layer F.SilkS))
    (fp_text value L (at 0 12.75 270) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 270) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad 1 smd rect (at -5 4 270) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C306-Pad2)"))
    (pad 2 smd rect (at -5 -4 270) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C306-Pad1)"))
  )
  (module custom-devices:L_12_same_45 (layer F.Cu) (tedit 5E859728)
    (at 175 118 270)
    (fp_text reference L302 (at 1.7 2.35 270) (layer F.SilkS))
    (fp_text value L (at 0 12.75 270) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 270) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad 1 smd rect (at -5 4 270) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C304-Pad2)"))
    (pad 2 smd rect (at -5 -4 270) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C304-Pad1)"))
  )
  (module custom-devices:L_12_same_45 (layer F.Cu) (tedit 5E859728)
    (at 156 118 270)
    (fp_text reference L301 (at 1.7 2.35 270) (layer F.SilkS))
    (fp_text value L (at 0 12.75 270) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 270) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad 1 smd rect (at -5 4 270) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C302-Pad2)"))
    (pad 2 smd rect (at -5 -4 270) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C302-Pad1)"))
  )
  (module custom-devices:UFL_pattern_mod (layer F.Cu) (tedit 5E85905E)
    (at 162 95)
    (fp_text reference XS501 (at -2.75 2) (layer F.SilkS))
    (fp_text value TestPoint_2Pole (at 0 -2.5) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.5 0.15) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 2 smd roundrect (at -1.5 0.15) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 1 smd roundrect (at 0 -1.5) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(C502-Pad1)"))
    (pad 2 smd roundrect (at 0 1.5) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
  )
  (module custom-devices:UFL_pattern_mod (layer F.Cu) (tedit 5E85905E)
    (at 170 95)
    (fp_text reference XS502 (at -2.75 2) (layer F.SilkS))
    (fp_text value TestPoint_2Pole (at 0 -2.5) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.5 0.15) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 2 smd roundrect (at -1.5 0.15) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 1 smd roundrect (at 0 -1.5) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 "Net-(C504-Pad2)"))
    (pad 2 smd roundrect (at 0 1.5) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
  )
  (module custom-devices:UFL_pattern_mod (layer F.Cu) (tedit 5E85905E)
    (at 181 95)
    (fp_text reference XS503 (at -2.75 2) (layer F.SilkS))
    (fp_text value TestPoint_2Pole (at 0 -2.5) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.5 0.15) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 2 smd roundrect (at -1.5 0.15) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 1 smd roundrect (at 0 -1.5) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(C504-Pad1)"))
    (pad 2 smd roundrect (at 0 1.5) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
  )
  (module custom-devices:UFL_pattern_mod (layer F.Cu) (tedit 5E85905E)
    (at 189 95)
    (fp_text reference XS504 (at -2.75 2) (layer F.SilkS))
    (fp_text value TestPoint_2Pole (at 0 -2.5) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.5 0.15) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 2 smd roundrect (at -1.5 0.15) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 1 smd roundrect (at 0 -1.5) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 "Net-(C506-Pad2)"))
    (pad 2 smd roundrect (at 0 1.5) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
  )
  (module custom-devices:UFL_pattern_mod (layer F.Cu) (tedit 5E85905E)
    (at 200 95)
    (fp_text reference XS505 (at -2.75 2) (layer F.SilkS))
    (fp_text value TestPoint_2Pole (at 0 -2.5) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.5 0.15) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 2 smd roundrect (at -1.5 0.15) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 1 smd roundrect (at 0 -1.5) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 "Net-(C506-Pad1)"))
    (pad 2 smd roundrect (at 0 1.5) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
  )
  (module custom-devices:UFL_pattern_mod (layer F.Cu) (tedit 5E85905E)
    (at 208 95)
    (fp_text reference XS506 (at -2.75 2) (layer F.SilkS))
    (fp_text value TestPoint_2Pole (at 0 -2.5) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.5 0.15) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 2 smd roundrect (at -1.5 0.15) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 1 smd roundrect (at 0 -1.5) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(C508-Pad2)"))
    (pad 2 smd roundrect (at 0 1.5) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
  )
  (module custom-devices:UFL_pattern_mod (layer F.Cu) (tedit 5E85905E)
    (at 162 106 180)
    (fp_text reference XS301 (at -2.75 2 180) (layer F.SilkS))
    (fp_text value TestPoint_2Pole (at 0 -2.5 180) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.5 0.15 180) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 2 smd roundrect (at -1.5 0.15 180) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 1 smd roundrect (at 0 -1.5 180) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C302-Pad1)"))
    (pad 2 smd roundrect (at 0 1.5 180) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
  )
  (module custom-devices:UFL_pattern_mod (layer F.Cu) (tedit 5E85905E)
    (at 170 106 180)
    (fp_text reference XS302 (at -2.75 2 180) (layer F.SilkS))
    (fp_text value TestPoint_2Pole (at 0 -2.5 180) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.5 0.15 180) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 2 smd roundrect (at -1.5 0.15 180) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 1 smd roundrect (at 0 -1.5 180) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(C304-Pad2)"))
    (pad 2 smd roundrect (at 0 1.5 180) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
  )
  (module custom-devices:UFL_pattern_mod (layer F.Cu) (tedit 5E85905E)
    (at 181 106 180)
    (fp_text reference XS303 (at -2.75 2 180) (layer F.SilkS))
    (fp_text value TestPoint_2Pole (at 0 -2.5 180) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.5 0.15 180) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 2 smd roundrect (at -1.5 0.15 180) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 1 smd roundrect (at 0 -1.5 180) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(C304-Pad1)"))
    (pad 2 smd roundrect (at 0 1.5 180) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
  )
  (module custom-devices:UFL_pattern_mod (layer F.Cu) (tedit 5E85905E)
    (at 189 106 180)
    (fp_text reference XS304 (at -2.75 2 180) (layer F.SilkS))
    (fp_text value TestPoint_2Pole (at 0 -2.5 180) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.5 0.15 180) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 2 smd roundrect (at -1.5 0.15 180) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 1 smd roundrect (at 0 -1.5 180) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(C306-Pad2)"))
    (pad 2 smd roundrect (at 0 1.5 180) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
  )
  (module custom-devices:UFL_pattern_mod (layer F.Cu) (tedit 5E85905E)
    (at 200 106 180)
    (fp_text reference XS305 (at -2.75 2 180) (layer F.SilkS))
    (fp_text value TestPoint_2Pole (at 0 -2.5 180) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.5 0.15 180) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 2 smd roundrect (at -1.5 0.15 180) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 1 smd roundrect (at 0 -1.5 180) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(C306-Pad1)"))
    (pad 2 smd roundrect (at 0 1.5 180) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
  )
  (module custom-devices:UFL_pattern_mod (layer F.Cu) (tedit 5E85905E)
    (at 208 106 180)
    (fp_text reference XS306 (at -2.75 2 180) (layer F.SilkS))
    (fp_text value TestPoint_2Pole (at 0 -2.5 180) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.5 0.15 180) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 2 smd roundrect (at -1.5 0.15 180) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 1 smd roundrect (at 0 -1.5 180) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(C308-Pad2)"))
    (pad 2 smd roundrect (at 0 1.5 180) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
  )
  (module custom-devices:UFL_pattern_mod (layer F.Cu) (tedit 5E85905E)
    (at 139.75 95.25)
    (fp_text reference XS104 (at -2.75 2) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 -2.5) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.5 0.15) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 2 smd roundrect (at -1.5 0.15) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 1 smd roundrect (at 0 -1.5) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 193 "/Low-pass B/FilterA"))
    (pad 2 smd roundrect (at 0 1.5) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
  )
  (module custom-devices:UFL_pattern_mod (layer F.Cu) (tedit 5E85905E)
    (at 227 106 180)
    (fp_text reference XS105 (at -2.75 2 180) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 -2.5 180) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.5 0.15 180) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 2 smd roundrect (at -1.5 0.15 180) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 1 smd roundrect (at 0 -1.5 180) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "/Low-pass A/FilterB"))
    (pad 2 smd roundrect (at 0 1.5 180) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
  )
  (module custom-devices:UFL_pattern_mod (layer F.Cu) (tedit 5E85905E)
    (at 227 95)
    (fp_text reference XS106 (at -2.75 2) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 -2.5) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.5 0.15) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 2 smd roundrect (at -1.5 0.15) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 1 smd roundrect (at 0 -1.5) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "/Low-pass B/FilterB"))
    (pad 2 smd roundrect (at 0 1.5) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
  )
  (module custom-devices:UFL_pattern_mod (layer F.Cu) (tedit 5E85905E)
    (at 213.25 132.25 180)
    (fp_text reference XS107 (at -2.75 2 180) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 -2.5 180) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.5 0.15 180) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 2 smd roundrect (at -1.5 0.15 180) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 1 smd roundrect (at 0 -1.5 180) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 186 "Net-(X106-Pad2)"))
    (pad 2 smd roundrect (at 0 1.5 180) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
  )
  (module custom-devices:UFL_pattern_mod (layer F.Cu) (tedit 5E85905E)
    (at 213.25 62.5 180)
    (fp_text reference XS108 (at 0 2.75 180) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 -2.5 180) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.5 0.15 180) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 2 smd roundrect (at -1.5 0.15 180) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 1 smd roundrect (at 0 -1.5 180) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 187 "Net-(X107-Pad2)"))
    (pad 2 smd roundrect (at 0 1.5 180) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
  )
  (module custom-devices:UFL_pattern_mod (layer F.Cu) (tedit 5E85905E)
    (at 139.75 105.75 180)
    (fp_text reference XS103 (at -2.75 2 180) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 -2.5 180) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.5 0.15 180) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 2 smd roundrect (at -1.5 0.15 180) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 1 smd roundrect (at 0 -1.5 180) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 191 "/Low-pass A/FilterA"))
    (pad 2 smd roundrect (at 0 1.5 180) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
  )
  (module custom-devices:UFL_pattern_mod (layer F.Cu) (tedit 5E85905E)
    (at 105.5 95.75)
    (fp_text reference XS401 (at -2.75 2) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 0 -2.5) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.5 0.15) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 2 smd roundrect (at -1.5 0.15) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 1 smd roundrect (at 0 -1.5) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 195 "Net-(X402-Pad2)"))
    (pad 2 smd roundrect (at 0 1.5) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
  )
  (module custom-devices:UFL_pattern_mod (layer F.Cu) (tedit 5E85905E)
    (at 123.5 95.75)
    (fp_text reference XS402 (at -2.75 2) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 0 -2.5) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.5 0.15) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 2 smd roundrect (at -1.5 0.15) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 1 smd roundrect (at 0 -1.5) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 196 "Net-(X403-Pad2)"))
    (pad 2 smd roundrect (at 0 1.5) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
  )
  (module custom-devices:UFL_pattern_mod (layer F.Cu) (tedit 5E85905E)
    (at 105.5 105.25 180)
    (fp_text reference XS201 (at -2.75 2 180) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 0 -2.5 180) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.5 0.15 180) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 2 smd roundrect (at -1.5 0.15 180) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 1 smd roundrect (at 0 -1.5 180) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 189 "Net-(X202-Pad2)"))
    (pad 2 smd roundrect (at 0 1.5 180) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
  )
  (module custom-devices:UFL_pattern_mod (layer F.Cu) (tedit 5E85905E)
    (at 123.5 105.25 180)
    (fp_text reference XS202 (at -2.75 2 180) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 0 -2.5 180) (layer F.Fab) hide)
    (pad 2 smd roundrect (at 1.5 0.15 180) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 2 smd roundrect (at -1.5 0.15 180) (size 0.95 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
    (pad 1 smd roundrect (at 0 -1.5 180) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 190 "Net-(X203-Pad2)"))
    (pad 2 smd roundrect (at 0 1.5 180) (size 1 1) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 GND))
  )
  (module custom-devices:L_12_same_n45 (layer F.Cu) (tedit 5E8597E6)
    (at 194 83 270)
    (fp_text reference L503 (at 1.7 2.35 270) (layer F.SilkS))
    (fp_text value L (at 0 12.75 270) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 270) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad 1 smd rect (at 5 4 270) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(C506-Pad2)"))
    (pad 2 smd rect (at 5 -4 270) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(C506-Pad1)"))
  )
  (module custom-devices:L_12_same_n45 (layer F.Cu) (tedit 5E8597E6)
    (at 213 83 270)
    (fp_text reference L504 (at 1.7 2.35 270) (layer F.SilkS))
    (fp_text value L (at 0 12.75 270) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 270) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad 1 smd rect (at 5 4 270) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(C508-Pad2)"))
    (pad 2 smd rect (at 5 -4 270) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(C508-Pad1)"))
  )
  (module custom-devices:L_12_same_n45 (layer F.Cu) (tedit 5E8597E6)
    (at 175 83 270)
    (fp_text reference L502 (at 1.7 2.35 270) (layer F.SilkS))
    (fp_text value L (at 0 12.75 270) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 270) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad 1 smd rect (at 5 4 270) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(C504-Pad2)"))
    (pad 2 smd rect (at 5 -4 270) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(C504-Pad1)"))
  )
  (module custom-devices:L_12_same_n45 (layer F.Cu) (tedit 5E8597E6)
    (at 156 83 270)
    (fp_text reference L501 (at 1.7 2.35 270) (layer F.SilkS))
    (fp_text value L (at 0 12.75 270) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 270) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad 1 smd rect (at 5 4 270) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(C502-Pad2)"))
    (pad 2 smd rect (at 5 -4 270) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(C502-Pad1)"))
  )
  (module custom-devices:Jumper3_0.9_0.68 (layer F.Cu) (tedit 5E859187)
    (at 105 109 330)
    (clearance 0.2)
    (attr smd)
    (fp_text reference X202 (at -0.116025 1.799038 150) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1 330) (layer F.Fab) hide)
    (pad 2 smd rect (at 0 0 330) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 189 "Net-(X202-Pad2)") (clearance 0.6805))
    (pad 1 smd rect (at -1.8 0 330) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C202-Pad1)") (clearance 0.6805))
    (pad 3 smd rect (at 1.8 0 330) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C204-Pad2)") (clearance 0.6805))
    (model SMD_Packages.3dshapes/Conn-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:Jumper3_0.9_0.68 (layer F.Cu) (tedit 5E859187)
    (at 123 109 330)
    (clearance 0.2)
    (attr smd)
    (fp_text reference X203 (at 0.008975 2.015544 330) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1 330) (layer F.Fab) hide)
    (pad 2 smd rect (at 0 0 330) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 190 "Net-(X203-Pad2)") (clearance 0.6805))
    (pad 1 smd rect (at -1.8 0 330) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C205-Pad1)") (clearance 0.6805))
    (pad 3 smd rect (at 1.8 0 330) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C207-Pad2)") (clearance 0.6805))
    (model SMD_Packages.3dshapes/Conn-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:Jumper3_0.9_0.68 (layer F.Cu) (tedit 5E859187)
    (at 105 92 30)
    (clearance 0.2)
    (attr smd)
    (fp_text reference X402 (at 0.225481 -1.890544 30) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1 30) (layer F.Fab) hide)
    (pad 2 smd rect (at 0 0 30) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 195 "Net-(X402-Pad2)") (clearance 0.6805))
    (pad 1 smd rect (at -1.8 0 30) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C402-Pad1)") (clearance 0.6805))
    (pad 3 smd rect (at 1.8 0 30) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(C404-Pad2)") (clearance 0.6805))
    (model SMD_Packages.3dshapes/Conn-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:Jumper3_0.9_0.68 (layer F.Cu) (tedit 5E859187)
    (at 123 92 30)
    (clearance 0.2)
    (attr smd)
    (fp_text reference X403 (at -0.116025 -1.799038 30) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1 30) (layer F.Fab) hide)
    (pad 2 smd rect (at 0 0 30) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 196 "Net-(X403-Pad2)") (clearance 0.6805))
    (pad 1 smd rect (at -1.8 0 30) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C405-Pad1)") (clearance 0.6805))
    (pad 3 smd rect (at 1.8 0 30) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(C407-Pad2)") (clearance 0.6805))
    (model SMD_Packages.3dshapes/Conn-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:DG983-2 (layer F.Cu) (tedit 5E8420C9)
    (at 222 64.5 90)
    (fp_text reference DA1401 (at 3.75 -0.75) (layer F.SilkS))
    (fp_text value DAT-31A-SN+ (at 0 3.38963 90) (layer F.Fab))
    (pad 21 smd rect (at 0 0 90) (size 2.0574 2.0574) (layers F.Cu F.Paste F.Mask)
      (net 18 GND) (clearance 0.4))
    (pad 20 smd rect (at -1.841499 1.016 90) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(DA1401-Pad20)"))
    (pad 19 smd rect (at -1.841499 0.508 90) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask)
      (net 106 "Net-(DA1401-Pad19)"))
    (pad 18 smd rect (at -1.841499 0 90) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 17 smd rect (at -1.841499 -0.508 90) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(DA1401-Pad17)"))
    (pad 16 smd rect (at -1.841499 -1.016 90) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(DA1401-Pad16)"))
    (pad 10 smd rect (at 1.841499 -1.016 90) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 9 smd rect (at 1.841499 -0.508 90) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask)
      (net 200 VDD))
    (pad 8 smd rect (at 1.841499 0 90) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(DA1401-Pad8)"))
    (pad 7 smd rect (at 1.841499 0.508 90) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(DA1401-Pad7)"))
    (pad 6 smd rect (at 1.841499 1.016 90) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask)
      (net 200 VDD))
    (pad 15 smd rect (at -1.016 -1.841499 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(DA1401-Pad15)"))
    (pad 14 smd rect (at -0.508 -1.841499 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask)
      (net 7 "/Attenuator B/RFout"))
    (pad 13 smd rect (at 0 -1.841499 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask)
      (net 200 VDD))
    (pad 12 smd rect (at 0.508 -1.841499 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 11 smd rect (at 1.016 -1.841499 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 5 smd rect (at 1.016 1.841499 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask)
      (net 100 /LE1))
    (pad 4 smd rect (at 0.508 1.841499 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask)
      (net 86 /YSCK))
    (pad 3 smd rect (at 0 1.841499 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask)
      (net 87 /YMOSI))
    (pad 2 smd rect (at -0.508 1.841499 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask)
      (net 4 "/Attenuator B/RFin"))
    (pad 1 smd rect (at -1.016 1.841499 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(DA1401-Pad1)"))
  )
  (module custom-devices:DG983-2 (layer F.Cu) (tedit 5E8420C9)
    (at 222 134.5 90)
    (fp_text reference DA701 (at 3 3.5) (layer F.SilkS))
    (fp_text value DAT-31A-SN+ (at 0 3.38963 90) (layer F.Fab))
    (pad 21 smd rect (at 0 0 90) (size 2.0574 2.0574) (layers F.Cu F.Paste F.Mask)
      (net 18 GND) (clearance 0.4))
    (pad 20 smd rect (at -1.841499 1.016 90) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(DA701-Pad20)"))
    (pad 19 smd rect (at -1.841499 0.508 90) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(DA701-Pad19)"))
    (pad 18 smd rect (at -1.841499 0 90) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 17 smd rect (at -1.841499 -0.508 90) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(DA701-Pad17)"))
    (pad 16 smd rect (at -1.841499 -1.016 90) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(DA701-Pad16)"))
    (pad 10 smd rect (at 1.841499 -1.016 90) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 9 smd rect (at 1.841499 -0.508 90) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask)
      (net 200 VDD))
    (pad 8 smd rect (at 1.841499 0 90) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(DA701-Pad8)"))
    (pad 7 smd rect (at 1.841499 0.508 90) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(DA701-Pad7)"))
    (pad 6 smd rect (at 1.841499 1.016 90) (size 0.8128 0.254) (layers F.Cu F.Paste F.Mask)
      (net 200 VDD))
    (pad 15 smd rect (at -1.016 -1.841499 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(DA701-Pad15)"))
    (pad 14 smd rect (at -0.508 -1.841499 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask)
      (net 6 "/Attenuator A/RFout"))
    (pad 13 smd rect (at 0 -1.841499 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask)
      (net 200 VDD))
    (pad 12 smd rect (at 0.508 -1.841499 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 11 smd rect (at 1.016 -1.841499 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 5 smd rect (at 1.016 1.841499 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask)
      (net 85 /LE0))
    (pad 4 smd rect (at 0.508 1.841499 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask)
      (net 86 /YSCK))
    (pad 3 smd rect (at 0 1.841499 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask)
      (net 87 /YMOSI))
    (pad 2 smd rect (at -0.508 1.841499 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask)
      (net 1 "/Attenuator A/RFin"))
    (pad 1 smd rect (at -1.016 1.841499 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(DA701-Pad1)"))
  )
  (module Package_SO:Mini-Circuits_CD542_H2.84mm (layer F.Cu) (tedit 5E1FE691)
    (at 137.25 63.75 90)
    (descr https://ww2.minicircuits.com/case_style/CD542.pdf)
    (tags "RF Transformer")
    (attr smd)
    (fp_text reference T1102 (at 0 -4.826 90) (layer F.SilkS))
    (fp_text value "FIXME: ADT4-6T" (at 0 5.08 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 6 smd rect (at 2.54 -2.54 90) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 164 "Net-(K1102-Pad3)"))
    (pad 5 smd rect (at 2.54 0 90) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 177 "Net-(T1102-Pad5)"))
    (pad 4 smd rect (at 2.54 2.54 90) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 3 smd rect (at -2.54 2.54 90) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(C1105-Pad1)"))
    (pad 2 smd rect (at -2.54 0 90) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -2.54 -2.54 90) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(C1104-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/Mini-Circuits_CD542_H2.84mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5CA30FA5)
    (at 93 113 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C201 (at -3 0) (layer F.SilkS))
    (fp_text value C (at 0 3.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 -180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 9 "Net-(C201-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 10 "Net-(C201-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5CA30FA5)
    (at 93 109 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C202 (at -3 0 180) (layer F.SilkS))
    (fp_text value C (at 0 3.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 10 "Net-(C201-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 11 "Net-(C202-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5E0B043D)
    (at 98 109 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C203 (at -3 0) (layer F.SilkS))
    (fp_text value C (at 0 3.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 11 "Net-(C202-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 9 "Net-(C201-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5CA30FA5)
    (at 111 113 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C204 (at -3 0) (layer F.SilkS))
    (fp_text value C (at 0 3.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 -180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 12 "Net-(C204-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 13 "Net-(C204-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5CA30FA5)
    (at 111 109 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C205 (at 3 0 180) (layer F.SilkS))
    (fp_text value C (at 0 3.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 12 "Net-(C204-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 14 "Net-(C205-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5CA30FA5)
    (at 116 109 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C206 (at -3 0 180) (layer F.SilkS))
    (fp_text value C (at 0 3.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 14 "Net-(C205-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 13 "Net-(C204-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5CA30FA5)
    (at 129 113 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C207 (at -3 0) (layer F.SilkS))
    (fp_text value C (at 0 3.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 -180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 15 "Net-(C207-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 16 "Net-(C207-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5CA30FA5)
    (at 129 109 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C208 (at -3 0) (layer F.SilkS))
    (fp_text value C (at 0 3.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 17 "Net-(C208-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 15 "Net-(C207-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5CA30FA5)
    (at 134 109 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C209 (at -3 0 180) (layer F.SilkS))
    (fp_text value C (at 0 3.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 16 "Net-(C207-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 17 "Net-(C208-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5E0AFF69)
    (at 148 113)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C301 (at -0.5 3.5) (layer F.SilkS))
    (fp_text value C_Small (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0 -270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.024999 0.000001) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 18 GND))
    (pad 2 smd roundrect (at 1.024999 -0.000001) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 19 "Net-(C301-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5CA30FA5)
    (at 156 109 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C302 (at 2.75 0) (layer F.SilkS))
    (fp_text value C_Small (at 0 3.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 20 "Net-(C302-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 21 "Net-(C302-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5E0AFF03)
    (at 165 112)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C303 (at 0.025 4.25) (layer F.SilkS))
    (fp_text value C_Small (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 22 "Net-(C303-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 18 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5CA30FA5)
    (at 175 109 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C304 (at -3 0) (layer F.SilkS))
    (fp_text value C_Small (at 0 3.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 -180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 23 "Net-(C304-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 24 "Net-(C304-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5CA30FA5)
    (at 184 112)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C305 (at 0 3.5) (layer F.SilkS))
    (fp_text value C_Small (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0 -270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 18 GND))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 25 "Net-(C305-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5E099DDA)
    (at 194 109 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C306 (at -3 1.25 180) (layer F.SilkS))
    (fp_text value C_Small (at 0 3.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 26 "Net-(C306-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 27 "Net-(C306-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5E099E12)
    (at 203 112)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C307 (at 0 3.5) (layer F.SilkS))
    (fp_text value C_Small (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 18 GND))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 28 "Net-(C307-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5CA30FA5)
    (at 213 109 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C308 (at -3 1.5) (layer F.SilkS))
    (fp_text value C_Small (at 0 3.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 -180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.024999 0 90) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 29 "Net-(C308-Pad1)"))
    (pad 2 smd roundrect (at 1.024999 0 90) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 30 "Net-(C308-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5E228BD4)
    (at 222.025 112 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C309 (at 0.025 -3.5) (layer F.SilkS))
    (fp_text value C_Small (at 0 3.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 -90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 31 "Net-(C309-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 18 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5CA30FA5)
    (at 93 88 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C401 (at -3 0 180) (layer F.SilkS))
    (fp_text value C (at 0 3.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 32 "Net-(C401-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 33 "Net-(C401-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5CA30FA5)
    (at 93 92 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C402 (at -3 0) (layer F.SilkS))
    (fp_text value C (at 0 3.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 -180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 34 "Net-(C402-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 33 "Net-(C401-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5CA30FA5)
    (at 98.5 92 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C403 (at -3 0) (layer F.SilkS))
    (fp_text value C (at 0 3.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 -180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 32 "Net-(C401-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 34 "Net-(C402-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5CA30FA5)
    (at 111.5 88 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C404 (at -3 0 180) (layer F.SilkS))
    (fp_text value C (at 0 3.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 35 "Net-(C404-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 36 "Net-(C404-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5CA30FA5)
    (at 111.5 92 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C405 (at -3 0) (layer F.SilkS))
    (fp_text value C (at 0 3.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 -180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 37 "Net-(C405-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 35 "Net-(C404-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5CA30FA5)
    (at 116.5 92 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C406 (at -3.024999 0) (layer F.SilkS))
    (fp_text value C (at 0 3.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 -180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 37 "Net-(C405-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 36 "Net-(C404-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5CA30FA5)
    (at 129.5 88 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C407 (at -3 0 180) (layer F.SilkS))
    (fp_text value C (at 0 3.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 38 "Net-(C407-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 39 "Net-(C407-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5CA30FA5)
    (at 129.5 92 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C408 (at -3 0) (layer F.SilkS))
    (fp_text value C (at 0 3.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 -180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 40 "Net-(C408-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 38 "Net-(C407-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5CA30FA5)
    (at 134.5 92 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C409 (at -3 0) (layer F.SilkS))
    (fp_text value C (at 0 3.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 -180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 39 "Net-(C407-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 40 "Net-(C408-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5CA30FA5)
    (at 148 88)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C501 (at 0 -3.5) (layer F.SilkS))
    (fp_text value C_Small (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.024999 0) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 18 GND))
    (pad 2 smd roundrect (at 1.024999 0) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 41 "Net-(C501-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5CA30FA5)
    (at 156 92 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C502 (at -3 0 180) (layer F.SilkS))
    (fp_text value C_Small (at 0 3.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 42 "Net-(C502-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 43 "Net-(C502-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5CA30FA5)
    (at 164.975 89)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C503 (at 0.025 -3.25) (layer F.SilkS))
    (fp_text value C_Small (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 18 GND))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 44 "Net-(C503-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5CA30FA5)
    (at 175 92 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C504 (at 3 0 180) (layer F.SilkS))
    (fp_text value C_Small (at 0 3.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 45 "Net-(C504-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 46 "Net-(C504-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5CA30FA5)
    (at 184 89)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C505 (at 0 -3.5) (layer F.SilkS))
    (fp_text value C_Small (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 18 GND))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 47 "Net-(C505-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5CA30FA5)
    (at 194 92 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C506 (at -3 0 180) (layer F.SilkS))
    (fp_text value C_Small (at 0 3.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 48 "Net-(C506-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 49 "Net-(C506-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5CA30FA5)
    (at 203 89)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C507 (at 0 -3.5) (layer F.SilkS))
    (fp_text value C_Small (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 50 "Net-(C507-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 18 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5CA30FA5)
    (at 213 92 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C508 (at 3 0 180) (layer F.SilkS))
    (fp_text value C_Small (at 0 3.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 51 "Net-(C508-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 52 "Net-(C508-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0805_x3 (layer F.Cu) (tedit 5CA30FA5)
    (at 222 89 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C509 (at 0.024999 3.5 180) (layer F.SilkS))
    (fp_text value C_Small (at 0 3.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 18 GND))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 4.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217)
      (net 53 "Net-(C509-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-223-3_TabPin2 (layer F.Cu) (tedit 5A02FF57)
    (at 257 57 90)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference DA601 (at -0.5 0.25 180) (layer F.SilkS))
    (fp_text value LM1117-3.3 (at 0 4.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 -180) (layer F.Fab))
    (pad 2 smd rect (at 3.15 0 90) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 197 +3V3))
    (pad 2 smd rect (at -3.15 0 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 197 +3V3))
    (pad 3 smd rect (at -3.15 2.3 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 54 +12V))
    (pad 1 smd rect (at -3.15 -2.3 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:DFN-10-1EP_3x3mm_P0.5mm_EP1.55x2.48mm (layer F.Cu) (tedit 5A64BE60)
    (at 254 82 180)
    (descr "10-Lead Plastic Dual Flat, No Lead Package (MF) - 3x3x0.9 mm Body [DFN] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference DA602 (at 0 -2.575 180) (layer F.SilkS))
    (fp_text value LT3045_DD (at 0 2.575 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.55 -1 180) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 201 +12VA))
    (pad 2 smd rect (at -1.55 -0.5 180) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 201 +12VA))
    (pad 3 smd rect (at -1.55 0 180) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 201 +12VA))
    (pad 4 smd rect (at -1.55 0.5 180) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(DA602-Pad4)"))
    (pad 5 smd rect (at -1.55 1 180) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(DA602-Pad5)"))
    (pad 6 smd rect (at 1.55 1 180) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 201 +12VA))
    (pad 7 smd rect (at 1.55 0.5 180) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(C604-Pad1)"))
    (pad 8 smd rect (at 1.55 0 180) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 9 smd rect (at 1.55 -0.5 180) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 198 +3.3VA))
    (pad 10 smd rect (at 1.55 -1 180) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask)
      (net 198 +3.3VA))
    (pad "" smd rect (at 0.3875 -0.62 180) (size 0.6 1.05) (layers F.Paste))
    (pad 11 smd rect (at 0 0 180) (size 1.55 2.48) (layers F.Cu F.Mask)
      (net 18 GND))
    (pad "" smd rect (at -0.3875 -0.62 180) (size 0.6 1.05) (layers F.Paste))
    (pad "" smd rect (at -0.3875 0.62 180) (size 0.6 1.05) (layers F.Paste))
    (pad "" smd rect (at 0.3875 0.62 180) (size 0.6 1.05) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-10-1EP_3x3mm_P0.5mm_EP1.55x2.48mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm (layer F.Cu) (tedit 5E26BCA5)
    (at 150 136.75 270)
    (descr "16-Lead Plastic Quad Flat, No Lead Package (NG) - 3x3x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference DA901 (at -2.75 3.25 180) (layer F.SilkS))
    (fp_text value LTC6400-20 (at 0 2.85 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad "" smd rect (at -0.45 -0.45 270) (size 0.73 0.73) (layers F.Paste))
    (pad "" smd rect (at 0.45 -0.45 270) (size 0.73 0.73) (layers F.Paste))
    (pad "" smd rect (at 0.45 0.45 270) (size 0.73 0.73) (layers F.Paste))
    (pad 17 smd rect (at 0 0 270) (size 1.8 1.8) (layers F.Cu F.Mask)
      (net 18 GND) (clearance 0.2))
    (pad "" smd rect (at -0.45 0.45 270) (size 0.73 0.73) (layers F.Paste))
    (pad 16 smd oval (at -0.75 -1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 59 "/Amplifier A/IN-"))
    (pad 15 smd oval (at -0.25 -1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 59 "/Amplifier A/IN-"))
    (pad 14 smd oval (at 0.25 -1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 57 "/Amplifier A/IN+"))
    (pad 13 smd oval (at 0.75 -1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 57 "/Amplifier A/IN+"))
    (pad 12 smd oval (at 1.475 -0.75 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND) (clearance 0.2))
    (pad 11 smd oval (at 1.475 -0.25 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 89 "/Control circuit/DO0"))
    (pad 10 smd oval (at 1.475 0.25 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 199 V+) (clearance 0.2))
    (pad 9 smd oval (at 1.475 0.75 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND) (clearance 0.2))
    (pad 8 smd oval (at 0.75 1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 61 "/Amplifier A/OUT+"))
    (pad 7 smd oval (at 0.25 1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(DA901-Pad7)") (clearance 0.2))
    (pad 6 smd oval (at -0.25 1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(DA901-Pad6)") (clearance 0.2))
    (pad 5 smd oval (at -0.75 1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 64 "/Amplifier A/OUT-"))
    (pad 4 smd oval (at -1.475 0.75 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 3 smd oval (at -1.475 0.25 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 199 V+) (clearance 0.2))
    (pad 2 smd oval (at -1.475 -0.25 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 65 "/Amplifier A/Vocm"))
    (pad 1 smd oval (at -1.475 -0.75 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 199 V+))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm (layer F.Cu) (tedit 5E26BCAA)
    (at 150 144.25 270)
    (descr "16-Lead Plastic Quad Flat, No Lead Package (NG) - 3x3x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference DA902 (at 2.75 3.5 180) (layer F.SilkS))
    (fp_text value LTC6400-20 (at 0 2.85 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd oval (at -1.475 -0.75 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 199 V+))
    (pad 2 smd oval (at -1.475 -0.25 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 65 "/Amplifier A/Vocm"))
    (pad 3 smd oval (at -1.475 0.25 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 199 V+) (clearance 0.2))
    (pad 4 smd oval (at -1.475 0.75 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 5 smd oval (at -0.75 1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 61 "/Amplifier A/OUT+"))
    (pad 6 smd oval (at -0.25 1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(DA902-Pad6)") (clearance 0.2))
    (pad 7 smd oval (at 0.25 1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(DA902-Pad7)") (clearance 0.2))
    (pad 8 smd oval (at 0.75 1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 64 "/Amplifier A/OUT-"))
    (pad 9 smd oval (at 1.475 0.75 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND) (clearance 0.2))
    (pad 10 smd oval (at 1.475 0.25 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 199 V+) (clearance 0.2))
    (pad 11 smd oval (at 1.475 -0.25 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 89 "/Control circuit/DO0"))
    (pad 12 smd oval (at 1.475 -0.75 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND) (clearance 0.2))
    (pad 13 smd oval (at 0.75 -1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 59 "/Amplifier A/IN-"))
    (pad 14 smd oval (at 0.25 -1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 59 "/Amplifier A/IN-"))
    (pad 15 smd oval (at -0.25 -1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 57 "/Amplifier A/IN+"))
    (pad 16 smd oval (at -0.75 -1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 57 "/Amplifier A/IN+"))
    (pad "" smd rect (at -0.45 0.45 270) (size 0.73 0.73) (layers F.Paste))
    (pad 17 smd rect (at 0 0 270) (size 1.8 1.8) (layers F.Cu F.Mask)
      (net 18 GND) (clearance 0.2))
    (pad "" smd rect (at 0.45 0.45 270) (size 0.73 0.73) (layers F.Paste))
    (pad "" smd rect (at 0.45 -0.45 270) (size 0.73 0.73) (layers F.Paste))
    (pad "" smd rect (at -0.45 -0.45 270) (size 0.73 0.73) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm (layer F.Cu) (tedit 5E26BCB4)
    (at 149.75 62.75 270)
    (descr "16-Lead Plastic Quad Flat, No Lead Package (NG) - 3x3x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference DA1101 (at -2.75 3.75 180) (layer F.SilkS))
    (fp_text value LTC6400-20 (at 0 2.85 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad "" smd rect (at -0.45 -0.45 270) (size 0.73 0.73) (layers F.Paste))
    (pad "" smd rect (at 0.45 -0.45 270) (size 0.73 0.73) (layers F.Paste))
    (pad "" smd rect (at 0.45 0.45 270) (size 0.73 0.73) (layers F.Paste))
    (pad 17 smd rect (at 0 0 270) (size 1.8 1.8) (layers F.Cu F.Mask)
      (net 18 GND) (clearance 0.2))
    (pad "" smd rect (at -0.45 0.45 270) (size 0.73 0.73) (layers F.Paste))
    (pad 16 smd oval (at -0.75 -1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 70 "/Amplifier B/IN-"))
    (pad 15 smd oval (at -0.25 -1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 70 "/Amplifier B/IN-"))
    (pad 14 smd oval (at 0.25 -1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 66 "/Amplifier B/IN+"))
    (pad 13 smd oval (at 0.75 -1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 66 "/Amplifier B/IN+"))
    (pad 12 smd oval (at 1.475 -0.75 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND) (clearance 0.2))
    (pad 11 smd oval (at 1.475 -0.25 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 94 "/Control circuit/DO1"))
    (pad 10 smd oval (at 1.475 0.25 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 199 V+) (clearance 0.2))
    (pad 9 smd oval (at 1.475 0.75 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND) (clearance 0.2))
    (pad 8 smd oval (at 0.75 1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 72 "/Amplifier B/OUT+"))
    (pad 7 smd oval (at 0.25 1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(DA1101-Pad7)"))
    (pad 6 smd oval (at -0.25 1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(DA1101-Pad6)"))
    (pad 5 smd oval (at -0.75 1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 73 "/Amplifier B/OUT-"))
    (pad 4 smd oval (at -1.475 0.75 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 3 smd oval (at -1.475 0.25 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 199 V+) (clearance 0.2))
    (pad 2 smd oval (at -1.475 -0.25 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 75 "/Amplifier B/Vocm"))
    (pad 1 smd oval (at -1.475 -0.75 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 199 V+))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm (layer F.Cu) (tedit 5E26BCBA)
    (at 149.75 70.25 270)
    (descr "16-Lead Plastic Quad Flat, No Lead Package (NG) - 3x3x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference DA1102 (at 1.75 5 180) (layer F.SilkS))
    (fp_text value LTC6400-20 (at 0 2.85 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd oval (at -1.475 -0.75 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 199 V+))
    (pad 2 smd oval (at -1.475 -0.25 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 75 "/Amplifier B/Vocm"))
    (pad 3 smd oval (at -1.475 0.25 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 199 V+) (clearance 0.2))
    (pad 4 smd oval (at -1.475 0.75 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 5 smd oval (at -0.75 1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 72 "/Amplifier B/OUT+"))
    (pad 6 smd oval (at -0.25 1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(DA1102-Pad6)"))
    (pad 7 smd oval (at 0.25 1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 98 "Net-(DA1102-Pad7)"))
    (pad 8 smd oval (at 0.75 1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 73 "/Amplifier B/OUT-"))
    (pad 9 smd oval (at 1.475 0.75 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND) (clearance 0.2))
    (pad 10 smd oval (at 1.475 0.25 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 199 V+) (clearance 0.2))
    (pad 11 smd oval (at 1.475 -0.25 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 94 "/Control circuit/DO1"))
    (pad 12 smd oval (at 1.475 -0.75 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND) (clearance 0.2))
    (pad 13 smd oval (at 0.75 -1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 70 "/Amplifier B/IN-"))
    (pad 14 smd oval (at 0.25 -1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 70 "/Amplifier B/IN-"))
    (pad 15 smd oval (at -0.25 -1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 66 "/Amplifier B/IN+"))
    (pad 16 smd oval (at -0.75 -1.475) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 66 "/Amplifier B/IN+"))
    (pad "" smd rect (at -0.45 0.45 270) (size 0.73 0.73) (layers F.Paste))
    (pad 17 smd rect (at 0 0 270) (size 1.8 1.8) (layers F.Cu F.Mask)
      (net 18 GND) (clearance 0.2))
    (pad "" smd rect (at 0.45 0.45 270) (size 0.73 0.73) (layers F.Paste))
    (pad "" smd rect (at 0.45 -0.45 270) (size 0.73 0.73) (layers F.Paste))
    (pad "" smd rect (at -0.45 -0.45 270) (size 0.73 0.73) (layers F.Paste))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_QFP:TQFP-32_7x7mm_P0.8mm (layer F.Cu) (tedit 5A02F146)
    (at 256.5 132.25 90)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference DD701 (at 0 0 45) (layer F.SilkS))
    (fp_text value ATmega48PA-AU (at 0 6.05 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -4.25 -2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 108 "Net-(DD701-Pad1)"))
    (pad 2 smd rect (at -4.25 -2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(DD701-Pad2)"))
    (pad 3 smd rect (at -4.25 -1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 4 smd rect (at -4.25 -0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 197 +3V3))
    (pad 5 smd rect (at -4.25 0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 6 smd rect (at -4.25 1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 197 +3V3))
    (pad 7 smd rect (at -4.25 2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(DD701-Pad7)"))
    (pad 8 smd rect (at -4.25 2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(DD701-Pad8)"))
    (pad 9 smd rect (at -2.8 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 112 "Net-(DD701-Pad9)"))
    (pad 10 smd rect (at -2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 113 "Net-(DD701-Pad10)"))
    (pad 11 smd rect (at -1.2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 114 "Net-(DD701-Pad11)"))
    (pad 12 smd rect (at -0.4 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(DD701-Pad12)"))
    (pad 13 smd rect (at 0.4 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 116 "Net-(DD701-Pad13)"))
    (pad 14 smd rect (at 1.2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(DD701-Pad14)"))
    (pad 15 smd rect (at 2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(DD701-Pad15)"))
    (pad 16 smd rect (at 2.8 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(DD701-Pad16)"))
    (pad 17 smd rect (at 4.25 2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(DD701-Pad17)"))
    (pad 18 smd rect (at 4.25 2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 197 +3V3))
    (pad 19 smd rect (at 4.25 1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(DD701-Pad19)"))
    (pad 20 smd rect (at 4.25 0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 122 "Net-(DD701-Pad20)"))
    (pad 21 smd rect (at 4.25 -0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 22 smd rect (at 4.25 -1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 123 "Net-(DD701-Pad22)"))
    (pad 23 smd rect (at 4.25 -2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(DD701-Pad23)"))
    (pad 24 smd rect (at 4.25 -2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(DD701-Pad24)"))
    (pad 25 smd rect (at 2.8 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 126 "Net-(DD701-Pad25)"))
    (pad 26 smd rect (at 2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(DD701-Pad26)"))
    (pad 27 smd rect (at 1.2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(DD701-Pad27)"))
    (pad 28 smd rect (at 0.4 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(DD701-Pad28)"))
    (pad 29 smd rect (at -0.4 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 130 "/Control circuit/~RST"))
    (pad 30 smd rect (at -1.2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 131 "Net-(DD701-Pad30)"))
    (pad 31 smd rect (at -2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(DD701-Pad31)"))
    (pad 32 smd rect (at -2.8 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(DD701-Pad32)"))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/TQFP-32_7x7mm_P0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-16_3.9x9.9mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 80.75 101 90)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference DD1301 (at 0.5 -0.5 180) (layer F.SilkS))
    (fp_text value 74HC595 (at 0 6 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 134 "Net-(DD1301-Pad1)"))
    (pad 2 smd rect (at -2.7 -3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 135 "Net-(DD1301-Pad2)"))
    (pad 3 smd rect (at -2.7 -1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 136 "Net-(DD1301-Pad3)"))
    (pad 4 smd rect (at -2.7 -0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 137 "Net-(DD1301-Pad4)"))
    (pad 5 smd rect (at -2.7 0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(DD1301-Pad5)"))
    (pad 6 smd rect (at -2.7 1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(DD1301-Pad6)"))
    (pad 7 smd rect (at -2.7 3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 140 "Net-(DD1301-Pad7)"))
    (pad 8 smd rect (at -2.7 4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 9 smd rect (at 2.7 4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 141 "/Face display/MISO"))
    (pad 10 smd rect (at 2.7 3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(DD1301-Pad10)"))
    (pad 11 smd rect (at 2.7 1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 86 /YSCK))
    (pad 12 smd rect (at 2.7 0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 143 /LED))
    (pad 13 smd rect (at 2.7 -0.635 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 14 smd rect (at 2.7 -1.905 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 87 /YMOSI))
    (pad 15 smd rect (at 2.7 -3.175 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(DD1301-Pad15)"))
    (pad 16 smd rect (at 2.7 -4.445 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 197 +3V3))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:Relay_DPDT_AXICOM_IMSeries_gull_wings (layer F.Cu) (tedit 5CDD1112)
    (at 183 133.75 90)
    (descr http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Specification+Or+Standard%7F108-98001%7FW5%7Fpdf%7FEnglish%7FENG_SS_108-98001_W5.pdf)
    (tags "AXICOM IM-Series Relay gull wing legs")
    (attr smd)
    (fp_text reference K901 (at 0.5 -0.25 45) (layer F.SilkS))
    (fp_text value IM03 (at 0 6.25 90) (layer F.Fab))
    (fp_text user %R (at 0.06 0 180) (layer F.Fab))
    (pad 1 smd rect (at -3.25 -3.8 90) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 145 "/Amplifier A/+12V"))
    (pad 2 smd rect (at -3.25 -0.6 90) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 146 "/Amplifier A/RFin"))
    (pad 3 smd rect (at -3.25 1.6 90) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(K901-Pad3)"))
    (pad 4 smd rect (at -3.25 3.8 90) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(K901-Pad4)"))
    (pad 5 smd rect (at 3.25 3.8 90) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 146 "/Amplifier A/RFin"))
    (pad 6 smd rect (at 3.25 1.6 90) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 149 "/Amplifier A/AMPBYPASS"))
    (pad 7 smd rect (at 3.25 -0.6 90) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 150 "Net-(K901-Pad7)"))
    (pad 8 smd rect (at 3.25 -3.8 90) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 151 "/Coil cur. amps/O0A"))
    (model ${KISYS3DMOD}/Relay_SMD.3dshapes/Relay_DPDT_AXICOM_IMSeries_JLeg.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:Relay_DPDT_AXICOM_IMSeries_gull_wings (layer F.Cu) (tedit 5CDD1112)
    (at 116.5 133.75 90)
    (descr http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Specification+Or+Standard%7F108-98001%7FW5%7Fpdf%7FEnglish%7FENG_SS_108-98001_W5.pdf)
    (tags "AXICOM IM-Series Relay gull wing legs")
    (attr smd)
    (fp_text reference K902 (at -0.25 -0.75 225) (layer F.SilkS))
    (fp_text value IM03 (at 0 6.25 90) (layer F.Fab))
    (fp_text user %R (at 0.06 0 180) (layer F.Fab))
    (pad 8 smd rect (at 3.25 -3.8 90) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 152 "/Coil cur. amps/O0B"))
    (pad 7 smd rect (at 3.249999 -0.6 90) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(K902-Pad7)"))
    (pad 6 smd rect (at 3.25 1.6 90) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 149 "/Amplifier A/AMPBYPASS"))
    (pad 5 smd rect (at 3.25 3.8 90) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 154 "/Amplifier A/RFout"))
    (pad 4 smd rect (at -3.25 3.8 90) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 155 "Net-(K902-Pad4)"))
    (pad 3 smd rect (at -3.25 1.6 90) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 156 "Net-(K902-Pad3)"))
    (pad 2 smd rect (at -3.25 -0.6 90) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 154 "/Amplifier A/RFout"))
    (pad 1 smd rect (at -3.25 -3.8 90) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 145 "/Amplifier A/+12V"))
    (model ${KISYS3DMOD}/Relay_SMD.3dshapes/Relay_DPDT_AXICOM_IMSeries_JLeg.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:Relay_DPDT_AXICOM_IMSeries_gull_wings (layer F.Cu) (tedit 5CDD1112)
    (at 182.75 59.75 90)
    (descr http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Specification+Or+Standard%7F108-98001%7FW5%7Fpdf%7FEnglish%7FENG_SS_108-98001_W5.pdf)
    (tags "AXICOM IM-Series Relay gull wing legs")
    (attr smd)
    (fp_text reference K1101 (at 0.25 -0.25 225) (layer F.SilkS))
    (fp_text value IM03 (at 0 6.25 90) (layer F.Fab))
    (fp_text user %R (at 0.059999 0 180) (layer F.Fab))
    (pad 8 smd rect (at 3.25 -3.8 90) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 157 "/Coil cur. amps/O1A"))
    (pad 7 smd rect (at 3.25 -0.6 90) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 158 "Net-(K1101-Pad7)"))
    (pad 6 smd rect (at 3.25 1.6 90) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 159 "/Amplifier B/AMPBYPASS"))
    (pad 5 smd rect (at 3.25 3.8 90) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 160 "/Amplifier B/RFin"))
    (pad 4 smd rect (at -3.25 3.8 90) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 161 "Net-(K1101-Pad4)"))
    (pad 3 smd rect (at -3.25 1.6 90) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 162 "Net-(K1101-Pad3)"))
    (pad 2 smd rect (at -3.25 -0.6 90) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 160 "/Amplifier B/RFin"))
    (pad 1 smd rect (at -3.25 -3.8 90) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 145 "/Amplifier A/+12V"))
    (model ${KISYS3DMOD}/Relay_SMD.3dshapes/Relay_DPDT_AXICOM_IMSeries_JLeg.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:Relay_DPDT_AXICOM_IMSeries_gull_wings (layer F.Cu) (tedit 5CDD1112)
    (at 116.25 59.75 90)
    (descr http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Specification+Or+Standard%7F108-98001%7FW5%7Fpdf%7FEnglish%7FENG_SS_108-98001_W5.pdf)
    (tags "AXICOM IM-Series Relay gull wing legs")
    (attr smd)
    (fp_text reference K1102 (at 0 -0.75 45) (layer F.SilkS))
    (fp_text value IM03 (at 0 6.25 90) (layer F.Fab))
    (fp_text user %R (at 0.06 0 180) (layer F.Fab))
    (pad 1 smd rect (at -3.25 -3.8 90) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 145 "/Amplifier A/+12V"))
    (pad 2 smd rect (at -3.25 -0.6 90) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 163 "/Amplifier B/RFout"))
    (pad 3 smd rect (at -3.25 1.6 90) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 164 "Net-(K1102-Pad3)"))
    (pad 4 smd rect (at -3.25 3.8 90) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(K1102-Pad4)"))
    (pad 5 smd rect (at 3.25 3.8 90) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 163 "/Amplifier B/RFout"))
    (pad 6 smd rect (at 3.25 1.6 90) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 159 "/Amplifier B/AMPBYPASS"))
    (pad 7 smd rect (at 3.249999 -0.6 90) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 166 "Net-(K1102-Pad7)"))
    (pad 8 smd rect (at 3.25 -3.8 90) (size 2.5 0.7) (layers F.Cu F.Paste F.Mask)
      (net 167 "/Coil cur. amps/O1B"))
    (model ${KISYS3DMOD}/Relay_SMD.3dshapes/Relay_DPDT_AXICOM_IMSeries_JLeg.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:L_Shuo_Xing_CD32 (layer F.Cu) (tedit 5E01B3DC)
    (at 234.5 139.25 180)
    (fp_text reference L1401 (at 0 -2.75 180) (layer F.SilkS))
    (fp_text value L_Core_Ferrite (at 0 2.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.3 0 180) (size 1.4 3.5) (layers F.Cu F.Paste F.Mask)
      (net 200 VDD))
    (pad 1 smd rect (at -1.3 0 180) (size 1.4 3.5) (layers F.Cu F.Paste F.Mask)
      (net 198 +3.3VA))
  )
  (module custom-devices:L_Shuo_Xing_CD32 (layer F.Cu) (tedit 5E01B3DC)
    (at 171.5 145 180)
    (fp_text reference L1402 (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value L_Core_Ferrite (at 0 2.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.3 0 180) (size 1.4 3.5) (layers F.Cu F.Paste F.Mask)
      (net 198 +3.3VA))
    (pad 2 smd rect (at 1.3 0 180) (size 1.4 3.5) (layers F.Cu F.Paste F.Mask)
      (net 199 V+))
  )
  (module custom-devices:L_Shuo_Xing_CD32 (layer F.Cu) (tedit 5E01B3DC)
    (at 229 59.5 180)
    (fp_text reference L1403 (at 0.25 -2.5 180) (layer F.SilkS))
    (fp_text value L_Core_Ferrite (at 0 2.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.3 0 180) (size 1.4 3.5) (layers F.Cu F.Paste F.Mask)
      (net 200 VDD))
    (pad 1 smd rect (at -1.3 0 180) (size 1.4 3.5) (layers F.Cu F.Paste F.Mask)
      (net 198 +3.3VA))
  )
  (module custom-devices:L_Shuo_Xing_CD32 (layer F.Cu) (tedit 5E01B3DC)
    (at 171.25 71 180)
    (fp_text reference L1404 (at 0 -2.75 180) (layer F.SilkS))
    (fp_text value L_Core_Ferrite (at 0 2.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.3 0 180) (size 1.4 3.5) (layers F.Cu F.Paste F.Mask)
      (net 198 +3.3VA))
    (pad 2 smd rect (at 1.3 0 180) (size 1.4 3.5) (layers F.Cu F.Paste F.Mask)
      (net 199 V+))
  )
  (module Package_SO:Mini-Circuits_CD542_H2.84mm (layer F.Cu) (tedit 5A365E23)
    (at 163.25 137.75 270)
    (descr https://ww2.minicircuits.com/case_style/CD542.pdf)
    (tags "RF Transformer")
    (attr smd)
    (fp_text reference T901 (at -4.75 0) (layer F.SilkS))
    (fp_text value "FIXME: ADT2-1T" (at 0 5.08 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 6 smd rect (at 2.54 -2.54 270) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(C901-Pad2)"))
    (pad 5 smd rect (at 2.54 0 270) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(C902-Pad2)"))
    (pad 4 smd rect (at 2.54 2.54 270) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(C903-Pad2)"))
    (pad 3 smd rect (at -2.54 2.54 270) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at -2.54 0 270) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -2.54 -2.54 270) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(K901-Pad3)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/Mini-Circuits_CD542_H2.84mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:Mini-Circuits_CD542_H2.84mm (layer F.Cu) (tedit 5A365E23)
    (at 137.5 137.75 90)
    (descr https://ww2.minicircuits.com/case_style/CD542.pdf)
    (tags "RF Transformer")
    (attr smd)
    (fp_text reference T902 (at 0 -4.826 90) (layer F.SilkS))
    (fp_text value "FIXME: ADT4-6T" (at 0 5.08 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2.54 -2.54 90) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(C904-Pad1)"))
    (pad 2 smd rect (at -2.54 0 90) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -2.54 2.54 90) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(C905-Pad1)"))
    (pad 4 smd rect (at 2.54 2.54 90) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 5 smd rect (at 2.54 0 90) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 176 "Net-(T902-Pad5)"))
    (pad 6 smd rect (at 2.54 -2.54 90) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 156 "Net-(K902-Pad3)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/Mini-Circuits_CD542_H2.84mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:Mini-Circuits_CD542_H2.84mm (layer F.Cu) (tedit 5E1FE698)
    (at 163 63.75 270)
    (descr https://ww2.minicircuits.com/case_style/CD542.pdf)
    (tags "RF Transformer")
    (attr smd)
    (fp_text reference T1101 (at -5.25 0) (layer F.SilkS))
    (fp_text value "FIXME: ADT2-1T" (at 0 5.08 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.54 -2.54 270) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 162 "Net-(K1101-Pad3)"))
    (pad 2 smd rect (at -2.54 0 270) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -2.54 2.54 270) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 4 smd rect (at 2.54 2.54 270) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(C1103-Pad2)"))
    (pad 5 smd rect (at 2.54 0 270) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(C1102-Pad2)"))
    (pad 6 smd rect (at 2.54 -2.54 270) (size 2.54 1.65) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(C1101-Pad2)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/Mini-Circuits_CD542_H2.84mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:SC-74-6_Handsoldering (layer F.Cu) (tedit 5CD291E1)
    (at 182.75 145 270)
    (descr "SC74-6, Handsoldering")
    (tags "SC74-6 Handsoldering")
    (attr smd)
    (fp_text reference VT1001 (at -2.75 -1.5 180) (layer F.SilkS))
    (fp_text value Q_NMOS_GDS (at 0.05 1.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.15 -0.95 180) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at -1.15 0 180) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 89 "/Control circuit/DO0"))
    (pad 3 smd rect (at -1.15 0.95 180) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 152 "/Coil cur. amps/O0B"))
    (pad 4 smd rect (at 1.15 0.95 180) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 5 smd rect (at 1.15 0 180) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 89 "/Control circuit/DO0"))
    (pad 6 smd rect (at 1.15 -0.95 180) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 151 "/Coil cur. amps/O0A"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SC-70-8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:SC-74-6_Handsoldering (layer F.Cu) (tedit 5CD291E1)
    (at 184.5 71 90)
    (descr "SC74-6, Handsoldering")
    (tags "SC74-6 Handsoldering")
    (attr smd)
    (fp_text reference VT1002 (at 0 -2.25 90) (layer F.SilkS))
    (fp_text value Q_NMOS_GDS (at 0.05 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 6 smd rect (at 1.15 -0.95) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 157 "/Coil cur. amps/O1A"))
    (pad 5 smd rect (at 1.15 0) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 94 "/Control circuit/DO1"))
    (pad 4 smd rect (at 1.15 0.95) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 3 smd rect (at -1.15 0.95) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 167 "/Coil cur. amps/O1B"))
    (pad 2 smd rect (at -1.15 0) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 94 "/Control circuit/DO1"))
    (pad 1 smd rect (at -1.15 -0.95) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SC-70-8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 254.438341 101.03969 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference X101 (at 0 -2.25 90) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 4.87 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 182 /~CS0))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 171 /~CS))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 254.438341 98.499691 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference X102 (at -0.04 4.5 270) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 4.87 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 183 /~CS1))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 171 /~CS))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 254.438342 95.95969 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference X103 (at 0.92 -2.5 270) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 4.87 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 184 /~CS2))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 171 /~CS))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 254.438341 93.419691 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference X104 (at -0.12 4.75 90) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 4.87 270) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 185 /~CS3))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 171 /~CS))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_Mega-Fit_76825-0002_2x01_P5.70mm_Horizontal (layer F.Cu) (tedit 5B780151)
    (at 259.3 70 270)
    (descr "Molex Mega-Fit Power Connectors, 76825-0002 (compatible alternatives: 172064-0002, 172064-1002), 1 Pins per row (http://www.molex.com/pdm_docs/sd/1720640002_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Mega-Fit top entry")
    (fp_text reference XP101 (at 0 -12.7 270) (layer F.SilkS))
    (fp_text value PWR (at 0 8.55 270) (layer F.Fab))
    (fp_text user %R (at 0 -15.2 270) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 3.7 3.7) (drill 1.8) (layers *.Cu *.Mask) (roundrect_rratio 0.067568)
      (net 18 GND))
    (pad 2 thru_hole circle (at 0 5.5 270) (size 3.7 3.7) (drill 1.8) (layers *.Cu *.Mask)
      (net 54 +12V))
    (pad "" np_thru_hole circle (at 0 -7.3 270) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_Mega-Fit_76825-0002_2x01_P5.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.00mm:PinHeader_2x07_P2.00mm_Horizontal (layer F.Cu) (tedit 59FED667)
    (at 269 124)
    (descr "Through hole angled pin header, 2x07, 2.00mm pitch, 4.2mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x07 2.00mm double row")
    (fp_text reference XP102 (at 4.1 -2) (layer F.SilkS))
    (fp_text value CTRL (at 4.1 14) (layer F.Fab))
    (fp_text user %R (at 4.25 6 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 169 /MISO))
    (pad 2 thru_hole oval (at 2 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 3 thru_hole oval (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 170 /MOSI))
    (pad 4 thru_hole oval (at 2 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 5 thru_hole oval (at 0 4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 168 /SCK))
    (pad 6 thru_hole oval (at 2 4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 7 thru_hole oval (at 0 6) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 182 /~CS0))
    (pad 8 thru_hole oval (at 2 6) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 9 thru_hole oval (at 0 8) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 183 /~CS1))
    (pad 10 thru_hole oval (at 2 8) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 11 thru_hole oval (at 0 10) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 184 /~CS2))
    (pad 12 thru_hole oval (at 2 10) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 13 thru_hole oval (at 0 12) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 185 /~CS3))
    (pad 14 thru_hole oval (at 2 12) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_2x07_P2.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:BarrelJack_CUI_PJ-047A (layer F.Cu) (tedit 5CECDE44)
    (at 267.1 60 180)
    (fp_text reference XP103 (at 0.6 5 180) (layer F.SilkS))
    (fp_text value PWR2 (at 0 -6 180) (layer F.Fab))
    (pad "" thru_hole oval (at -3.7 -3.7 180) (size 3.6 1.8) (drill oval 2.4 0.9) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at -3.7 3.7 180) (size 3.6 1.8) (drill oval 2.4 0.9) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2 0 180) (size 2.4 2.4) (drill 2.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at 3.7 3.3 180) (size 3 2) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 54 +12V))
    (pad 3 thru_hole oval (at 3.7 -3.3 180) (size 3 2) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 194 "Net-(XP103-Pad3)"))
    (pad 2 thru_hole oval (at 1.5 0 270) (size 3 2) (drill oval 2 1.1) (layers *.Cu *.Mask)
      (net 18 GND))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x09_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 250.84 145.5 90)
    (descr "Through hole straight pin header, 1x09, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x09 2.54mm single row")
    (fp_text reference XP1201 (at 1 -2.09 270) (layer F.SilkS))
    (fp_text value Conn_01x09_Male (at 0 22.65 90) (layer F.Fab))
    (fp_text user %R (at 0 10.16 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 130 "/Control circuit/~RST"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 168 /SCK))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 169 /MISO))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 170 /MOSI))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 171 /~CS))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 197 +3V3))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x09_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0603 (layer F.Cu) (tedit 58E0A8B2)
    (at 254.75 123 90)
    (descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference R1208 (at 2.25 0 180) (layer F.SilkS))
    (fp_text value 560 (at 0 2.8 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 5 smd rect (at 0.9 1.2 90) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 89 "/Control circuit/DO0"))
    (pad 6 smd rect (at 0.9 0.4 90) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 94 "/Control circuit/DO1"))
    (pad 8 smd rect (at 0.9 -1.2 90) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 100 /LE1))
    (pad 7 smd rect (at 0.9 -0.4 90) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 85 /LE0))
    (pad 4 smd rect (at -0.9 1.2 90) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(DD701-Pad23)"))
    (pad 2 smd rect (at -0.9 -0.4 90) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(DD701-Pad27)"))
    (pad 3 smd rect (at -0.9 0.4 90) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(DD701-Pad24)"))
    (pad 1 smd rect (at -0.9 -1.2 90) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(DD701-Pad28)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0603 (layer F.Cu) (tedit 58E0A8B2)
    (at 72.25 102.25)
    (descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference R1301 (at -0.5 2.5) (layer F.SilkS))
    (fp_text value 560 (at 0 2.8) (layer F.Fab))
    (fp_text user %R (at 0 0 -270) (layer F.Fab))
    (pad 1 smd rect (at -0.9 -1.2) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 172 "Net-(R1301-Pad1)"))
    (pad 3 smd rect (at -0.9 0.4) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 179 "Net-(R1301-Pad3)"))
    (pad 2 smd rect (at -0.9 -0.4) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 173 "Net-(R1301-Pad2)"))
    (pad 4 smd rect (at -0.9 1.2) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 178 "Net-(R1301-Pad4)"))
    (pad 7 smd rect (at 0.9 -0.4) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 135 "Net-(DD1301-Pad2)"))
    (pad 8 smd rect (at 0.9 -1.2) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 136 "Net-(DD1301-Pad3)"))
    (pad 6 smd rect (at 0.9 0.4) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 134 "Net-(DD1301-Pad1)"))
    (pad 5 smd rect (at 0.9 1.2) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(DD1301-Pad15)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0603 (layer F.Cu) (tedit 58E0A8B2)
    (at 72.25 97.5)
    (descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference R1302 (at -0.5 -2.5) (layer F.SilkS))
    (fp_text value 560 (at 0 2.8) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.9 -1.2) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 175 "Net-(R1302-Pad1)"))
    (pad 3 smd rect (at -0.9 0.4) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 181 "Net-(R1302-Pad3)"))
    (pad 2 smd rect (at -0.9 -0.4) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 174 "Net-(R1302-Pad2)"))
    (pad 4 smd rect (at -0.9 1.2) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 180 "Net-(R1302-Pad4)"))
    (pad 7 smd rect (at 0.9 -0.4) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(DD1301-Pad6)"))
    (pad 8 smd rect (at 0.9 -1.2) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 140 "Net-(DD1301-Pad7)"))
    (pad 6 smd rect (at 0.9 0.4) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(DD1301-Pad5)"))
    (pad 5 smd rect (at 0.9 1.2) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 137 "Net-(DD1301-Pad4)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:Jumper_0.9_0.68 (layer F.Cu) (tedit 5E044FF0)
    (at 250 70.75 90)
    (clearance 0.2)
    (attr smd)
    (fp_text reference X105 (at 0 -1.5 90) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.799999 0 90) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 145 "/Amplifier A/+12V") (clearance 0.6805))
    (pad 2 smd rect (at 0.799999 0 90) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 54 +12V) (clearance 0.6805))
    (model SMD_Packages.3dshapes/Conn-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:Jumper3_0.9_0.68 (layer F.Cu) (tedit 5E044E25)
    (at 213.25 135 180)
    (clearance 0.2)
    (attr smd)
    (fp_text reference X106 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value Jumper_NC_Dual (at 0 1 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0 0 180) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 186 "Net-(X106-Pad2)") (clearance 0.6805))
    (pad 1 smd rect (at -1.6 0 180) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C103-Pad1)") (clearance 0.6805))
    (pad 3 smd rect (at 1.6 0 180) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 146 "/Amplifier A/RFin") (clearance 0.6805))
    (model SMD_Packages.3dshapes/Conn-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:Jumper3_0.9_0.68 (layer F.Cu) (tedit 5E044E25)
    (at 213.25 65 180)
    (clearance 0.2)
    (attr smd)
    (fp_text reference X107 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value Jumper_NC_Dual (at 0 1 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0 0 180) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 187 "Net-(X107-Pad2)") (clearance 0.6805))
    (pad 1 smd rect (at -1.6 0 180) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C104-Pad1)") (clearance 0.6805))
    (pad 3 smd rect (at 1.6 0 180) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 160 "/Amplifier B/RFin") (clearance 0.6805))
    (model SMD_Packages.3dshapes/Conn-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:Jumper_0.9_0.68 (layer F.Cu) (tedit 5E044FF0)
    (at 59 117.5)
    (clearance 0.2)
    (attr smd)
    (fp_text reference X201 (at 0.55 -1.75) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.8 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C201-Pad2)") (clearance 0.6805))
    (pad 1 smd rect (at -0.8 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 188 "/High-pass A/FilterA") (clearance 0.6805))
    (model SMD_Packages.3dshapes/Conn-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:Jumper_0.9_0.68 (layer F.Cu) (tedit 5E044FF0)
    (at 137.799999 108)
    (clearance 0.2)
    (attr smd)
    (fp_text reference X205 (at 0.700001 1.75) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.799999 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 191 "/Low-pass A/FilterA") (clearance 0.6805))
    (pad 1 smd rect (at -0.799999 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C208-Pad1)") (clearance 0.6805))
    (model SMD_Packages.3dshapes/Conn-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:Jumper_0.9_0.68 (layer F.Cu) (tedit 5E044FF0)
    (at 141.75 108)
    (clearance 0.2)
    (attr smd)
    (fp_text reference X301 (at 0.75 1.75) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.8 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 191 "/Low-pass A/FilterA") (clearance 0.6805))
    (pad 2 smd rect (at 0.8 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C302-Pad2)") (clearance 0.6805))
    (model SMD_Packages.3dshapes/Conn-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:Jumper_0.9_0.68 (layer F.Cu) (tedit 5E0B057A)
    (at 149 108.799999 90)
    (clearance 0.2)
    (attr smd)
    (fp_text reference X302 (at 2.549999 0) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.799999 0 90) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C301-Pad2)") (clearance 0.6805))
    (pad 2 smd rect (at 0.799999 0 90) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C302-Pad2)") (clearance 0.6805))
    (model SMD_Packages.3dshapes/Conn-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:Jumper3_0.9_0.68 (layer F.Cu) (tedit 5E0AFEA0)
    (at 166 108)
    (clearance 0.2)
    (attr smd)
    (fp_text reference X303 (at 0 -2) (layer F.SilkS))
    (fp_text value Jumper_NC_Dual (at 0 1) (layer F.Fab) hide)
    (pad 3 smd rect (at 1.6 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C304-Pad2)") (clearance 0.6805))
    (pad 1 smd rect (at -1.6 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C302-Pad1)") (clearance 0.6805))
    (pad 2 smd rect (at 0 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C303-Pad2)") (clearance 0.6805))
    (model SMD_Packages.3dshapes/Conn-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:Jumper3_0.9_0.68 (layer F.Cu) (tedit 5E044E25)
    (at 185 108)
    (clearance 0.2)
    (attr smd)
    (fp_text reference X304 (at 0 -1.75) (layer F.SilkS))
    (fp_text value Jumper_NC_Dual (at 0 1) (layer F.Fab) hide)
    (pad 2 smd rect (at 0 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(C305-Pad2)") (clearance 0.6805))
    (pad 1 smd rect (at -1.6 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(C304-Pad1)") (clearance 0.6805))
    (pad 3 smd rect (at 1.6 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(C306-Pad2)") (clearance 0.6805))
    (model SMD_Packages.3dshapes/Conn-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:Jumper3_0.9_0.68 (layer F.Cu) (tedit 5E099DF5)
    (at 204 108)
    (clearance 0.2)
    (attr smd)
    (fp_text reference X305 (at 0 -2) (layer F.SilkS))
    (fp_text value Jumper_NC_Dual (at 0 1) (layer F.Fab) hide)
    (pad 2 smd rect (at 0 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C307-Pad2)") (clearance 0.6805))
    (pad 1 smd rect (at -1.6 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(C306-Pad1)") (clearance 0.6805))
    (pad 3 smd rect (at 1.6 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C308-Pad2)") (clearance 0.6805))
    (model SMD_Packages.3dshapes/Conn-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:Jumper_0.9_0.68 (layer F.Cu) (tedit 5E044FF0)
    (at 221 108.8 90)
    (clearance 0.2)
    (attr smd)
    (fp_text reference X306 (at 3.8 0.25 90) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.8 0 90) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C308-Pad1)") (clearance 0.6805))
    (pad 1 smd rect (at -0.8 0 90) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C309-Pad2)") (clearance 0.6805))
    (model SMD_Packages.3dshapes/Conn-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:Jumper_0.9_0.68 (layer F.Cu) (tedit 5E044FF0)
    (at 224 108)
    (clearance 0.2)
    (attr smd)
    (fp_text reference X307 (at 1.5 1.75) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.8 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "/Low-pass A/FilterB") (clearance 0.6805))
    (pad 1 smd rect (at -0.8 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C308-Pad1)") (clearance 0.6805))
    (model SMD_Packages.3dshapes/Conn-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:Jumper_0.9_0.68 (layer F.Cu) (tedit 5E044FF0)
    (at 59 82.5)
    (clearance 0.2)
    (attr smd)
    (fp_text reference X401 (at 0 -1.5) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.8 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C401-Pad2)") (clearance 0.6805))
    (pad 1 smd rect (at -0.8 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 192 "/High-pass B/FilterA") (clearance 0.6805))
    (model SMD_Packages.3dshapes/Conn-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:Jumper_0.9_0.68 (layer F.Cu) (tedit 5E044FF0)
    (at 137.75 93)
    (clearance 0.2)
    (attr smd)
    (fp_text reference X405 (at 1 -1.5) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.799999 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(C408-Pad1)") (clearance 0.6805))
    (pad 2 smd rect (at 0.799999 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 193 "/Low-pass B/FilterA") (clearance 0.6805))
    (model SMD_Packages.3dshapes/Conn-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:Jumper_0.9_0.68 (layer F.Cu) (tedit 5E044FF0)
    (at 141.75 93)
    (clearance 0.2)
    (attr smd)
    (fp_text reference X501 (at 1 -1.5) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.799999 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 193 "/Low-pass B/FilterA") (clearance 0.6805))
    (pad 2 smd rect (at 0.799999 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(C502-Pad2)") (clearance 0.6805))
    (model SMD_Packages.3dshapes/Conn-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:Jumper_0.9_0.68 (layer F.Cu) (tedit 5E044FF0)
    (at 149 92.200001 270)
    (clearance 0.2)
    (attr smd)
    (fp_text reference X502 (at 2.828174 0.103553 180) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.799999 0 270) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(C501-Pad2)") (clearance 0.6805))
    (pad 2 smd rect (at 0.799999 0 270) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(C502-Pad2)") (clearance 0.6805))
    (model SMD_Packages.3dshapes/Conn-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:Jumper3_0.9_0.68 (layer F.Cu) (tedit 5E044E25)
    (at 166 93)
    (clearance 0.2)
    (attr smd)
    (fp_text reference X503 (at 0 1.5) (layer F.SilkS))
    (fp_text value Jumper_NC_Dual (at 0 1) (layer F.Fab) hide)
    (pad 2 smd rect (at 0 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(C503-Pad2)") (clearance 0.6805))
    (pad 1 smd rect (at -1.6 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(C502-Pad1)") (clearance 0.6805))
    (pad 3 smd rect (at 1.6 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(C504-Pad2)") (clearance 0.6805))
    (model SMD_Packages.3dshapes/Conn-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:Jumper3_0.9_0.68 (layer F.Cu) (tedit 5E044E25)
    (at 185 93)
    (clearance 0.2)
    (attr smd)
    (fp_text reference X504 (at 0 1.75) (layer F.SilkS))
    (fp_text value Jumper_NC_Dual (at 0 1) (layer F.Fab) hide)
    (pad 3 smd rect (at 1.6 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(C506-Pad2)") (clearance 0.6805))
    (pad 1 smd rect (at -1.6 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(C504-Pad1)") (clearance 0.6805))
    (pad 2 smd rect (at 0 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(C505-Pad2)") (clearance 0.6805))
    (model SMD_Packages.3dshapes/Conn-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:Jumper3_0.9_0.68 (layer F.Cu) (tedit 5E044E25)
    (at 204 93)
    (clearance 0.2)
    (attr smd)
    (fp_text reference X505 (at 0 1.75) (layer F.SilkS))
    (fp_text value Jumper_NC_Dual (at 0 1) (layer F.Fab) hide)
    (pad 3 smd rect (at 1.6 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(C508-Pad2)") (clearance 0.6805))
    (pad 1 smd rect (at -1.6 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(C506-Pad1)") (clearance 0.6805))
    (pad 2 smd rect (at 0 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(C507-Pad2)") (clearance 0.6805))
    (model SMD_Packages.3dshapes/Conn-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:Jumper_0.9_0.68 (layer F.Cu) (tedit 5E044FF0)
    (at 221 92.2 270)
    (clearance 0.2)
    (attr smd)
    (fp_text reference X506 (at -2.2 1.75 90) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.8 0 270) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(C508-Pad1)") (clearance 0.6805))
    (pad 1 smd rect (at -0.8 0 270) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(C509-Pad2)") (clearance 0.6805))
    (model SMD_Packages.3dshapes/Conn-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:Jumper_0.9_0.68 (layer F.Cu) (tedit 5E044FF0)
    (at 224 93)
    (clearance 0.2)
    (attr smd)
    (fp_text reference X507 (at 2 -2) (layer F.SilkS))
    (fp_text value Jumper_NC_Small (at 0 1) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.8 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "/Low-pass B/FilterB") (clearance 0.6805))
    (pad 1 smd rect (at -0.8 0) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(C508-Pad1)") (clearance 0.6805))
    (model SMD_Packages.3dshapes/Conn-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:SMA_side_0.9_1.05 (layer F.Cu) (tedit 5E04989E)
    (at 52.5 117.5)
    (fp_text reference XS101 (at 0 4.5) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 -4.5) (layer F.Fab))
    (pad 2 smd rect (at 0 2.5) (size 5 2) (layers B.Cu B.Paste B.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 0 -2.5) (size 5 2) (layers B.Cu B.Paste B.Mask)
      (net 18 GND))
    (pad 1 smd rect (at 0 0) (size 5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 188 "/High-pass A/FilterA"))
    (pad 2 smd rect (at 0 -2.5) (size 5 2) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 0 2.5) (size 5 2) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
  )
  (module custom-devices:SMA_side_0.9_1.05 (layer F.Cu) (tedit 5E04989E)
    (at 52.5 82.5)
    (fp_text reference XS102 (at 0 4.5) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 -4.5) (layer F.Fab))
    (pad 2 smd rect (at 0 2.5) (size 5 2) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 0 -2.5) (size 5 2) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 1 smd rect (at 0 0) (size 5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 192 "/High-pass B/FilterA"))
    (pad 2 smd rect (at 0 -2.5) (size 5 2) (layers B.Cu B.Paste B.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 0 2.5) (size 5 2) (layers B.Cu B.Paste B.Mask)
      (net 18 GND))
  )
  (module custom-devices:SMA_side_0.9_1.05 (layer F.Cu) (tedit 5E04989E)
    (at 53 135)
    (fp_text reference XS109 (at 0 -4.5) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 -4.5) (layer F.Fab))
    (pad 2 smd rect (at 0 2.5) (size 5 2) (layers B.Cu B.Paste B.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 0 -2.5) (size 5 2) (layers B.Cu B.Paste B.Mask)
      (net 18 GND))
    (pad 1 smd rect (at 0 0) (size 5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 154 "/Amplifier A/RFout"))
    (pad 2 smd rect (at 0 -2.5) (size 5 2) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 0 2.5) (size 5 2) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
  )
  (module custom-devices:SMA_side_0.9_1.05 (layer F.Cu) (tedit 5E04989E)
    (at 52.5 65)
    (fp_text reference XS110 (at 0 4.5) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 -4.5) (layer F.Fab))
    (pad 2 smd rect (at 0 2.5) (size 5 2) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 0 -2.5) (size 5 2) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 1 smd rect (at 0 0) (size 5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 163 "/Amplifier B/RFout"))
    (pad 2 smd rect (at 0 -2.5) (size 5 2) (layers B.Cu B.Paste B.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 0 2.5) (size 5 2) (layers B.Cu B.Paste B.Mask)
      (net 18 GND))
  )
  (module custom-devices:Schroff-60807-181 (layer F.Cu) (tedit 5E049B0C)
    (at 53.57 55.55)
    (fp_text reference X112 (at 0 3.7) (layer F.SilkS))
    (fp_text value MountingHole_Pad (at 0 -5.4) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask)
      (net 18 GND))
  )
  (module custom-devices:Amphenol-73950-1005LF (layer F.Cu) (tedit 5E254DAD)
    (at 271.1 96 90)
    (fp_text reference P101 (at 0 -3.1 90) (layer F.SilkS))
    (fp_text value Amphenol73950 (at 0 -0.5 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at 4 0 90) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -4 0 90) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad 2D4 thru_hole circle (at -13 -10 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 185 /~CS3))
    (pad 2E3 thru_hole circle (at -11 -12 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 2C4 thru_hole circle (at -13 -8 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 183 /~CS1))
    (pad 2B5 thru_hole circle (at -15 -6 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 182 /~CS0))
    (pad 2A5 thru_hole circle (at -15 -4 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 169 /MISO))
    (pad 2E4 thru_hole circle (at -13 -12 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 2E6 thru_hole circle (at -17 -12 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 2B6 thru_hole circle (at -17 -6 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 182 /~CS0))
    (pad 2E5 thru_hole circle (at -15 -12 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 2D5 thru_hole circle (at -15 -10 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 185 /~CS3))
    (pad 2C6 thru_hole circle (at -17 -8 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 183 /~CS1))
    (pad 2E1 thru_hole circle (at -7 -12 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 2D3 thru_hole circle (at -11 -10 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 2A3 thru_hole circle (at -11 -4 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 170 /MOSI))
    (pad 2A4 thru_hole circle (at -13 -4 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 169 /MISO))
    (pad 2A6 thru_hole circle (at -17 -4 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 169 /MISO))
    (pad 2C5 thru_hole circle (at -15 -8 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 183 /~CS1))
    (pad 2B3 thru_hole circle (at -11 -6 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 168 /SCK))
    (pad 2B4 thru_hole circle (at -13 -6 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 182 /~CS0))
    (pad 2C2 thru_hole circle (at -9 -8 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 184 /~CS2))
    (pad 2D6 thru_hole circle (at -17 -10 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 185 /~CS3))
    (pad 2C1 thru_hole circle (at -7 -8 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 184 /~CS2))
    (pad 2C3 thru_hole circle (at -11 -8 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 184 /~CS2))
    (pad 2A2 thru_hole circle (at -9 -4 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 170 /MOSI))
    (pad 2B2 thru_hole circle (at -9 -6 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 168 /SCK))
    (pad 2A1 thru_hole circle (at -7 -4 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 170 /MOSI))
    (pad 2B1 thru_hole circle (at -7 -6 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 168 /SCK))
    (pad 2E2 thru_hole circle (at -9 -12 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 2D1 thru_hole circle (at -7 -10 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 2D2 thru_hole circle (at -9 -10 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 1B6 thru_hole circle (at 7 -6 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 1A6 thru_hole circle (at 7 -4 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 1E6 thru_hole circle (at 7 -12 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 1D6 thru_hole circle (at 7 -10 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 1C6 thru_hole circle (at 7 -8 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 1D5 thru_hole circle (at 9 -10 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 1C5 thru_hole circle (at 9 -8 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 1E5 thru_hole circle (at 9 -12 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 1A5 thru_hole circle (at 9 -4 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 1B5 thru_hole circle (at 9 -6 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 1E4 thru_hole circle (at 11 -12 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 1D4 thru_hole circle (at 11 -10 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 1A4 thru_hole circle (at 11 -4 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 1B4 thru_hole circle (at 11 -6 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 1C4 thru_hole circle (at 11 -8 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 1C3 thru_hole circle (at 13 -8 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 +12V))
    (pad 1A3 thru_hole circle (at 13 -4 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 +12V))
    (pad 1B3 thru_hole circle (at 13 -6 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 +12V))
    (pad 1E3 thru_hole circle (at 13 -12 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 +12V))
    (pad 1D3 thru_hole circle (at 13 -10 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 +12V))
    (pad 1E2 thru_hole circle (at 15 -12 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 +12V))
    (pad 1C2 thru_hole circle (at 15 -8 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 +12V))
    (pad 1A2 thru_hole circle (at 15 -4 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 +12V))
    (pad 1B2 thru_hole circle (at 15 -6 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 +12V))
    (pad 1D2 thru_hole circle (at 15 -10 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 +12V))
    (pad 1E1 thru_hole circle (at 17 -12 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 +12V))
    (pad 1D1 thru_hole circle (at 17 -10 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 +12V))
    (pad 1C1 thru_hole circle (at 17 -8 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 +12V))
    (pad 1B1 thru_hole circle (at 17 -6 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 +12V))
    (pad 1A1 thru_hole circle (at 17 -4 90) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 +12V))
    (pad "" np_thru_hole circle (at 16 0 90) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 8 0 90) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -16 0 90) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -8 0 90) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 12 0 90) (size 2.05 2.05) (drill 2.05) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -12 0 90) (size 2.05 2.05) (drill 2.05) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 2.05 2.05) (drill 2.05) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x07_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 251 106.75)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference XP104 (at -0.5 -2.25) (layer F.SilkS))
    (fp_text value Out_Test_Connector (at 0 17.57) (layer F.Fab))
    (fp_text user %R (at 0 7.62 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 86 /YSCK))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 87 /YMOSI))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 "/Control circuit/DO0"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 94 "/Control circuit/DO1"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 /LE0))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 100 /LE1))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 143 /LED))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0603-1206_HandSoldering (layer F.Cu) (tedit 5D45451F)
    (at 257 63 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C601 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 10u (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.675 0 180) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 54 +12V))
    (pad 2 smd rect (at 1.675 0 180) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0603-1206_HandSoldering (layer F.Cu) (tedit 5D45451F)
    (at 252 56 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C602 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 10u (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.675 0 90) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 1 smd rect (at -1.675 0 90) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 197 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0603-1206_HandSoldering (layer F.Cu) (tedit 5D45451F)
    (at 252.25 89 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C603 (at -3 -1.5 180) (layer F.SilkS))
    (fp_text value 10µ (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.675 0 180) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 1.675 0 180) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 198 +3.3VA))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0603-1206_HandSoldering (layer F.Cu) (tedit 5D45451F)
    (at 250 81 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C604 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 4.7µ (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.675 0 90) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 1 smd rect (at -1.675 0 90) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(C604-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0603-1206_HandSoldering (layer F.Cu) (tedit 5D45451F)
    (at 256 76 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C605 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 4.7µ (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.675 0 180) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 201 +12VA))
    (pad 2 smd rect (at 1.675 0 180) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 250.25 75.25 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R603 (at 0 -1.7 270) (layer F.SilkS))
    (fp_text value 1k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(DA602-Pad5)"))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 252.5 86 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R604 (at -2.75 -1.5 180) (layer F.SilkS))
    (fp_text value 30.1k (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(C604-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 261.75 76)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R605 (at 4.25 0) (layer F.SilkS))
    (fp_text value 0R0 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 201 +12VA))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 54 +12V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 227.75 135)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C101 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 1u (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "/Attenuator A/RFin"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "/Low-pass A/FilterB"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 227.5 65)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C102 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 1u (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "/Low-pass B/FilterB"))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "/Attenuator B/RFin"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 217 135)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C103 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 1u (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C103-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "/Attenuator A/RFout"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 217 65)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C104 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 1u (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C104-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "/Attenuator B/RFout"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 164.75 143)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C901 (at -0.75 1.5) (layer F.SilkS))
    (fp_text value 0.1µ (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(C901-Pad2)"))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 57 "/Amplifier A/IN+"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 168.75 139.5 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C902 (at 0 1.75 90) (layer F.SilkS))
    (fp_text value 0.1µ (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(C902-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 156.5 140.5)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C903 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 0.1µ (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(C903-Pad2)"))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 59 "/Amplifier A/IN-"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 136.25 143)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C904 (at 0 1.75) (layer F.SilkS))
    (fp_text value 0.1µ (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(C904-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 61 "/Amplifier A/OUT+"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 144.25 140.5)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C905 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 0.1µ (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 64 "/Amplifier A/OUT-"))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(C905-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0603-1206_HandSoldering (layer F.Cu) (tedit 5D45451F)
    (at 150.25 140.5 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C906 (at 4.25 -2.25 225) (layer F.SilkS))
    (fp_text value 10µ (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.675 0 180) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 1.675 0 180) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 65 "/Amplifier A/Vocm"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0603-1206_HandSoldering (layer F.Cu) (tedit 5D45451F)
    (at 155.5 134.75 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C907 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 10µ (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.675 0 180) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 1.675 0 180) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 65 "/Amplifier A/Vocm"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 164.5 69)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1101 (at -1 1.5) (layer F.SilkS))
    (fp_text value 0.1µ (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(C1101-Pad2)"))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 66 "/Amplifier B/IN+"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 168.75 65.75 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1102 (at 0 1.5 90) (layer F.SilkS))
    (fp_text value 0.1µ (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(C1102-Pad2)"))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 156.125 66.5)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1103 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 0.1µ (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 70 "/Amplifier B/IN-"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(C1103-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 136 69)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1104 (at 0 1.75) (layer F.SilkS))
    (fp_text value 0.1µ (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 72 "/Amplifier B/OUT+"))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(C1104-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 143.875001 66.5)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1105 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 0.1µ (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(C1105-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 73 "/Amplifier B/OUT-"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0603-1206_HandSoldering (layer F.Cu) (tedit 5D45451F)
    (at 150 66.5 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1106 (at 4.75 -3 225) (layer F.SilkS))
    (fp_text value 10µ (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.675 0 180) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 1.675 0 180) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 75 "/Amplifier B/Vocm"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0603-1206_HandSoldering (layer F.Cu) (tedit 5D45451F)
    (at 155.25 60.75 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1107 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 10µ (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.675 0 180) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 75 "/Amplifier B/Vocm"))
    (pad 1 smd rect (at -1.675 0 180) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0603-1206_HandSoldering (layer F.Cu) (tedit 5D45451F)
    (at 174.75 145 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1401 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 10u (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.675 0 270) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 198 +3.3VA))
    (pad 2 smd rect (at 1.675 0 270) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0603-1206_HandSoldering (layer F.Cu) (tedit 5D45451F)
    (at 231.25 139.25 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1402 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 10u (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.675 0 90) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 1 smd rect (at -1.675 0 90) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 200 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0603-1206_HandSoldering (layer F.Cu) (tedit 5D45451F)
    (at 232.5 59.5 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1403 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 10u (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.675 0 270) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 198 +3.3VA))
    (pad 2 smd rect (at 1.675 0 270) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0603-1206_HandSoldering (layer F.Cu) (tedit 5D45451F)
    (at 168.25 145.25 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1404 (at -1.25 -1.75 90) (layer F.SilkS))
    (fp_text value 10u (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.675 0 90) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 1 smd rect (at -1.675 0 90) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 199 V+))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0603-1206_HandSoldering (layer F.Cu) (tedit 5D45451F)
    (at 174.5 71.25 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1405 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 10u (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 2 smd rect (at 1.675 0 270) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 1 smd rect (at -1.675 0 270) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 198 +3.3VA))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0603-1206_HandSoldering (layer F.Cu) (tedit 5D45451F)
    (at 225.75 58.75 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1406 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 10u (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.675 0 90) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 1 smd rect (at -1.675 0 90) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 200 VDD))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0603-1206_HandSoldering (layer F.Cu) (tedit 5D45451F)
    (at 238 139.25 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1407 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 10u (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.675 0 270) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 198 +3.3VA))
    (pad 2 smd rect (at 1.675 0 270) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom-devices:C_0603-1206_HandSoldering (layer F.Cu) (tedit 5D45451F)
    (at 168.056156 71.25 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1408 (at -1 -1.75 90) (layer F.SilkS))
    (fp_text value 10u (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.675 0 90) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 1 smd rect (at -1.675 0 90) (size 2.65 1.6) (layers F.Cu F.Paste F.Mask)
      (net 199 V+))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 225 139.5 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R701 (at -4 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(DA701-Pad20)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 223 139.5 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R702 (at -4 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(DA701-Pad19)"))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 221 139.5 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R703 (at -4 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(DA701-Pad17)"))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 219 139.5 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R704 (at -4 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(DA701-Pad16)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 217 139.5 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R705 (at -4 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(DA701-Pad15)"))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 227 139.5 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R706 (at -4 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(DA701-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 189.5 133.75 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R901 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 50 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(K901-Pad4)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 123 133.75 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R902 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 50 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 155 "Net-(K902-Pad4)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 176.75 134.75 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R903 (at 0 -1.7 270) (layer F.SilkS))
    (fp_text value 50 (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 150 "Net-(K901-Pad7)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 110 134.5 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R904 (at 0 -1.7 270) (layer F.SilkS))
    (fp_text value 50 (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(K902-Pad7)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 154.75 145.75)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R905 (at 0 -1.7) (layer F.SilkS))
    (fp_text value "1k ±1%" (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 65 "/Amplifier A/Vocm"))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 199 V+))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 159.5 145.75 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R906 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value "1k ±1%" (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 65 "/Amplifier A/Vocm"))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 189.25 59.75 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1101 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 50 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 161 "Net-(K1101-Pad4)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 122.75 60 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1102 (at 0 1.75 90) (layer F.SilkS))
    (fp_text value 50 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(K1102-Pad4)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 176.25 60.75 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1103 (at 0 -1.7 270) (layer F.SilkS))
    (fp_text value 50 (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 158 "Net-(K1101-Pad7)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 109.75 60.25 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1104 (at -5 0 270) (layer F.SilkS))
    (fp_text value 50 (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 166 "Net-(K1102-Pad7)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 154.5 71.75)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1105 (at 0 -1.7) (layer F.SilkS))
    (fp_text value "1k ±1%" (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 75 "/Amplifier B/Vocm"))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 199 V+))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 159.25 71.75 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1106 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value "1k ±1%" (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 75 "/Amplifier B/Vocm"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 265 128)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1201 (at -4.25 -1.25 -45) (layer F.SilkS))
    (fp_text value 680 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(DD701-Pad17)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 168 /SCK))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 265 124)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1202 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 47 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 169 /MISO))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(DD701-Pad16)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 265 126)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1203 (at -4.25 -1.25 -45) (layer F.SilkS))
    (fp_text value 680 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(DD701-Pad15)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 170 /MOSI))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 265 130)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1204 (at 0 2) (layer F.SilkS))
    (fp_text value 680 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 171 /~CS))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(DD701-Pad14)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 254.25 141.25 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1205 (at -1.5 -3.25) (layer F.SilkS))
    (fp_text value 100k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 130 "/Control circuit/~RST"))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 197 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 255.25 106.75 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1206 (at 0 1.5 180) (layer F.SilkS))
    (fp_text value 47 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(DD701-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 86 /YSCK))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 251 138.75)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1207 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 680 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 202 "/Control circuit/RDY"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 108 "Net-(DD701-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 255.25 109.25 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1209 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value 47 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 87 /YMOSI))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(DD701-Pad31)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 250.25 125.75 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1210 (at 0 -1.7 270) (layer F.SilkS))
    (fp_text value 560 (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 143 /LED))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(DD701-Pad26)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 87.5 101.25 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1309 (at 0 -1.7 270) (layer F.SilkS))
    (fp_text value 100k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 197 +3V3))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(DD1301-Pad10)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 225 69.5 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1401 (at -4.75 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(DA1401-Pad20)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 223 69.5 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1402 (at -4.75 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 106 "Net-(DA1401-Pad19)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 221 69.5 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1403 (at -4.75 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(DA1401-Pad17)"))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 219 69.5 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1404 (at -4.75 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(DA1401-Pad16)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 217 69.5 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1405 (at -4.75 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(DA1401-Pad15)"))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 227 69.5 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1406 (at -4.75 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(DA1401-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 174.5 134.25 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference VD901 (at 0 -2 90) (layer F.SilkS))
    (fp_text value D (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 151 "/Coil cur. amps/O0A"))
    (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 145 "/Amplifier A/+12V"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 107.25 134 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference VD902 (at 0 -2 90) (layer F.SilkS))
    (fp_text value D (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 145 "/Amplifier A/+12V"))
    (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 152 "/Coil cur. amps/O0B"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 173.75 60.25 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference VD1101 (at 0 -2 90) (layer F.SilkS))
    (fp_text value D (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 145 "/Amplifier A/+12V"))
    (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 157 "/Coil cur. amps/O1A"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 107.25 60 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference VD1102 (at 0 -2 90) (layer F.SilkS))
    (fp_text value D (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 167 "/Coil cur. amps/O1B"))
    (pad 1 smd rect (at -1.65 0 90) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 145 "/Amplifier A/+12V"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 595FC9C0)
    (at 53 100)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference VD1207 (at 5 0) (layer F.SilkS))
    (fp_text value RDY (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 202 "/Control circuit/RDY"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 595FC9C0)
    (at 53 110)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference VD1301 (at 5 0) (layer F.SilkS))
    (fp_text value LED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 178 "Net-(R1301-Pad4)"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 595FC9C0)
    (at 53 107.5)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference VD1302 (at 5 0) (layer F.SilkS))
    (fp_text value LED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 179 "Net-(R1301-Pad3)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 595FC9C0)
    (at 53 105)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference VD1303 (at 5 0) (layer F.SilkS))
    (fp_text value LED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 173 "Net-(R1301-Pad2)"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 595FC9C0)
    (at 53 102.5)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference VD1304 (at 5 0) (layer F.SilkS))
    (fp_text value LED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 172 "Net-(R1301-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603_HandSoldering locked (layer F.Cu) (tedit 595FC9C0)
    (at 53 97.5)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference VD1305 (at 5 0) (layer F.SilkS))
    (fp_text value LED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 180 "Net-(R1302-Pad4)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603_HandSoldering locked (layer F.Cu) (tedit 595FC9C0)
    (at 53 95)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference VD1306 (at 5 0) (layer F.SilkS))
    (fp_text value LED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 181 "Net-(R1302-Pad3)"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603_HandSoldering locked (layer F.Cu) (tedit 595FC9C0)
    (at 53 92.5)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference VD1307 (at 5 0.25) (layer F.SilkS))
    (fp_text value LED (at 0 1.55) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 174 "Net-(R1302-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603_HandSoldering locked (layer F.Cu) (tedit 595FC9C0)
    (at 53 90)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference VD1308 (at 5 0.25) (layer F.SilkS))
    (fp_text value LED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 175 "Net-(R1302-Pad1)"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module custom-devices:L_12_n45 (layer F.Cu) (tedit 5E169FBC)
    (at 98 120 225)
    (fp_text reference L201 (at 1.7 2.35 225) (layer F.SilkS))
    (fp_text value L (at 0 12.75 225) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 225) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad 1 smd rect (at -5 4 225) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C201-Pad1)"))
    (pad 2 smd rect (at 5 -4 225) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
  )
  (module custom-devices:L_12_n45 (layer F.Cu) (tedit 5E169FBC)
    (at 116 120 225)
    (fp_text reference L202 (at 1.7 2.35 225) (layer F.SilkS))
    (fp_text value L (at 0 12.75 225) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 225) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad 1 smd rect (at -5 4 225) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C204-Pad1)"))
    (pad 2 smd rect (at 5 -4 225) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
  )
  (module custom-devices:L_12_n45 (layer F.Cu) (tedit 5E169FBC)
    (at 134 120 225)
    (fp_text reference L203 (at 1.7 2.35 225) (layer F.SilkS))
    (fp_text value L (at 0 12.75 225) (layer F.Fab) hide)
    (pad 2 smd rect (at 5 -4 225) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 1 smd rect (at -5 4 225) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C207-Pad1)"))
    (pad "" np_thru_hole circle (at 0 0 225) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module custom-devices:L_12_45 (layer F.Cu) (tedit 5DF32BFA)
    (at 98 81 315)
    (fp_text reference L401 (at 1.7 2.35 315) (layer F.SilkS))
    (fp_text value L (at 0 12.75 315) (layer F.Fab) hide)
    (pad 2 smd rect (at -5 -4 315) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 1 smd rect (at 5 4 315) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C401-Pad1)"))
    (pad "" np_thru_hole circle (at 0 0 315) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module custom-devices:L_12_45 (layer F.Cu) (tedit 5DF32BFA)
    (at 116 81 315)
    (fp_text reference L402 (at 1.7 2.35 315) (layer F.SilkS))
    (fp_text value L (at 0 12.75 315) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 315) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad 1 smd rect (at 5 4 315) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C404-Pad1)"))
    (pad 2 smd rect (at -5 -4 315) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
  )
  (module custom-devices:L_12_45 (layer F.Cu) (tedit 5DF32BFA)
    (at 134 81 315)
    (fp_text reference L403 (at 1.7 2.35 315) (layer F.SilkS))
    (fp_text value L (at 0 12.75 315) (layer F.Fab) hide)
    (pad 2 smd rect (at -5 -4 315) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 1 smd rect (at 5 4 315) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(C407-Pad1)"))
    (pad "" np_thru_hole circle (at 0 0 315) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module custom-devices:0.9w-5r-angle90 (layer F.Cu) (tedit 5E8C867B)
    (at 235 130 180)
    (fp_text reference REF** (at 0 0.5 180) (layer F.SilkS) hide)
    (fp_text value 0.9w-5r-angle90 (at 0 -0.5 180) (layer F.Fab))
    (pad 1 smd custom (at 0 0 180) (size 0.9 0.9) (layers F.Cu)
      (net 2 "/Low-pass A/FilterB") (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_line (start 0 0) (end 0.00685 -0.26168) (width 0.9))
        (gr_line (start 0.00685 -0.26168) (end 0.02739 -0.52264) (width 0.9))
        (gr_line (start 0.02739 -0.52264) (end 0.06156 -0.78217) (width 0.9))
        (gr_line (start 0.06156 -0.78217) (end 0.10926 -1.03956) (width 0.9))
        (gr_line (start 0.10926 -1.03956) (end 0.17037 -1.2941) (width 0.9))
        (gr_line (start 0.17037 -1.2941) (end 0.24472 -1.54508) (width 0.9))
        (gr_line (start 0.24472 -1.54508) (end 0.3321 -1.79184) (width 0.9))
        (gr_line (start 0.3321 -1.79184) (end 0.43227 -2.03368) (width 0.9))
        (gr_line (start 0.43227 -2.03368) (end 0.54497 -2.26995) (width 0.9))
        (gr_line (start 0.54497 -2.26995) (end 0.66987 -2.5) (width 0.9))
        (gr_line (start 0.66987 -2.5) (end 0.80665 -2.7232) (width 0.9))
        (gr_line (start 0.80665 -2.7232) (end 0.95492 -2.93893) (width 0.9))
        (gr_line (start 0.95492 -2.93893) (end 1.11427 -3.1466) (width 0.9))
        (gr_line (start 1.11427 -3.1466) (end 1.28428 -3.34565) (width 0.9))
        (gr_line (start 1.28428 -3.34565) (end 1.46447 -3.53553) (width 0.9))
        (gr_line (start 1.46447 -3.53553) (end 1.65435 -3.71572) (width 0.9))
        (gr_line (start 1.65435 -3.71572) (end 1.8534 -3.88573) (width 0.9))
        (gr_line (start 1.8534 -3.88573) (end 2.06107 -4.04508) (width 0.9))
        (gr_line (start 2.06107 -4.04508) (end 2.2768 -4.19335) (width 0.9))
        (gr_line (start 2.2768 -4.19335) (end 2.5 -4.33013) (width 0.9))
        (gr_line (start 2.5 -4.33013) (end 2.73005 -4.45503) (width 0.9))
        (gr_line (start 2.73005 -4.45503) (end 2.96632 -4.56773) (width 0.9))
        (gr_line (start 2.96632 -4.56773) (end 3.20816 -4.6679) (width 0.9))
        (gr_line (start 3.20816 -4.6679) (end 3.45492 -4.75528) (width 0.9))
        (gr_line (start 3.45492 -4.75528) (end 3.7059 -4.82963) (width 0.9))
        (gr_line (start 3.7059 -4.82963) (end 3.96044 -4.89074) (width 0.9))
        (gr_line (start 3.96044 -4.89074) (end 4.21783 -4.93844) (width 0.9))
        (gr_line (start 4.21783 -4.93844) (end 4.47736 -4.97261) (width 0.9))
        (gr_line (start 4.47736 -4.97261) (end 4.73832 -4.99315) (width 0.9))
        (gr_line (start 4.73832 -4.99315) (end 5 -5) (width 0.9))
      ))
    (pad 1 smd circle (at 5 -5 180) (size 0.9 0.9) (layers F.Cu)
      (net 2 "/Low-pass A/FilterB"))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965 (layer F.Cu) (tedit 5E8EEB4E)
    (at 64 92.5)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965 (at 0 3.8) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 5E8EEFE0)
    (at 75 140)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965_Pad (at 0 3.8) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 18 GND))
  )
  (dimension 3.5 (width 0.3) (layer Dwgs.User)
    (gr_text "3,500 мм" (at 44.4 88.037889 90) (layer Dwgs.User))
    (feature1 (pts (xy 50 86.287889) (xy 45.913579 86.287889)))
    (feature2 (pts (xy 50 89.787889) (xy 45.913579 89.787889)))
    (crossbar (pts (xy 46.5 89.787889) (xy 46.5 86.287889)))
    (arrow1a (pts (xy 46.5 86.287889) (xy 47.086421 87.414393)))
    (arrow1b (pts (xy 46.5 86.287889) (xy 45.913579 87.414393)))
    (arrow2a (pts (xy 46.5 89.787889) (xy 47.086421 88.661385)))
    (arrow2b (pts (xy 46.5 89.787889) (xy 45.913579 88.661385)))
  )
  (dimension 17.5 (width 0.3) (layer Dwgs.User)
    (gr_text "17,500 мм" (at 42.4 73.75 270) (layer Dwgs.User))
    (feature1 (pts (xy 50 82.5) (xy 43.913579 82.5)))
    (feature2 (pts (xy 50 65) (xy 43.913579 65)))
    (crossbar (pts (xy 44.5 65) (xy 44.5 82.5)))
    (arrow1a (pts (xy 44.5 82.5) (xy 43.913579 81.373496)))
    (arrow1b (pts (xy 44.5 82.5) (xy 45.086421 81.373496)))
    (arrow2a (pts (xy 44.5 65) (xy 43.913579 66.126504)))
    (arrow2b (pts (xy 44.5 65) (xy 45.086421 66.126504)))
  )
  (dimension 17.5 (width 0.3) (layer Dwgs.User)
    (gr_text "17,500 мм" (at 42.4 126.25 270) (layer Dwgs.User))
    (feature1 (pts (xy 50 135) (xy 43.913579 135)))
    (feature2 (pts (xy 50 117.5) (xy 43.913579 117.5)))
    (crossbar (pts (xy 44.5 117.5) (xy 44.5 135)))
    (arrow1a (pts (xy 44.5 135) (xy 43.913579 133.873496)))
    (arrow1b (pts (xy 44.5 135) (xy 45.086421 133.873496)))
    (arrow2a (pts (xy 44.5 117.5) (xy 43.913579 118.626504)))
    (arrow2b (pts (xy 44.5 117.5) (xy 45.086421 118.626504)))
  )
  (dimension 15 (width 0.3) (layer Dwgs.User)
    (gr_text "15,000 мм" (at 39.9 142.5 270) (layer Dwgs.User))
    (feature1 (pts (xy 50 150) (xy 41.413579 150)))
    (feature2 (pts (xy 50 135) (xy 41.413579 135)))
    (crossbar (pts (xy 42 135) (xy 42 150)))
    (arrow1a (pts (xy 42 150) (xy 41.413579 148.873496)))
    (arrow1b (pts (xy 42 150) (xy 42.586421 148.873496)))
    (arrow2a (pts (xy 42 135) (xy 41.413579 136.126504)))
    (arrow2b (pts (xy 42 135) (xy 42.586421 136.126504)))
  )
  (dimension 15 (width 0.3) (layer Dwgs.User)
    (gr_text "15,000 мм" (at 39.9 57.5 270) (layer Dwgs.User))
    (feature1 (pts (xy 50 65) (xy 41.413579 65)))
    (feature2 (pts (xy 50 50) (xy 41.413579 50)))
    (crossbar (pts (xy 42 50) (xy 42 65)))
    (arrow1a (pts (xy 42 65) (xy 41.413579 63.873496)))
    (arrow1b (pts (xy 42 65) (xy 42.586421 63.873496)))
    (arrow2a (pts (xy 42 50) (xy 41.413579 51.126504)))
    (arrow2b (pts (xy 42 50) (xy 42.586421 51.126504)))
  )
  (gr_text "LED\n" (at 246 122) (layer F.SilkS))
  (gr_text LE1 (at 246 119.5) (layer F.SilkS))
  (gr_text LE0 (at 246 117) (layer F.SilkS))
  (gr_text DO1 (at 246 114.5) (layer F.SilkS))
  (gr_text DO0 (at 246 112) (layer F.SilkS))
  (gr_text YMOSI (at 246 109.22) (layer F.SilkS))
  (gr_text YSCK (at 246 106.807) (layer F.SilkS))
  (dimension 7.5 (width 0.3) (layer Dwgs.User)
    (gr_text "7,500 мм" (at 36.4 86.25 90) (layer Dwgs.User))
    (feature1 (pts (xy 50 82.5) (xy 37.913579 82.5)))
    (feature2 (pts (xy 50 90) (xy 37.913579 90)))
    (crossbar (pts (xy 38.5 90) (xy 38.5 82.5)))
    (arrow1a (pts (xy 38.5 82.5) (xy 39.086421 83.626504)))
    (arrow1b (pts (xy 38.5 82.5) (xy 37.913579 83.626504)))
    (arrow2a (pts (xy 38.5 90) (xy 39.086421 88.873496)))
    (arrow2b (pts (xy 38.5 90) (xy 37.913579 88.873496)))
  )
  (dimension 7.5 (width 0.3) (layer Dwgs.User)
    (gr_text "7,500 мм" (at 42.4 113.75 270) (layer Dwgs.User))
    (feature1 (pts (xy 50 117.5) (xy 43.913579 117.5)))
    (feature2 (pts (xy 50 110) (xy 43.913579 110)))
    (crossbar (pts (xy 44.5 110) (xy 44.5 117.5)))
    (arrow1a (pts (xy 44.5 117.5) (xy 43.913579 116.373496)))
    (arrow1b (pts (xy 44.5 117.5) (xy 45.086421 116.373496)))
    (arrow2a (pts (xy 44.5 110) (xy 43.913579 111.126504)))
    (arrow2b (pts (xy 44.5 110) (xy 45.086421 111.126504)))
  )
  (gr_text GND (at 271.25 142.75 90) (layer F.SilkS))
  (gr_text 3V3 (at 268.75 142.75 90) (layer F.SilkS))
  (gr_text ~CS~ (at 266.25 143 90) (layer F.SilkS))
  (gr_text MOSI (at 263.5 142.5 90) (layer F.SilkS))
  (gr_text MISO (at 261 142.5 90) (layer F.SilkS))
  (gr_text SCK (at 258.5 142.75 90) (layer F.SilkS))
  (gr_text ~RST~ (at 256 142.75 90) (layer F.SilkS))
  (gr_text GND (at 252.25 142.5) (layer F.SilkS))
  (dimension 10 (width 0.3) (layer Dwgs.User)
    (gr_text "10,000 мм" (at 287.1 65 270) (layer Dwgs.User))
    (feature1 (pts (xy 274 70) (xy 285.586421 70)))
    (feature2 (pts (xy 274 60) (xy 285.586421 60)))
    (crossbar (pts (xy 285 60) (xy 285 70)))
    (arrow1a (pts (xy 285 70) (xy 284.413579 68.873496)))
    (arrow1b (pts (xy 285 70) (xy 285.586421 68.873496)))
    (arrow2a (pts (xy 285 60) (xy 284.413579 61.126504)))
    (arrow2b (pts (xy 285 60) (xy 285.586421 61.126504)))
  )
  (dimension 10 (width 0.3) (layer Dwgs.User)
    (gr_text "10,000 мм" (at 287.1 55 270) (layer Dwgs.User))
    (feature1 (pts (xy 274 60) (xy 285.586421 60)))
    (feature2 (pts (xy 274 50) (xy 285.586421 50)))
    (crossbar (pts (xy 285 50) (xy 285 60)))
    (arrow1a (pts (xy 285 60) (xy 284.413579 58.873496)))
    (arrow1b (pts (xy 285 60) (xy 285.586421 58.873496)))
    (arrow2a (pts (xy 285 50) (xy 284.413579 51.126504)))
    (arrow2b (pts (xy 285 50) (xy 285.586421 51.126504)))
  )
  (gr_text "МНАС.758725.005\nМНАС.687264.006" (at 72.5 125) (layer F.Cu))
  (dimension 100 (width 0.3) (layer Dwgs.User)
    (gr_text "100,000 мм" (at 305.100254 99.999842 -89.99970894) (layer Dwgs.User))
    (feature1 (pts (xy 274.1 50) (xy 303.586421 49.99985)))
    (feature2 (pts (xy 274.100508 150) (xy 303.586929 149.99985)))
    (crossbar (pts (xy 303.000508 149.999853) (xy 303 49.999853)))
    (arrow1a (pts (xy 303 49.999853) (xy 303.586426 51.126354)))
    (arrow1b (pts (xy 303 49.999853) (xy 302.413585 51.12636)))
    (arrow2a (pts (xy 303.000508 149.999853) (xy 303.586923 148.873346)))
    (arrow2b (pts (xy 303.000508 149.999853) (xy 302.414082 148.873352)))
  )
  (dimension 224.1 (width 0.3) (layer Dwgs.User)
    (gr_text "224,100 мм" (at 162.05 183.1) (layer Dwgs.User))
    (feature1 (pts (xy 50 150) (xy 50 181.586421)))
    (feature2 (pts (xy 274.1 150) (xy 274.1 181.586421)))
    (crossbar (pts (xy 274.1 181) (xy 50 181)))
    (arrow1a (pts (xy 50 181) (xy 51.126504 180.413579)))
    (arrow1b (pts (xy 50 181) (xy 51.126504 181.586421)))
    (arrow2a (pts (xy 274.1 181) (xy 272.973496 180.413579)))
    (arrow2b (pts (xy 274.1 181) (xy 272.973496 181.586421)))
  )
  (dimension 46 (width 0.3) (layer Dwgs.User)
    (gr_text "46,000 мм" (at 294 73 90) (layer Dwgs.User))
    (feature1 (pts (xy 274 50) (xy 292.486421 50)))
    (feature2 (pts (xy 274 96) (xy 292.486421 96)))
    (crossbar (pts (xy 291.9 96) (xy 291.9 50)))
    (arrow1a (pts (xy 291.9 50) (xy 292.486421 51.126504)))
    (arrow1b (pts (xy 291.9 50) (xy 291.313579 51.126504)))
    (arrow2a (pts (xy 291.9 96) (xy 292.486421 94.873496)))
    (arrow2b (pts (xy 291.9 96) (xy 291.313579 94.873496)))
  )
  (gr_text "FIXME: check board\ndimensions!" (at 31.5 150 90) (layer Cmts.User))
  (gr_line (start 50 150) (end 50 50) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 274.1 150) (end 50 150) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 274.1 50) (end 274.1 150) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50 50) (end 274.1 50) (layer Edge.Cuts) (width 0.1))
  (zone (net 18) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.128)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 50 50) (xy 274.1 50) (xy 274.1 150) (xy 50 150)
      )
    )
  )
  (zone (net 18) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.128)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 50 50) (xy 274.1 50) (xy 274.1 150) (xy 50 150)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F.Cu In1.Cu In2.Cu B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 274.1 52.5) (xy 50 52.5) (xy 50 50) (xy 274.1 50)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F.Cu In1.Cu In2.Cu B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 274.1 150) (xy 274.1 148.25) (xy 50 148.25) (xy 50 150)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.499999 96.750002) (xy 124.500002 96.749999) (xy 124.499999 94.750001) (xy 122.500001 94.749999)
      )
    )
  )
  (zone (net 18) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 274.1 150) (xy 50 150) (xy 50 50) (xy 274.1 50)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.5 96.750001) (xy 106.500003 96.749998) (xy 106.5 94.75) (xy 104.500002 94.749998)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.75 96.250001) (xy 140.750003 96.249998) (xy 140.75 94.25) (xy 138.750002 94.249998)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.999997 96.000001) (xy 163 95.999998) (xy 162.999997 94) (xy 160.999999 93.999998)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 180 96.000001) (xy 182.000003 95.999998) (xy 182 94) (xy 180.000002 93.999998)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 169 96.000001) (xy 171.000003 95.999998) (xy 171 94) (xy 169.000002 93.999998)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 188 96.000001) (xy 190.000003 95.999998) (xy 190 94) (xy 188.000002 93.999998)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 199 96.000001) (xy 201.000003 95.999998) (xy 201 94) (xy 199.000002 93.999998)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 207 96.000001) (xy 209.000003 95.999998) (xy 209 94) (xy 207.000002 93.999998)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 225.999997 96.000001) (xy 228 95.999998) (xy 227.999997 94) (xy 225.999999 93.999998)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.5 106.25) (xy 106.500003 106.249997) (xy 106.5 104.249999) (xy 104.500002 104.249997)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.5 106.25) (xy 124.500003 106.249997) (xy 124.5 104.249999) (xy 122.500002 104.249997)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 138.749997 106.749991) (xy 140.75 106.749988) (xy 140.749997 104.74999) (xy 138.749999 104.749988)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.999999 104.399998) (xy 106.000002 104.400001) (xy 105.999999 106.399999) (xy 104.000001 106.400001)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 188 104.999999) (xy 190.000003 105.000002) (xy 190 107) (xy 188.000002 107.000002)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.999998 105.012057) (xy 163.000001 105.01206) (xy 162.999998 107.012058) (xy 161 107.01206)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 180 104.999999) (xy 182.000003 105.000002) (xy 182 107) (xy 180.000002 107.000002)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 206.999998 104.999997) (xy 209.000001 105) (xy 208.999998 106.999998) (xy 207 107)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 169 104.999999) (xy 171.000003 105.000002) (xy 171 107) (xy 169.000002 107.000002)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 225.999997 107.000001) (xy 228 106.999998) (xy 227.999997 105) (xy 225.999999 104.999998)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 198.999998 104.999997) (xy 201.000001 105) (xy 200.999998 106.999998) (xy 199 107)
      )
    )
  )
  (zone (net 199) (net_name V+) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.128)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149 134) (xy 149 147.25) (xy 151.5 147.25) (xy 151.5 134)
      )
    )
  )
  (zone (net 199) (net_name V+) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.128)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148.75 60) (xy 148.75 73.25) (xy 151.25 73.25) (xy 151.25 60)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 212.249999 131.249999) (xy 214.250002 131.250002) (xy 214.249999 133.25) (xy 212.250001 133.250002)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 212.249999 61.499998) (xy 214.250002 61.500001) (xy 214.249999 63.499999) (xy 212.250001 63.500001)
      )
    )
  )
)
