(kicad_pcb (version 20171130) (host pcbnew 5.0.2+dfsg1-1)
  (general
    (thickness 1.6)
    (drawings 41)
    (tracks 204)
    (zones 0)
    (modules 34)
    (nets 67)
  )
  (page A4)
  (title_block
    (title "Программатор ICSP и UART")
    (date 2020-03-05)
    (company -)
    (comment 2 "Уланов П.Н.")
    (comment 3 -)
    (comment 4 -)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.1 1.8)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 +3V3)
  (net 4 /SCK)
  (net 5 /MISO)
  (net 6 /MOSI)
  (net 7 /SS)
  (net 8 /RESET)
  (net 9 +3.3VA)
  (net 10 "Net-(C2-Pad2)")
  (net 11 "Net-(C4-Pad2)")
  (net 12 "Net-(C5-Pad2)")
  (net 13 "Net-(C6-Pad2)")
  (net 14 /RST)
  (net 15 /RxDc)
  (net 16 /TxDc)
  (net 17 /RxD)
  (net 18 /TxD)
  (net 19 "Net-(DD1-Pad5)")
  (net 20 "Net-(DD1-Pad6)")
  (net 21 "Net-(DD1-Pad9)")
  (net 22 "Net-(DD1-Pad10)")
  (net 23 "Net-(DD1-Pad11)")
  (net 24 "Net-(DD1-Pad12)")
  (net 25 "Net-(DD1-Pad13)")
  (net 26 "Net-(DD1-Pad14)")
  (net 27 "Net-(DD1-Pad15)")
  (net 28 "Net-(DD2-Pad1)")
  (net 29 "Net-(DD2-Pad2)")
  (net 30 "Net-(DD2-Pad9)")
  (net 31 "Net-(DD2-Pad10)")
  (net 32 "Net-(DD2-Pad11)")
  (net 33 "Net-(DD2-Pad12)")
  (net 34 "Net-(DD2-Pad13)")
  (net 35 "Net-(DD2-Pad14)")
  (net 36 "Net-(DD2-Pad15)")
  (net 37 "Net-(DD2-Pad16)")
  (net 38 "Net-(DD2-Pad17)")
  (net 39 "Net-(DD2-Pad18)")
  (net 40 "Net-(DD2-Pad19)")
  (net 41 "Net-(DD2-Pad20)")
  (net 42 "Net-(DD2-Pad22)")
  (net 43 "Net-(DD2-Pad23)")
  (net 44 "Net-(DD2-Pad24)")
  (net 45 "Net-(DD2-Pad25)")
  (net 46 "Net-(DD2-Pad26)")
  (net 47 "Net-(DD2-Pad27)")
  (net 48 "Net-(DD2-Pad28)")
  (net 49 "Net-(DD2-Pad32)")
  (net 50 "Net-(R1-Pad1)")
  (net 51 "Net-(R2-Pad1)")
  (net 52 "Net-(R9-Pad2)")
  (net 53 "Net-(R11-Pad1)")
  (net 54 "Net-(R12-Pad1)")
  (net 55 "Net-(RN1-Pad1)")
  (net 56 "Net-(RN1-Pad2)")
  (net 57 "Net-(RN1-Pad3)")
  (net 58 "Net-(RN1-Pad4)")
  (net 59 "Net-(RN2-Pad4)")
  (net 60 "Net-(RN2-Pad3)")
  (net 61 "Net-(RN2-Pad2)")
  (net 62 "Net-(RN2-Pad1)")
  (net 63 "Net-(XS1-Pad4)")
  (net 64 "Net-(RN2-Pad6)")
  (net 65 "Net-(RN2-Pad5)")
  (net 66 "Net-(R3-Pad2)")
  (net_class Default "Это класс цепей по умолчанию."
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3.3VA)
    (add_net +3V3)
    (add_net +5V)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RESET)
    (add_net /RST)
    (add_net /RxD)
    (add_net /RxDc)
    (add_net /SCK)
    (add_net /SS)
    (add_net /TxD)
    (add_net /TxDc)
    (add_net GND)
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(DD1-Pad10)")
    (add_net "Net-(DD1-Pad11)")
    (add_net "Net-(DD1-Pad12)")
    (add_net "Net-(DD1-Pad13)")
    (add_net "Net-(DD1-Pad14)")
    (add_net "Net-(DD1-Pad15)")
    (add_net "Net-(DD1-Pad5)")
    (add_net "Net-(DD1-Pad6)")
    (add_net "Net-(DD1-Pad9)")
    (add_net "Net-(DD2-Pad1)")
    (add_net "Net-(DD2-Pad10)")
    (add_net "Net-(DD2-Pad11)")
    (add_net "Net-(DD2-Pad12)")
    (add_net "Net-(DD2-Pad13)")
    (add_net "Net-(DD2-Pad14)")
    (add_net "Net-(DD2-Pad15)")
    (add_net "Net-(DD2-Pad16)")
    (add_net "Net-(DD2-Pad17)")
    (add_net "Net-(DD2-Pad18)")
    (add_net "Net-(DD2-Pad19)")
    (add_net "Net-(DD2-Pad2)")
    (add_net "Net-(DD2-Pad20)")
    (add_net "Net-(DD2-Pad22)")
    (add_net "Net-(DD2-Pad23)")
    (add_net "Net-(DD2-Pad24)")
    (add_net "Net-(DD2-Pad25)")
    (add_net "Net-(DD2-Pad26)")
    (add_net "Net-(DD2-Pad27)")
    (add_net "Net-(DD2-Pad28)")
    (add_net "Net-(DD2-Pad32)")
    (add_net "Net-(DD2-Pad9)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(RN1-Pad1)")
    (add_net "Net-(RN1-Pad2)")
    (add_net "Net-(RN1-Pad3)")
    (add_net "Net-(RN1-Pad4)")
    (add_net "Net-(RN2-Pad1)")
    (add_net "Net-(RN2-Pad2)")
    (add_net "Net-(RN2-Pad3)")
    (add_net "Net-(RN2-Pad4)")
    (add_net "Net-(RN2-Pad5)")
    (add_net "Net-(RN2-Pad6)")
    (add_net "Net-(XS1-Pad4)")
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 51 147.25 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 3 0 180) (layer F.SilkS))
    (fp_text value 0.33u (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 98.5 148.5 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 1.75 180) (layer F.SilkS))
    (fp_text value 12p (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C2-Pad2)"))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 58 147.25 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 3 0 180) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 87.75 151.000001 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 12p (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 57 137.5 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at -1.25 1.25 90) (layer F.SilkS))
    (fp_text value 22p (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C5-Pad2)"))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 65.25 138.25 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at -1.25 1.5 90) (layer F.SilkS))
    (fp_text value 22p (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C6-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 72 149.75)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 1.5 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-B_EIA-3528-21_Hand (layer F.Cu) (tedit 58CC8C08)
    (at 71.75 144.5 90)
    (descr "Tantalum capacitor, Case B, EIA 3528-21, 3.5x2.8x1.9mm, Hand soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C8 (at 0 2.5 90) (layer F.SilkS))
    (fp_text value 22u (at 0 3.15 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.15 0 90) (size 3.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 2.15 0 90) (size 3.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-B_EIA-3528-21.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-89-3_Handsoldering (layer F.Cu) (tedit 58CE4E7F)
    (at 54.5 148.23 270)
    (descr "SOT-89-3 Handsoldering")
    (tags "SOT-89-3 Handsoldering")
    (attr smd)
    (fp_text reference DA1 (at 3 1.75 270) (layer F.SilkS))
    (fp_text value L78L33_SOT89 (at 0.5 3.15 270) (layer F.Fab))
    (fp_text user %R (at 0.38 0) (layer F.Fab))
    (pad 1 smd rect (at -1.98 -1.5 180) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at -1.98 0 180) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.98 1.5 180) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.98 0 180) (size 2 4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd trapezoid (at -0.37 0) (size 1.5 0.75) (rect_delta 0 0.5 ) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-89-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-16_3.9x9.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64)
    (at 64.5 144.5 270)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference DD1 (at -0.5 -3.5 180) (layer F.SilkS))
    (fp_text value CH340G (at 0 6 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.7 -3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 /TxD))
    (pad 3 smd rect (at -2.7 -1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /RxD))
    (pad 4 smd rect (at -2.7 -0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 5 smd rect (at -2.7 0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(DD1-Pad5)"))
    (pad 6 smd rect (at -2.7 1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(DD1-Pad6)"))
    (pad 7 smd rect (at -2.7 3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C6-Pad2)"))
    (pad 8 smd rect (at -2.7 4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C5-Pad2)"))
    (pad 9 smd rect (at 2.7 4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(DD1-Pad9)"))
    (pad 10 smd rect (at 2.7 3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(DD1-Pad10)"))
    (pad 11 smd rect (at 2.7 1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(DD1-Pad11)"))
    (pad 12 smd rect (at 2.7 0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(DD1-Pad12)"))
    (pad 13 smd rect (at 2.7 -0.635 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(DD1-Pad13)"))
    (pad 14 smd rect (at 2.7 -1.905 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(DD1-Pad14)"))
    (pad 15 smd rect (at 2.7 -3.175 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(DD1-Pad15)"))
    (pad 16 smd rect (at 2.7 -4.445 270) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-16_3.9x9.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 58CC9A48)
    (at 93.75 142 90)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference DD2 (at 0 -0.25) (layer F.SilkS))
    (fp_text value ATmega328P-AU (at 0 6.05 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -4.25 -2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(DD2-Pad1)"))
    (pad 2 smd rect (at -4.25 -2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(DD2-Pad2)"))
    (pad 3 smd rect (at -4.25 -1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -4.25 -0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 +3.3VA))
    (pad 5 smd rect (at -4.25 0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -4.25 1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 +3.3VA))
    (pad 7 smd rect (at -4.25 2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C4-Pad2)"))
    (pad 8 smd rect (at -4.25 2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C2-Pad2)"))
    (pad 9 smd rect (at -2.8 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(DD2-Pad9)"))
    (pad 10 smd rect (at -2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(DD2-Pad10)"))
    (pad 11 smd rect (at -1.2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(DD2-Pad11)"))
    (pad 12 smd rect (at -0.4 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(DD2-Pad12)"))
    (pad 13 smd rect (at 0.4 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(DD2-Pad13)"))
    (pad 14 smd rect (at 1.2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(DD2-Pad14)"))
    (pad 15 smd rect (at 2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(DD2-Pad15)"))
    (pad 16 smd rect (at 2.8 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(DD2-Pad16)"))
    (pad 17 smd rect (at 4.25 2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(DD2-Pad17)"))
    (pad 18 smd rect (at 4.25 2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(DD2-Pad18)"))
    (pad 19 smd rect (at 4.25 1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(DD2-Pad19)"))
    (pad 20 smd rect (at 4.25 0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(DD2-Pad20)"))
    (pad 21 smd rect (at 4.25 -0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 22 smd rect (at 4.25 -1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(DD2-Pad22)"))
    (pad 23 smd rect (at 4.25 -2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(DD2-Pad23)"))
    (pad 24 smd rect (at 4.25 -2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(DD2-Pad24)"))
    (pad 25 smd rect (at 2.8 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(DD2-Pad25)"))
    (pad 26 smd rect (at 2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(DD2-Pad26)"))
    (pad 27 smd rect (at 1.2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(DD2-Pad27)"))
    (pad 28 smd rect (at 0.4 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(DD2-Pad28)"))
    (pad 29 smd rect (at -0.4 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 /RESET))
    (pad 30 smd rect (at -1.2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 /RxDc))
    (pad 31 smd rect (at -2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 /TxDc))
    (pad 32 smd rect (at -2.8 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(DD2-Pad32)"))
    (model ${KISYS3DMOD}/Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_HC49-U_Vertical (layer F.Cu) (tedit 5E60C4CF)
    (at 97.25 152.25 180)
    (descr "Crystal THT HC-49/U http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49/U")
    (fp_text reference ZQ1 (at 2.44 -3.525 180) (layer F.SilkS))
    (fp_text value 7.37M (at 2.44 3.525 180) (layer F.Fab))
    (fp_text user %R (at 2.44 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C2-Pad2)"))
    (pad 2 thru_hole circle (at 4.88 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_HC49-U_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_SMD_3225-4pin_3.2x2.5mm_HandSoldering (layer F.Cu) (tedit 5E60B823)
    (at 61.000001 138)
    (descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, hand-soldering, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal hand-soldering")
    (attr smd)
    (fp_text reference ZQ2 (at -4.000001 2.5) (layer F.SilkS))
    (fp_text value 12M (at 0 3.05) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.45 1.15) (size 2.1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C5-Pad2)"))
    (pad 2 smd rect (at 1.45 1.15) (size 2.1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.45 -1.15) (size 2.1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C6-Pad2)"))
    (pad 4 smd rect (at -1.45 -1.15) (size 2.1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_SMD_3225-4pin_3.2x2.5mm_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_B3S-1000 (layer F.Cu) (tedit 5E63619E)
    (at 104.5 151.75 270)
    (descr "Surface Mount Tactile Switch for High-Density Packaging")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SB1 (at -0.25 -0.25 180) (layer F.SilkS))
    (fp_text value SW_Push (at 0 4.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -4.5 270) (layer F.Fab))
    (pad 1 smd rect (at -3.975 -2.25 270) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 3.975 -2.25 270) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -3.975 2.25 270) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(R3-Pad2)"))
    (pad 2 smd rect (at 3.975 2.25 270) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_B3S-1000.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 68.5 137.25 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 1.5 180) (layer F.SilkS))
    (fp_text value 1K (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /RxD))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 69.75 139.25 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -2 1.5 180) (layer F.SilkS))
    (fp_text value 1K (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /TxD))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 82 154.25 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 1.5 270) (layer F.SilkS))
    (fp_text value 1K (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /RST))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 87.5 138 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 2.25 1.75) (layer F.SilkS))
    (fp_text value 1K (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /RESET))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 102.75 145.5 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at -3.25 0 180) (layer F.SilkS))
    (fp_text value 47 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(DD2-Pad14)"))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 /SS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 83.947 154.25 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0.25 1.803 90) (layer F.SilkS))
    (fp_text value 100K (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 +3.3VA))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 102.75 143.5 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at -3.25 0 180) (layer F.SilkS))
    (fp_text value 47 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 /MOSI))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(DD2-Pad15)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 102.75 141.5 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at -3.25 0 180) (layer F.SilkS))
    (fp_text value 1K (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(DD2-Pad16)"))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 /MISO))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 113.25 155)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at -3.25 0.25) (layer F.SilkS))
    (fp_text value 1K (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(R9-Pad2)"))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 102.75 139.5 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 3.25 1.25 180) (layer F.SilkS))
    (fp_text value 47 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 /SCK))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(DD2-Pad17)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 102.75 137 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 3.5 0 180) (layer F.SilkS))
    (fp_text value 660 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(DD2-Pad23)"))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(R11-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 111.75 136.75)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at 3.75 -1) (layer F.SilkS))
    (fp_text value 660 (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(R12-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 /SS))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 595FC9C0)
    (at 107.25 137 180)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference VD1 (at -3.25 -1.5 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(R11-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 595FC9C0)
    (at 107.25 138.5)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference VD2 (at 0 -2.75) (layer F.SilkS))
    (fp_text value LED (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(R12-Pad1)"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Connectors:USB_Micro-B (layer F.Cu) (tedit 5E60B755)
    (at 52.5 140 270)
    (descr "Micro USB Type B Receptacle")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference XS1 (at 0 0.75 270) (layer F.SilkS))
    (fp_text value USB_B_Micro (at 0 5.01 270) (layer F.Fab))
    (pad 1 smd rect (at -1.3 -1.35) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -0.65 -1.35) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(DD1-Pad6)"))
    (pad 3 smd rect (at 0 -1.35) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(DD1-Pad5)"))
    (pad 4 smd rect (at 0.65 -1.35) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(XS1-Pad4)"))
    (pad 5 smd rect (at 1.3 -1.35) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at -2.5 -1.35) (size 0.95 1.25) (drill oval 0.55 0.85) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 2.5 -1.35) (size 0.95 1.25) (drill oval 0.55 0.85) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at -3.5 1.35) (size 1.55 1) (drill oval 1.15 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 3.5 1.35) (size 1.55 1) (drill oval 1.15 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x07_Pitch2.54mm (layer B.Cu) (tedit 5E60B760)
    (at 74.37 154.5 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference XP1 (at -0.25 3 180) (layer B.SilkS))
    (fp_text value Conn_01x07 (at 0 -17.57 90) (layer B.Fab))
    (fp_text user %R (at 0 -7.62) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(RN2-Pad2)"))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(RN2-Pad1)"))
    (pad 4 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(RN1-Pad4)"))
    (pad 5 thru_hole oval (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(RN1-Pad3)"))
    (pad 6 thru_hole oval (at 0 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(RN1-Pad2)"))
    (pad 7 thru_hole oval (at 0 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(RN1-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x06_Pitch2.54mm (layer B.Cu) (tedit 5E60B73D)
    (at 79 150)
    (descr "Through hole straight pin header, 2x06, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x06 2.54mm double row")
    (fp_text reference XP2 (at 2 2.33) (layer B.SilkS))
    (fp_text value Conn_02x04_Counter_Clockwise (at 1.27 -15.03) (layer B.Fab))
    (fp_text user %R (at 1.27 -6.35 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(RN1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /RST))
    (pad 3 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 4 thru_hole oval (at 2.54 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 +3.3VA))
    (pad 5 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 6 thru_hole oval (at 2.54 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 +3.3VA))
    (pad 7 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(R2-Pad1)"))
    (pad 8 thru_hole oval (at 2.54 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /RxDc))
    (pad 9 thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(R1-Pad1)"))
    (pad 10 thru_hole oval (at 2.54 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /TxDc))
    (pad 11 thru_hole oval (at 0 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 12 thru_hole oval (at 2.54 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x06_Pitch2.54mm (layer B.Cu) (tedit 5E60B72B)
    (at 112.75 152.25)
    (descr "Through hole angled pin header, 1x06, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x06 2.54mm single row")
    (fp_text reference XP3 (at 2.5 -5 -90) (layer B.SilkS))
    (fp_text value Conn_01x04_Male (at 4.385 -14.97) (layer B.Fab))
    (fp_text user %R (at 2.77 -6.35 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(R9-Pad2)"))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /MOSI))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /MISO))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /SCK))
    (pad 5 thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /SS))
    (pad 6 thru_hole oval (at 0 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_Array_Concave_4x0603 (layer F.Cu) (tedit 58E0A85E)
    (at 62 150 90)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN1 (at -0.25 -2.25 90) (layer F.SilkS))
    (fp_text value 680 (at 0 2.6 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 5 smd rect (at 0.85 1.2 90) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(DD1-Pad12)"))
    (pad 6 smd rect (at 0.85 0.4 90) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(DD1-Pad11)"))
    (pad 7 smd rect (at 0.85 -0.4 90) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(DD1-Pad10)"))
    (pad 8 smd rect (at 0.85 -1.2 90) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(DD1-Pad9)"))
    (pad 4 smd rect (at -0.85 1.2 90) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(RN1-Pad4)"))
    (pad 1 smd rect (at -0.85 -1.2 90) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(RN1-Pad1)"))
    (pad 3 smd rect (at -0.85 0.4 90) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(RN1-Pad3)"))
    (pad 2 smd rect (at -0.85 -0.4 90) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(RN1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_Array_Concave_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_Array_Concave_4x0603 (layer F.Cu) (tedit 58E0A85E)
    (at 66.75 150 90)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA06P (see cra06p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN2 (at -0.25 -2.25 90) (layer F.SilkS))
    (fp_text value 680 (at 0 2.6 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at -0.85 -0.4 90) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(RN2-Pad2)"))
    (pad 3 smd rect (at -0.85 0.4 90) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(RN2-Pad3)"))
    (pad 1 smd rect (at -0.85 -1.2 90) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(RN2-Pad1)"))
    (pad 4 smd rect (at -0.85 1.2 90) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(RN2-Pad4)"))
    (pad 8 smd rect (at 0.85 -1.2 90) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(DD1-Pad13)"))
    (pad 7 smd rect (at 0.85 -0.4 90) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(DD1-Pad14)"))
    (pad 6 smd rect (at 0.85 0.4 90) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(RN2-Pad6)"))
    (pad 5 smd rect (at 0.85 1.2 90) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(RN2-Pad5)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_Array_Concave_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Условия распространения\nhttps://creativecommons.org/licenses/by-sa/3.0/ Attribution-ShareAlike 3.0 Unported (CC BY-SA 3.0)" (at 110.25 130) (layer Cmts.User))
  (gr_text "Программатор ICSP\nИмеет возможность прошивать как через SPI, \nтак и через последовательный порт за счет \nиспользования CH340G\nМонтаж односторонний для простоты изготовления\nПри изготовлении на двухстороннем текстолите \nнужно зенковать все отверстия на обратной стороне, \nкроме идущих на общий\nПодходит для заказа на заводе\nКонденсатор С8 танталовый - чтобы обеспечить нужную емкость\n в 22uF, при его отсутствии можно заменить двумя \nна 10uF, напаянными друг на друга, типоразмер - 1206" (at 127 150.25) (layer Cmts.User))
  (gr_text GND (at 74.25 153) (layer F.SilkS))
  (gr_text ~DSR~ (at 61.75 153) (layer F.SilkS))
  (gr_text ~RTS~ (at 71.75 153) (layer F.SilkS))
  (gr_text ~RI~ (at 64.25 153) (layer F.SilkS))
  (gr_text ~DCD~ (at 66.75 153) (layer F.SilkS))
  (gr_text ~DTR~ (at 69.25 153) (layer F.SilkS))
  (gr_text ~CTS~ (at 59 153) (layer F.SilkS))
  (gr_text ~RST~ (at 84.75 149.86) (layer F.SilkS))
  (gr_line (start 117 135) (end 50 135) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 117 157) (end 117 135) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 50 157) (end 117 157) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 50 135) (end 50 157) (layer Edge.Cuts) (width 0.2))
  (dimension 22 (width 0.3) (layer Dwgs.User)
    (gr_text "22,000 мм" (at 41.9 146 270) (layer Dwgs.User))
    (feature1 (pts (xy 50 157) (xy 43.413579 157)))
    (feature2 (pts (xy 50 135) (xy 43.413579 135)))
    (crossbar (pts (xy 44 135) (xy 44 157)))
    (arrow1a (pts (xy 44 157) (xy 43.413579 155.873496)))
    (arrow1b (pts (xy 44 157) (xy 44.586421 155.873496)))
    (arrow2a (pts (xy 44 135) (xy 43.413579 136.126504)))
    (arrow2b (pts (xy 44 135) (xy 44.586421 136.126504)))
  )
  (dimension 67 (width 0.3) (layer Dwgs.User)
    (gr_text "67,000 мм" (at 83.5 163.1) (layer Dwgs.User))
    (feature1 (pts (xy 117 157) (xy 117 161.586421)))
    (feature2 (pts (xy 50 157) (xy 50 161.586421)))
    (crossbar (pts (xy 50 161) (xy 117 161)))
    (arrow1a (pts (xy 117 161) (xy 115.873496 161.586421)))
    (arrow1b (pts (xy 117 161) (xy 115.873496 160.413579)))
    (arrow2a (pts (xy 50 161) (xy 51.126504 161.586421)))
    (arrow2b (pts (xy 50 161) (xy 51.126504 160.413579)))
  )
  (gr_text ~PRST~ (at 110 152.5) (layer F.SilkS))
  (gr_text MOSI (at 110 150) (layer F.SilkS))
  (gr_text MISO (at 110 147.25) (layer F.SilkS))
  (gr_text SCK (at 110 144.75) (layer F.SilkS))
  (gr_text ~RST~ (at 110 142) (layer F.SilkS))
  (gr_text GND (at 110 139.75) (layer F.SilkS))
  (gr_text 3.3V (at 84.25 145.5 90) (layer F.SilkS))
  (gr_text TXD (at 85.09 139.7) (layer F.SilkS))
  (gr_text RXD (at 84.963 142.24) (layer F.SilkS))
  (gr_text GND (at 85 137.16) (layer F.SilkS))
  (gr_text ~RST~ (at 75.692 149.86) (layer F.SilkS))
  (gr_text 3.3V (at 76.25 145.25 90) (layer F.SilkS))
  (gr_text TXD (at 75.692 142.24) (layer F.SilkS))
  (gr_text RXD (at 75.692 139.7) (layer F.SilkS))
  (gr_text GND (at 75.692 137.16) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.128)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50 135) (xy 50 157) (xy 117 157) (xy 117 135)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.128)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.065227 157) (xy 50.065227 135) (xy 117.065227 135) (xy 117.065227 157)
      )
    )
  )
)
