(kicad_pcb (version 20171130) (host pcbnew 5.1.9+dfsg1-1)
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 174)
    (zones 0)
    (modules 52)
    (nets 38)
  )
  (page A4)
  (title_block
    (title "Evrucky Vacuum Diode Examination Device PCB")
    (date 2022-02-11)
    (company "Ivan Shmakov")
    (comment 1 "CC BY-SA 3.0+")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.75)
    (trace_clearance 0.25)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 1.2)
    (via_drill 0.8)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 /COM)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 /FU_N)
  (net 6 /FU_L)
  (net 7 /MAINSL)
  (net 8 /MAINSN)
  (net 9 /SW_L)
  (net 10 /ANODE)
  (net 11 "Net-(R2-Pad3)")
  (net 12 "Net-(R2-Pad1)")
  (net 13 "Net-(R5-Pad1)")
  (net 14 /ATX)
  (net 15 /COIL+)
  (net 16 /50VACX)
  (net 17 /50VACY)
  (net 18 /METERACY)
  (net 19 /METERACX)
  (net 20 "Net-(R2-Pad2)")
  (net 21 /COILAMP)
  (net 22 /HEATERAC)
  (net 23 "Net-(C7-Pad2)")
  (net 24 "Net-(VD10-Pad2)")
  (net 25 /T_L)
  (net 26 /COILCOM)
  (net 27 /T_N)
  (net 28 "Net-(C4-Pad2)")
  (net 29 "Net-(C4-Pad1)")
  (net 30 "Net-(C6-Pad1)")
  (net 31 "Net-(C6-Pad2)")
  (net 32 "Net-(K1-Pad3)")
  (net 33 "Net-(R6-Pad1)")
  (net 34 "Net-(VD5-Pad2)")
  (net 35 "Net-(XP1-Pad1)")
  (net 36 "Net-(C5-Pad1)")
  (net 37 "Net-(VD9-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.25)
    (trace_width 0.75)
    (via_dia 1.2)
    (via_drill 0.8)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /50VACX)
    (add_net /50VACY)
    (add_net /ANODE)
    (add_net /COM)
    (add_net /HEATERAC)
    (add_net /METERACX)
    (add_net /METERACY)
    (add_net /T_L)
    (add_net /T_N)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(K1-Pad3)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R2-Pad3)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(VD10-Pad2)")
    (add_net "Net-(VD5-Pad2)")
    (add_net "Net-(VD9-Pad4)")
    (add_net "Net-(XP1-Pad1)")
  )
  (net_class "3 A" ""
    (clearance 0.3)
    (trace_width 2.5)
    (via_dia 1.5)
    (via_drill 1)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /ATX)
    (add_net /COIL+)
    (add_net /COILAMP)
    (add_net /COILCOM)
    (add_net /FU_L)
    (add_net /FU_N)
    (add_net /MAINSL)
    (add_net /MAINSN)
    (add_net /SW_L)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 130 125 180)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference X15 (at 4.385 -2.27) (layer F.SilkS))
    (fp_text value Conn_01x06 (at 4.385 14.97) (layer F.Fab))
    (fp_text user %R (at 2.77 6.35 90) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /COILCOM))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /COILAMP))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /COM))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /ANODE))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /COM))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D12.5mm_P5.00mm (layer B.Cu) (tedit 5AE50EF1)
    (at 225 82.5 90)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=12.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 12.5mm Electrolytic Capacitor")
    (fp_text reference C1 (at 2.5 7.5 270) (layer B.SilkS))
    (fp_text value 47 (at 2.5 -7.5 270) (layer B.Fab))
    (fp_text user %R (at 2.500001 -2.500001 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 /COM))
    (model ${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D12.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3_ISO14580 (layer F.Cu) (tedit 56D1B4CB)
    (at 250 100)
    (descr "Mounting Hole 3.2mm, no annular, M3, ISO14580")
    (tags "mounting hole 3.2mm no annular m3 iso14580")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.75) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO14580 (at 0 3.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3_ISO14580 (layer F.Cu) (tedit 56D1B4CB)
    (at 50 100)
    (descr "Mounting Hole 3.2mm, no annular, M3, ISO14580")
    (tags "mounting hole 3.2mm no annular m3 iso14580")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.75) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO14580 (at 0 3.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEF)
    (at 214.361715 80.926687 315)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 0 -1.05 135) (layer F.SilkS))
    (fp_text value 4.7 (at 0 1.05 135) (layer F.Fab))
    (fp_text user %R (at 0 -0.68 135) (layer F.Fab))
    (pad 2 smd roundrect (at 0.8625 0 315) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /COM))
    (pad 1 smd roundrect (at -0.8625 0 315) (size 1.075 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C3-Pad1)"))
    (model ${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 240 70 90)
    (descr "Through hole angled pin header, 1x06, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x06 2.54mm single row")
    (fp_text reference XP2 (at 4.385 -2.27 90) (layer F.SilkS))
    (fp_text value Conn_01x06_Male (at 4.385 7.35 90) (layer F.Fab))
    (fp_text user %R (at 2.77 2.54) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /COM))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /HEATERAC))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /METERACX))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /METERACY))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /50VACX))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /50VACY))
    (model ${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 135 65 90)
    (descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 2.54mm single row")
    (fp_text reference XP3 (at 4.385 -2.27 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 4.385 7.35 90) (layer F.Fab))
    (fp_text user %R (at 2.77 2.54) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /T_N))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /T_L))
    (model ${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5C745284)
    (at 86.959619 75.459619 315)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "net tie solder jumper bridged")
    (attr virtual)
    (fp_text reference X5 (at 0 -1.8 135) (layer F.SilkS))
    (fp_text value Jumper_2_Bridged (at 0 1.9 135) (layer F.Fab))
    (pad 2 smd custom (at 0.65 0 315) (size 1 0.5) (layers F.Cu F.Mask)
      (net 5 /FU_N) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0 315) (size 1 0.5) (layers F.Cu F.Mask)
      (net 23 "Net-(C7-Pad2)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module Capacitor_THT:C_Rect_L19.0mm_W11.0mm_P15.00mm_MKS4 (layer B.Cu) (tedit 5AE50EF0)
    (at 75 90 90)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=19*11mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 19mm width 11mm Capacitor")
    (fp_text reference C7 (at 0 1.05 90) (layer B.SilkS))
    (fp_text value 0.1 (at 0 -1.05 90) (layer B.Fab))
    (fp_text user %R (at 0 0.68 90) (layer B.Fab))
    (pad 2 thru_hole circle (at 15 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 23 "Net-(C7-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 /FU_L))
    (model ${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L19.0mm_W11.0mm_P15.00mm_MKS4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_8x10 (layer F.Cu) (tedit 5BCA39D0)
    (at 130 133.25 270)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 8.0x10mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C2 (at 0 -5.2 90) (layer F.SilkS))
    (fp_text value 330 (at 0 5.2 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -3.25 0 270) (size 3.5 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd roundrect (at 3.25 0 270) (size 3.5 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 2 /COM))
    (model ${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_8x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse:Fuseholder_Cylinder-5x20mm_Stelvio-Kontek_PTF78_Horizontal_Open (layer B.Cu) (tedit 5B7EAE13)
    (at 65 90 90)
    (descr https://www.tme.eu/en/Document/3b48dbe2b9714a62652c97b08fcd464b/PTF78.pdf)
    (tags "Fuseholder horizontal open 5x20 Stelvio-Kontek PTF/78")
    (fp_text reference FU1 (at 11.25 6 270) (layer B.SilkS))
    (fp_text value "3 A" (at 13 -6 270) (layer B.Fab))
    (fp_text user %R (at 11.25 -4 270) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 6 /FU_L))
    (pad 2 thru_hole circle (at 22.6 0 90) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 7 /MAINSL))
    (model ${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuseholder_Cylinder-5x20mm_Stelvio-Kontek_PTF78_Horizontal_Open.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse:Fuseholder_Cylinder-5x20mm_Stelvio-Kontek_PTF78_Horizontal_Open (layer B.Cu) (tedit 5B7EAE13)
    (at 85 90 90)
    (descr https://www.tme.eu/en/Document/3b48dbe2b9714a62652c97b08fcd464b/PTF78.pdf)
    (tags "Fuseholder horizontal open 5x20 Stelvio-Kontek PTF/78")
    (fp_text reference FU2 (at 11.25 6 270) (layer B.SilkS))
    (fp_text value "3 A" (at 13 -6 270) (layer B.Fab))
    (fp_text user %R (at 11.25 -4 270) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 5 /FU_N))
    (pad 2 thru_hole circle (at 22.6 0 90) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 8 /MAINSN))
    (model ${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuseholder_Cylinder-5x20mm_Stelvio-Kontek_PTF78_Horizontal_Open.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse:Fuseholder_Cylinder-5x20mm_Stelvio-Kontek_PTF78_Horizontal_Open (layer B.Cu) (tedit 5B7EAE13)
    (at 132.6 75 180)
    (descr https://www.tme.eu/en/Document/3b48dbe2b9714a62652c97b08fcd464b/PTF78.pdf)
    (tags "Fuseholder horizontal open 5x20 Stelvio-Kontek PTF/78")
    (fp_text reference FU4 (at 11.25 6) (layer B.SilkS))
    (fp_text value "0.1 A" (at 13 -6) (layer B.Fab))
    (fp_text user %R (at 11.25 -4) (layer B.Fab))
    (pad 2 thru_hole circle (at 22.6 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 9 /SW_L))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 25 /T_L))
    (model ${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuseholder_Cylinder-5x20mm_Stelvio-Kontek_PTF78_Horizontal_Open.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 211.957107 74.457107 135)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.65 135) (layer F.SilkS))
    (fp_text value "1 k" (at 0 1.65 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 135) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 10 /ANODE))
    (pad 1 smd roundrect (at -1 0 135) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 165 113.5 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value "3.9 k" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 11 "Net-(R2-Pad3)"))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 10 /ANODE))
    (model ${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 173.5 110 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 -1.65) (layer F.SilkS))
    (fp_text value "5.6 k" (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 12 "Net-(R2-Pad1)"))
    (pad 1 smd roundrect (at -1 0 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 2 /COM))
    (model ${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 234.0875 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 -1.43) (layer F.SilkS))
    (fp_text value "15 k" (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(R5-Pad1)"))
    (pad 2 smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:Diode_Bridge_Vishay_KBPC1 (layer F.Cu) (tedit 5A74AB8C)
    (at 150 79.999999)
    (descr "Single phase bridge rectifier case KBPC1, see http://www.vishay.com/docs/93585/vs-kbpc1series.pdf")
    (tags "Diode Bridge")
    (fp_text reference VD1 (at 11.6 14.9 180) (layer F.SilkS))
    (fp_text value KBPC310 (at 5.35 -4.35 180) (layer F.Fab))
    (fp_text user %R (at 5.2 5.415 180) (layer F.Fab))
    (pad 3 thru_hole circle (at 10.5 10.5) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 26 /COILCOM))
    (pad 4 thru_hole circle (at 10.5 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 14 /ATX))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 /COIL+))
    (pad 2 thru_hole circle (at 0.1 10.5) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 /FU_N))
    (model ${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/Diode_Bridge_Vishay_KBPC1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:Diode_Bridge_Vishay_DFS (layer F.Cu) (tedit 5A4F675E)
    (at 237.499999 80.000001 90)
    (descr "SMD diode bridge DFS, see http://www.vishay.com/docs/88854/padlayouts.pdf")
    (tags DFS)
    (attr smd)
    (fp_text reference VD2 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value DB207S-TR (at 0 5.2 90) (layer F.Fab))
    (fp_text user %R (at 0 -0.065 90) (layer F.Fab))
    (pad 1 smd rect (at -4.37 -2.55 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at -4.37 2.55 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 /COM))
    (pad 3 smd rect (at 4.37 2.55 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 16 /50VACX))
    (pad 4 smd rect (at 4.37 -2.55 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 17 /50VACY))
    (model ${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/Diode_Bridge_Vishay_DFS.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:Diode_Bridge_Vishay_DFS (layer F.Cu) (tedit 5A4F675E)
    (at 250 80 90)
    (descr "SMD diode bridge DFS, see http://www.vishay.com/docs/88854/padlayouts.pdf")
    (tags DFS)
    (attr smd)
    (fp_text reference VD3 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value DB207S-TR (at 0 5.2 90) (layer F.Fab))
    (fp_text user %R (at 0 -0.065 90) (layer F.Fab))
    (pad 4 smd rect (at 4.37 -2.55 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 /METERACY))
    (pad 3 smd rect (at 4.37 2.55 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 19 /METERACX))
    (pad 2 smd rect (at -4.37 2.55 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 /COM))
    (pad 1 smd rect (at -4.37 -2.55 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/Diode_Bridge_Vishay_DFS.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_MiniMELF_Handsoldering (layer F.Cu) (tedit 5905D919)
    (at 213.990485 84.09099 315)
    (descr "Diode Mini-MELF (SOD-80) Handsoldering")
    (tags "Diode Mini-MELF (SOD-80) Handsoldering")
    (attr smd)
    (fp_text reference VD4 (at 0 -1.75 135) (layer F.SilkS))
    (fp_text value "BZV55 C3V3" (at 0 1.75 135) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 135) (layer F.Fab))
    (pad 1 smd rect (at -2.75 0 315) (size 3.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 2.75 0 315) (size 3.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 /COM))
    (model ${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEF0)
    (at 230 89.125 270)
    (descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (attr smd)
    (fp_text reference VD7 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value KPH-1608SEC (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /COM))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(R5-Pad1)"))
    (model ${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_MiniMELF_Handsoldering (layer F.Cu) (tedit 5905D919)
    (at 210.278175 90.985282 45)
    (descr "Diode Mini-MELF (SOD-80) Handsoldering")
    (tags "Diode Mini-MELF (SOD-80) Handsoldering")
    (attr smd)
    (fp_text reference VD8 (at 0 -1.75 45) (layer F.SilkS))
    (fp_text value "BZV55 C15" (at 0 1.75 45) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 45) (layer F.Fab))
    (pad 1 smd rect (at -2.75 0 45) (size 3.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R2-Pad2)"))
    (pad 2 smd rect (at 2.75 0 45) (size 3.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model ${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-252-3_TabPin2 (layer F.Cu) (tedit 5A70F30B)
    (at 203.843505 84.126345 135)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference VT1 (at 0 -4.5 135) (layer F.SilkS))
    (fp_text value IRFR120NTR (at 0 4.5 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd rect (at -4.2 -2.28 135) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R2-Pad2)"))
    (pad 2 smd rect (at -4.2 0 135) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 10 /ANODE))
    (pad 3 smd rect (at -4.2 2.28 135) (size 2.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 2.1 0 135) (size 6.4 5.8) (layers F.Cu F.Mask)
      (net 10 /ANODE))
    (pad "" smd rect (at 3.775 1.525 135) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 0.425 -1.525 135) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 3.775 -1.525 135) (size 3.05 2.75) (layers F.Paste))
    (pad "" smd rect (at 0.425 1.525 135) (size 3.05 2.75) (layers F.Paste))
    (model ${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TO-252-3_TabPin2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_TopOnly (layer F.Cu) (tedit 56D1B4CB)
    (at 65 60)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference X1 (at 0 -4.2) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 7 /MAINSL))
    (pad 1 connect circle (at 0 0) (size 6.4 6.4) (layers F.Cu F.Mask)
      (net 7 /MAINSL))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_TopOnly (layer F.Cu) (tedit 56D1B4CB)
    (at 85 60)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference X2 (at 0 -4.2) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 connect circle (at 0 0) (size 6.4 6.4) (layers F.Cu F.Mask)
      (net 8 /MAINSN))
    (pad 1 thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 8 /MAINSN))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_TopOnly (layer F.Cu) (tedit 56D1B4CB)
    (at 125 60)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference X3 (at 0 -4.2) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 9 /SW_L))
    (pad 1 connect circle (at 0 0) (size 6.4 6.4) (layers F.Cu F.Mask)
      (net 9 /SW_L))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_TopOnly (layer F.Cu) (tedit 56D1B4CB)
    (at 105 60)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference X4 (at 0 -4.2) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 5 /FU_N))
    (pad 1 connect circle (at 0 0) (size 6.4 6.4) (layers F.Cu F.Mask)
      (net 5 /FU_N))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_TopOnly (layer F.Cu) (tedit 56D1B4CB)
    (at 172.5 60)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference X6 (at 0 -4.2) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 connect circle (at 0 0) (size 6.4 6.4) (layers F.Cu F.Mask)
      (net 14 /ATX))
    (pad 1 thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 14 /ATX))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_TopOnly (layer F.Cu) (tedit 56D1B4CB)
    (at 152.5 60)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference X12 (at 0 -4.2) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 15 /COIL+))
    (pad 1 connect circle (at 0 0) (size 6.4 6.4) (layers F.Cu F.Mask)
      (net 15 /COIL+))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_TopOnly (layer F.Cu) (tedit 56D1B4CB)
    (at 125 85)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference X13 (at 0 -4.2) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 connect circle (at 0 0) (size 6.4 6.4) (layers F.Cu F.Mask)
      (net 21 /COILAMP))
    (pad 1 thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 21 /COILAMP))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_TopOnly (layer F.Cu) (tedit 56D1B4CB)
    (at 192.5 60)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference X14 (at 0 -4.2) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 connect circle (at 0 0) (size 6.4 6.4) (layers F.Cu F.Mask)
      (net 26 /COILCOM))
    (pad 1 thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 26 /COILCOM))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 227.42 70 90)
    (descr "Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x03 2.54mm single row")
    (fp_text reference XP1 (at 4.385 -2.27 90) (layer F.SilkS))
    (fp_text value Conn_01x03_Male (at 4.385 7.35 90) (layer F.Fab))
    (fp_text user %R (at 2.77 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(XP1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /COM))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /HEATERAC))
    (model ${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5C745284)
    (at 210.65 60)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "net tie solder jumper bridged")
    (attr virtual)
    (fp_text reference X7 (at 0 -1.8) (layer F.SilkS))
    (fp_text value Jumper_2_Bridged (at 0 1.9) (layer F.Fab))
    (pad 2 smd custom (at 0.65 0) (size 1 0.5) (layers F.Cu F.Mask)
      (net 2 /COM) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0) (size 1 0.5) (layers F.Cu F.Mask)
      (net 26 /COILCOM) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5C745284)
    (at 140.85 59.35 180)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "net tie solder jumper bridged")
    (attr virtual)
    (fp_text reference X8 (at 0 -1.8) (layer F.SilkS))
    (fp_text value Jumper_2_Bridged (at 0 1.9) (layer F.Fab))
    (pad 1 smd custom (at -0.65 0 180) (size 1 0.5) (layers F.Cu F.Mask)
      (net 5 /FU_N) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0 180) (size 1 0.5) (layers F.Cu F.Mask)
      (net 27 /T_N) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 170 114.92)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference R2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value "20 k" (at 0 12.49) (layer F.Fab))
    (fp_text user %R (at 0 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(R2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(R2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(R2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_8x10 (layer F.Cu) (tedit 5BCA39D0)
    (at 65.201903 117.298097 225)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 8.0x10mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C6 (at 0 -5.2 45) (layer F.SilkS))
    (fp_text value 330 (at 0 5.2 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 1 smd roundrect (at -3.25 0 225) (size 3.5 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 30 "Net-(C6-Pad1)"))
    (pad 2 smd roundrect (at 3.25 0 225) (size 3.5 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 31 "Net-(C6-Pad2)"))
    (model ${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_8x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module movsudi-2022:NRP05-C (layer B.Cu) (tedit 61FCE0A2)
    (at 97.5 115)
    (fp_text reference K1 (at 0 -1.27) (layer B.SilkS))
    (fp_text value NRP05-C (at 0 0.5) (layer B.Fab))
    (pad 1 thru_hole circle (at -7.62 -3.8) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask)
      (net 30 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at -7.62 3.8) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask)
      (net 31 "Net-(C6-Pad2)"))
    (pad 3 thru_hole circle (at 3.58 -3.8) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask)
      (net 32 "Net-(K1-Pad3)"))
    (pad 4 thru_hole circle (at 5.08 3.8) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 /FU_L))
    (pad 5 thru_hole circle (at 7.62 -3.8) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask)
      (net 9 /SW_L))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 85 112.5 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 30 "Net-(C6-Pad1)"))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 33 "Net-(R6-Pad1)"))
    (model ${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 57.792893 124.207107 225)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 0 -1.65 45) (layer F.SilkS))
    (fp_text value "560 k" (at 0 1.65 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 1 smd roundrect (at -1 0 225) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 28 "Net-(C4-Pad2)"))
    (pad 2 smd roundrect (at 1 0 225) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333)
      (net 36 "Net-(C5-Pad1)"))
    (model ${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_Push_1P1T_NO_6x6mm_H9.5mm (layer F.Cu) (tedit 5CA1CA7F)
    (at 50 127.25 180)
    (descr "tactile push button, 6x6mm e.g. PTS645xx series, height=9.5mm")
    (tags "tact sw push 6mm smd")
    (attr smd)
    (fp_text reference SB1 (at 0 -4.05) (layer F.SilkS))
    (fp_text value SW_Push (at 0 4.15) (layer F.Fab))
    (fp_text user %R (at 0 -4.05) (layer F.Fab))
    (pad 2 smd rect (at -3.975 2.25 180) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C5-Pad1)"))
    (pad 1 smd rect (at -3.975 -2.25 180) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C4-Pad1)"))
    (pad 1 smd rect (at 3.975 -2.25 180) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 3.975 2.25 180) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(C5-Pad1)"))
    (model ${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_PUSH_6mm_H9.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_Push_1P1T_NO_6x6mm_H9.5mm (layer F.Cu) (tedit 5CA1CA7F)
    (at 80.59826 121.219759 225)
    (descr "tactile push button, 6x6mm e.g. PTS645xx series, height=9.5mm")
    (tags "tact sw push 6mm smd")
    (attr smd)
    (fp_text reference SB2 (at 0 -4.05 45) (layer F.SilkS))
    (fp_text value SW_Push (at 0 4.15 45) (layer F.Fab))
    (fp_text user %R (at 0 -4.05 45) (layer F.Fab))
    (pad 2 smd rect (at 3.975 2.25 225) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R6-Pad1)"))
    (pad 1 smd rect (at 3.975 -2.25 225) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C6-Pad2)"))
    (pad 1 smd rect (at -3.975 -2.25 225) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C6-Pad2)"))
    (pad 2 smd rect (at -3.975 2.25 225) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R6-Pad1)"))
    (model ${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_PUSH_6mm_H9.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEF0)
    (at 70 75.875 270)
    (descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (attr smd)
    (fp_text reference VD5 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value KPH-1608SEC (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(C7-Pad2)"))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(VD5-Pad2)"))
    (model ${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_MiniMELF_Handsoldering (layer F.Cu) (tedit 5905D919)
    (at 80 77.75 90)
    (descr "Diode Mini-MELF (SOD-80) Handsoldering")
    (tags "Diode Mini-MELF (SOD-80) Handsoldering")
    (attr smd)
    (fp_text reference VD6 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value "BZV55 C2V7" (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -2.75 0 90) (size 3.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(VD5-Pad2)"))
    (pad 2 smd rect (at 2.75 0 90) (size 3.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C7-Pad2)"))
    (model ${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:Diode_Bridge_Vishay_DFS (layer F.Cu) (tedit 5A4F675E)
    (at 97.5 127.5 315)
    (descr "SMD diode bridge DFS, see http://www.vishay.com/docs/88854/padlayouts.pdf")
    (tags DFS)
    (attr smd)
    (fp_text reference VD9 (at 0 -5.1 135) (layer F.SilkS))
    (fp_text value DB207S-TR (at 0 5.2 135) (layer F.Fab))
    (fp_text user %R (at 0 -0.065 135) (layer F.Fab))
    (pad 1 smd rect (at -4.37 -2.55 315) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at -4.37 2.55 315) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C6-Pad2)"))
    (pad 3 smd rect (at 4.37 2.55 315) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C4-Pad2)"))
    (pad 4 smd rect (at 4.37 -2.55 315) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(VD9-Pad4)"))
    (model ${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/Diode_Bridge_Vishay_DFS.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_MiniMELF_Handsoldering (layer F.Cu) (tedit 5905D919)
    (at 78.055456 113.444544 225)
    (descr "Diode Mini-MELF (SOD-80) Handsoldering")
    (tags "Diode Mini-MELF (SOD-80) Handsoldering")
    (attr smd)
    (fp_text reference VD10 (at 0 -1.75 45) (layer F.SilkS))
    (fp_text value "BZV55 C5V1" (at 0 1.75 45) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 45) (layer F.Fab))
    (pad 2 smd rect (at 2.75 0 225) (size 3.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(VD10-Pad2)"))
    (pad 1 smd rect (at -2.75 0 225) (size 3.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(C6-Pad1)"))
    (model ${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_MiniMELF_Handsoldering (layer F.Cu) (tedit 5905D919)
    (at 71.055456 120.444544 225)
    (descr "Diode Mini-MELF (SOD-80) Handsoldering")
    (tags "Diode Mini-MELF (SOD-80) Handsoldering")
    (attr smd)
    (fp_text reference VD11 (at 0 -1.75 45) (layer F.SilkS))
    (fp_text value "BZV55 C5V1" (at 0 1.75 45) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 45) (layer F.Fab))
    (pad 1 smd rect (at -2.75 0 225) (size 3.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(VD10-Pad2)"))
    (pad 2 smd rect (at 2.75 0 225) (size 3.3 1.7) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C6-Pad2)"))
    (model ${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 217.5 70 90)
    (descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 2.54mm single row")
    (fp_text reference XP4 (at 4.385 -2.27 90) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 4.385 4.81 90) (layer F.Fab))
    (fp_text user %R (at 2.77 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /ANODE))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(XP1-Pad1)"))
    (model ${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse:Fuseholder_Cylinder-5x20mm_Stelvio-Kontek_PTF78_Horizontal_Open (layer B.Cu) (tedit 5B7EAE13)
    (at 45 90 90)
    (descr https://www.tme.eu/en/Document/3b48dbe2b9714a62652c97b08fcd464b/PTF78.pdf)
    (tags "Fuseholder horizontal open 5x20 Stelvio-Kontek PTF/78")
    (fp_text reference FU3 (at 11.25 6 270) (layer B.SilkS))
    (fp_text value "0.1 A" (at 13 -6 270) (layer B.Fab))
    (fp_text user %R (at 11.25 -4 270) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 36 "Net-(C5-Pad1)"))
    (pad 2 thru_hole circle (at 22.6 0 90) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 6 /FU_L))
    (model ${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuseholder_Cylinder-5x20mm_Stelvio-Kontek_PTF78_Horizontal_Open.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5C745284)
    (at 92.5 75 135)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "net tie solder jumper bridged")
    (attr virtual)
    (fp_text reference X9 (at 0 -1.8 135) (layer F.SilkS))
    (fp_text value Jumper_2_Bridged (at 0 1.9 135) (layer F.Fab))
    (pad 2 smd custom (at 0.65 0 135) (size 1 0.5) (layers F.Cu F.Mask)
      (net 5 /FU_N) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0 135) (size 1 0.5) (layers F.Cu F.Mask)
      (net 37 "Net-(VD9-Pad4)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module Capacitor_THT:C_Rect_L26.5mm_W8.5mm_P22.50mm_MKS4 (layer B.Cu) (tedit 5AE50EF0)
    (at 45 135)
    (descr "C, Rect series, Radial, pin pitch=22.50mm, , length*width=26.5*8.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf")
    (tags "C Rect series Radial pin pitch 22.50mm  length 26.5mm width 8.5mm Capacitor")
    (fp_text reference C4 (at 11.25 5.5) (layer B.SilkS))
    (fp_text value 0.33 (at 11.25 -5.5) (layer B.Fab))
    (fp_text user %R (at 11.25 0) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 29 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 22.5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 28 "Net-(C4-Pad2)"))
    (model ${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L26.5mm_W8.5mm_P22.50mm_MKS4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L13.0mm_W8.0mm_P10.00mm_FKS3_FKP3_MKS4 (layer B.Cu) (tedit 5AE50EF0)
    (at 45 120)
    (descr "C, Rect series, Radial, pin pitch=10.00mm, , length*width=13*8mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf, http://www.wima.com/EN/WIMA_MKS_4.pdf")
    (tags "C Rect series Radial pin pitch 10.00mm  length 13mm width 8mm Capacitor")
    (fp_text reference C5 (at 5 5.25) (layer B.SilkS))
    (fp_text value 0.047 (at 5 -5.25) (layer B.Fab))
    (fp_text user %R (at 5 0) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(C5-Pad1)"))
    (pad 2 thru_hole circle (at 10 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(C4-Pad2)"))
    (model ${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L13.0mm_W8.0mm_P10.00mm_FKS3_FKP3_MKS4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "FIXME: footprint?" (at 135 112.5 90) (layer Cmts.User))
  (gr_text "FIXME: footprint?" (at 177.5 122.5 45) (layer Cmts.User))
  (gr_line (start 215 120) (end 185 150) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 255 120) (end 215 120) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 265 110) (end 255 120) (layer Edge.Cuts) (width 0.05))
  (dimension 240 (width 0.15) (layer Dwgs.User)
    (gr_text "240,000 mm" (at 145 38.7) (layer Dwgs.User))
    (feature1 (pts (xy 265 50) (xy 265 39.413579)))
    (feature2 (pts (xy 25 50) (xy 25 39.413579)))
    (crossbar (pts (xy 25 40) (xy 265 40)))
    (arrow1a (pts (xy 265 40) (xy 263.873496 40.586421)))
    (arrow1b (pts (xy 265 40) (xy 263.873496 39.413579)))
    (arrow2a (pts (xy 25 40) (xy 26.126504 40.586421)))
    (arrow2b (pts (xy 25 40) (xy 26.126504 39.413579)))
  )
  (gr_line (start 25 150) (end 25 50) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 185 150) (end 25 150) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 265 50) (end 265 110) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 25 50) (end 265 50) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name /COM) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 257.5 72.5) (xy 257.5 82.5) (xy 252.5 87.5) (xy 232.5 87.5) (xy 227.5 92.5)
        (xy 217.5 92.5) (xy 215 95) (xy 205 95) (xy 200 90) (xy 200 85)
        (xy 217.5 67.5) (xy 252.5 67.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160 144.973416) (xy 140 144.973416) (xy 140 99.973416) (xy 160 99.973416)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 265 106) (xy 25 106) (xy 25 93.5) (xy 265 93.5)
      )
    )
  )
  (zone (net 2) (net_name /COM) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135 140) (xy 125 140) (xy 125 122) (xy 135 122)
      )
    )
  )
)
