(kicad_pcb (version 20171130) (host pcbnew 5.1.9+dfsg1-1)
  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 37)
    (zones 0)
    (modules 19)
    (nets 11)
  )
  (page A4)
  (title_block
    (title "Gutubha Linear Shunt Regulator")
    (date 2022-02-25)
    (company "Ivan Shmakov")
    (comment 1 "CC BY-SA 3.0+")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.75)
    (trace_clearance 0.4)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 1.5)
    (via_drill 0.8)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 /COM)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(R1-Pad1)")
  (net 5 /VOUT)
  (net 6 "Net-(R3-Pad1)")
  (net 7 "Net-(R4-Pad1)")
  (net 8 "Net-(R4-Pad2)")
  (net 9 "Net-(VD2-Pad1)")
  (net 10 "Net-(VD2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.4)
    (trace_width 0.75)
    (via_dia 1.5)
    (via_drill 0.8)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /COM)
    (add_net /VOUT)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(VD2-Pad1)")
    (add_net "Net-(VD2-Pad2)")
  )
  (module Capacitor_SMD:CP_Elec_10x12.6 (layer B.Cu) (tedit 5BCA39D1)
    (at 95.5 65.25 270)
    (descr "SMD capacitor, aluminum electrolytic, Panasonic F12, 10.0x12.6mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C2 (at -6.25 4.5 180) (layer B.SilkS))
    (fp_text value 330 (at 0 -5.2 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 4.35 0 270) (size 4.4 1.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.131579)
      (net 2 /COM))
    (pad 1 smd roundrect (at -4.35 0 270) (size 4.4 1.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.131579)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_10x12.6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D12.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF1)
    (at 82.5 60 270)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=12.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 12.5mm Electrolytic Capacitor")
    (fp_text reference C1 (at -5 0 180) (layer F.SilkS))
    (fp_text value 47 (at 2.5 7.5 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 /COM))
    (model ${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D12.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer B.Cu) (tedit 5F68FEEE)
    (at 79.354765 58.145235 45)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at -1.915927 2.12132 45) (layer B.SilkS))
    (fp_text value "10 k" (at 0 -1.43 45) (layer B.Fab))
    (fp_text user %R (at 0 0 45) (layer B.Fab))
    (pad 1 smd roundrect (at -0.9125 0 45) (size 0.975 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(R1-Pad1)"))
    (pad 2 smd roundrect (at 0.9125 0 45) (size 0.975 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 122.5 65.04)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference R4 (at -3 -2.54) (layer B.SilkS))
    (fp_text value "20 k" (at 0 -7.41) (layer B.Fab))
    (fp_text user %R (at 0 -2.54 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(R4-Pad1)"))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(R4-Pad2)"))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(R3-Pad1)"))
    (model ${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer B.Cu) (tedit 5F68FEF0)
    (at 76 62.375 90)
    (descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (attr smd)
    (fp_text reference VD1 (at -0.125 -2 90) (layer B.SilkS))
    (fp_text value KPH-1608SEC (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /COM))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(R1-Pad1)"))
    (model ${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:Diode_Bridge_Vishay_DFS (layer B.Cu) (tedit 5A4F675E)
    (at 65 62.5)
    (descr "SMD diode bridge DFS, see http://www.vishay.com/docs/88854/padlayouts.pdf")
    (tags DFS)
    (attr smd)
    (fp_text reference VD2 (at 0 5.5) (layer B.SilkS))
    (fp_text value DB203S-TR (at 0 -5.2) (layer B.Fab))
    (fp_text user %R (at 0 0.065) (layer B.Fab))
    (pad 1 smd rect (at -4.37 2.55) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(VD2-Pad1)"))
    (pad 2 smd rect (at -4.37 -2.55) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(VD2-Pad2)"))
    (pad 3 smd rect (at 4.37 -2.55) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 4 smd rect (at 4.37 2.55) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 2 /COM))
    (model ${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/Diode_Bridge_Vishay_DFS.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_MiniMELF_Handsoldering (layer B.Cu) (tedit 5905D919)
    (at 102.5 62.5 90)
    (descr "Diode Mini-MELF (SOD-80) Handsoldering")
    (tags "Diode Mini-MELF (SOD-80) Handsoldering")
    (attr smd)
    (fp_text reference VD3 (at 0 1.75 90) (layer B.SilkS))
    (fp_text value "BZV55 C15" (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 2 smd rect (at 2.75 0 90) (size 3.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 1 smd rect (at -2.75 0 90) (size 3.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(R4-Pad2)"))
    (model ${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_MiniMELF_Handsoldering (layer B.Cu) (tedit 5905D919)
    (at 88.5 66.25 270)
    (descr "Diode Mini-MELF (SOD-80) Handsoldering")
    (tags "Diode Mini-MELF (SOD-80) Handsoldering")
    (attr smd)
    (fp_text reference VD4 (at 0.034675 2.061261 90) (layer B.SilkS))
    (fp_text value "BZV55 C3V3" (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -2.75 0 270) (size 3.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 2.75 0 270) (size 3.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 2 /COM))
    (model ${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:TO-252-3_TabPin2 (layer B.Cu) (tedit 5A70F30B)
    (at 110.4 62.5)
    (descr "TO-252 / DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
    (tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
    (attr smd)
    (fp_text reference VT1 (at 2.1 -5) (layer B.SilkS))
    (fp_text value IRFR120NTR (at 0 -4.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -4.2 2.28) (size 2.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(R4-Pad2)"))
    (pad 2 smd rect (at -4.2 0) (size 2.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 5 /VOUT))
    (pad 3 smd rect (at -4.2 -2.28) (size 2.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 2.1 0) (size 6.4 5.8) (layers B.Cu B.Mask)
      (net 5 /VOUT))
    (pad "" smd rect (at 3.775 -1.525) (size 3.05 2.75) (layers B.Paste))
    (pad "" smd rect (at 0.425 1.525) (size 3.05 2.75) (layers B.Paste))
    (pad "" smd rect (at 3.775 1.525) (size 3.05 2.75) (layers B.Paste))
    (pad "" smd rect (at 0.425 -1.525) (size 3.05 2.75) (layers B.Paste))
    (model ${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TO-252-3_TabPin2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_TopOnly (layer B.Cu) (tedit 56D1B4CB)
    (at 55 55)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference X1 (at 0 -5) (layer B.SilkS))
    (fp_text value Conn_01x01 (at 0 -4.2) (layer B.Fab))
    (fp_text user %R (at 0.3 0) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 10 "Net-(VD2-Pad2)"))
    (pad 1 connect circle (at 0 0) (size 6.4 6.4) (layers B.Cu B.Mask)
      (net 10 "Net-(VD2-Pad2)"))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_TopOnly (layer B.Cu) (tedit 56D1B4CB)
    (at 55 70)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference X2 (at 0 5) (layer B.SilkS))
    (fp_text value Conn_01x01 (at 0 -4.2) (layer B.Fab))
    (fp_text user %R (at 0.3 0) (layer B.Fab))
    (pad 1 connect circle (at 0 0) (size 6.4 6.4) (layers B.Cu B.Mask)
      (net 9 "Net-(VD2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 9 "Net-(VD2-Pad1)"))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_TopOnly (layer B.Cu) (tedit 56D1B4CB)
    (at 75 55)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference X3 (at -5 0) (layer B.SilkS))
    (fp_text value Conn_01x01 (at 0 -4.2) (layer B.Fab))
    (fp_text user %R (at 0.3 0) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 connect circle (at 0 0) (size 6.4 6.4) (layers B.Cu B.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_TopOnly (layer B.Cu) (tedit 56D1B4CB)
    (at 75 70)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference X4 (at -5 0) (layer B.SilkS))
    (fp_text value Conn_01x01 (at 0 -4.2) (layer B.Fab))
    (fp_text user %R (at 0.3 0) (layer B.Fab))
    (pad 1 connect circle (at 0 0) (size 6.4 6.4) (layers B.Cu B.Mask)
      (net 2 /COM))
    (pad 1 thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 /COM))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_TopOnly (layer B.Cu) (tedit 56D1B4CB)
    (at 120 55)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference X5 (at -5 0) (layer B.SilkS))
    (fp_text value Conn_01x01 (at 0 -4.2) (layer B.Fab))
    (fp_text user %R (at 0.3 0) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 5 /VOUT))
    (pad 1 connect circle (at 0 0) (size 6.4 6.4) (layers B.Cu B.Mask)
      (net 5 /VOUT))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_TopOnly (layer B.Cu) (tedit 56D1B4CB)
    (at 120 70)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference X6 (at -5 0) (layer B.SilkS))
    (fp_text value Conn_01x01 (at 0 -4.2) (layer B.Fab))
    (fp_text user %R (at 0.3 0) (layer B.Fab))
    (pad 1 connect circle (at 0 0) (size 6.4 6.4) (layers B.Cu B.Mask)
      (net 2 /COM))
    (pad 1 thru_hole circle (at 0 0) (size 3.6 3.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 /COM))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer B.Cu) (tedit 5F68FEEE)
    (at 119 60 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 1.5 1.65) (layer B.SilkS))
    (fp_text value "82 k" (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -1 0 180) (size 1.2 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.208333)
      (net 6 "Net-(R3-Pad1)"))
    (pad 2 smd roundrect (at 1 0 180) (size 1.2 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.208333)
      (net 5 /VOUT))
    (model ${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer B.Cu) (tedit 5F68FEEE)
    (at 119.031093 65.236172 15)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at -3.513733 1.402185 15) (layer B.SilkS))
    (fp_text value "15 k" (at 0 -1.65 15) (layer B.Fab))
    (fp_text user %R (at 0 0 15) (layer B.Fab))
    (pad 2 smd roundrect (at 1 0 15) (size 1.2 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.208333)
      (net 7 "Net-(R4-Pad1)"))
    (pad 1 smd roundrect (at -1 0 15) (size 1.2 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.208333)
      (net 2 /COM))
    (model ${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer B.Cu) (tedit 5F68FEEE)
    (at 112.5 67.9125 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 -2 90) (layer B.SilkS))
    (fp_text value "560 k" (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.208333)
      (net 8 "Net-(R4-Pad2)"))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.208333)
      (net 5 /VOUT))
    (model ${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P20.32mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 90 55)
    (descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=20.32mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
    (tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 20.32mm 2W length 11.9mm diameter 4.5mm")
    (fp_text reference R2 (at 10.16 -3.37) (layer F.SilkS))
    (fp_text value "1 k" (at 10.16 3.37) (layer F.Fab))
    (fp_text user %R (at 10.16 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 20.32 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 /VOUT))
    (model ${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P20.32mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 50 75) (end 50 50) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125 75) (end 50 75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125 50) (end 125 75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 50 50) (end 125 50) (layer Edge.Cuts) (width 0.05))
  (zone (net 5) (net_name /VOUT) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.25 53.75) (xy 118.5 58.5) (xy 118.5 61.5) (xy 117 63) (xy 109 63)
        (xy 109 54) (xy 112 51) (xy 120.5 51)
      )
    )
  )
  (zone (net 2) (net_name /COM) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 87 66.5) (xy 97 66.5) (xy 100.5 70) (xy 118.5 70) (xy 121.75 66.75)
        (xy 125 66.75) (xy 125 75) (xy 65 75) (xy 65 67.5) (xy 70 62.5)
        (xy 83 62.5)
      )
    )
  )
)
