(kicad_pcb (version 20171130) (host pcbnew 5.1.9+dfsg1-1)
  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 35)
    (zones 0)
    (modules 19)
    (nets 9)
  )
  (page A4)
  (title_block
    (title "Geawvat Adjustable Current Regulator PCB")
    (date 2022-02-25)
    (company "Ivan Shmakov")
    (comment 1 "CC BY-SA 3.0+")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.8)
    (user_trace_width 1.25)
    (trace_clearance 0.25)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 1.5)
    (via_drill 0.8)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5.5 5.5)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 /COM)
  (net 3 "Net-(C3-Pad2)")
  (net 4 "Net-(R1-Pad1)")
  (net 5 "Net-(R3-Pad2)")
  (net 6 "Net-(R5-Pad1)")
  (net 7 /VOUT)
  (net 8 "Net-(XP1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.25)
    (trace_width 0.8)
    (via_dia 1.5)
    (via_drill 0.8)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /COM)
    (add_net /VOUT)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(XP1-Pad3)")
  )
  (module MountingHole:MountingHole_3.2mm_M3_ISO14580_Pad (layer B.Cu) (tedit 56D1B4CB)
    (at 115 60)
    (descr "Mounting Hole 3.2mm, M3, ISO14580")
    (tags "mounting hole 3.2mm m3 iso14580")
    (attr virtual)
    (fp_text reference REF** (at 0 3.75) (layer B.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO14580_Pad (at 0 -3.75) (layer B.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3_ISO14580_Pad (layer B.Cu) (tedit 56D1B4CB)
    (at 115 115)
    (descr "Mounting Hole 3.2mm, M3, ISO14580")
    (tags "mounting hole 3.2mm m3 iso14580")
    (attr virtual)
    (fp_text reference REF** (at 0 3.75) (layer B.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO14580_Pad (at 0 -3.75) (layer B.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 /COM))
  )
  (module MountingHole:MountingHole_3.2mm_M3_ISO14580_Pad (layer B.Cu) (tedit 56D1B4CB)
    (at 60 115)
    (descr "Mounting Hole 3.2mm, M3, ISO14580")
    (tags "mounting hole 3.2mm m3 iso14580")
    (attr virtual)
    (fp_text reference REF** (at 0 3.75) (layer B.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO14580_Pad (at 0 -3.75) (layer B.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3_ISO14580_Pad (layer B.Cu) (tedit 56D1B4CB)
    (at 60 60)
    (descr "Mounting Hole 3.2mm, M3, ISO14580")
    (tags "mounting hole 3.2mm m3 iso14580")
    (attr virtual)
    (fp_text reference REF** (at 0 3.75) (layer B.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO14580_Pad (at 0 -3.75) (layer B.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 /COM))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 77.46 60 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference VD1 (at 2.489713 1.444413 180) (layer F.SilkS))
    (fp_text value KPH-1608SEC (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(R1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /COM))
    (model ${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Alps_RK163_Single_Horizontal (layer F.Cu) (tedit 5A3D4993)
    (at 121 110)
    (descr "Potentiometer, horizontal, Alps RK163 Single, http://www.alps.com/prod/info/E/HTML/Potentiometer/RotaryPotentiometers/RK16/RK16_list.html")
    (tags "Potentiometer horizontal Alps RK163 Single")
    (fp_text reference R4 (at -1 5) (layer F.SilkS))
    (fp_text value "50 k" (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 -10) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 0 -5) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 "Net-(R3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 "Net-(R3-Pad2)"))
    (model ${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alps_RK163_Single_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 120 87.5)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference X2 (at -3.32 1.46) (layer B.SilkS))
    (fp_text value Conn_01x01 (at 0 -4.2) (layer B.Fab))
    (fp_text user %R (at 0.3 0) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /VOUT))
    (model ${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 120 92.5)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference X3 (at -3.32 -1.5) (layer B.SilkS))
    (fp_text value Conn_01x01 (at 0 -4.2) (layer B.Fab))
    (fp_text user %R (at 0.3 0) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /COM))
    (model ${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D12.5mm_P5.00mm (layer F.Cu) (tedit 5AE50EF1)
    (at 75 75 90)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=12.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 12.5mm Electrolytic Capacitor")
    (fp_text reference C1 (at 2.5 -7.5 90) (layer F.SilkS))
    (fp_text value 47 (at 2.5 7.5 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 /COM))
    (model ${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D12.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder (layer B.Cu) (tedit 5F68FEEF)
    (at 85 74.1375 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0.6375 1.5 90) (layer B.SilkS))
    (fp_text value 1 (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 /COM))
    (model ${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_10x12.6 (layer B.Cu) (tedit 5BCA39D1)
    (at 93 79.5 270)
    (descr "SMD capacitor, aluminum electrolytic, Panasonic F12, 10.0x12.6mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C3 (at 0 6.2 90) (layer B.SilkS))
    (fp_text value 330 (at 0 -6.2 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -4.35 0 270) (size 4.4 1.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.131579)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at 4.35 0 270) (size 4.4 1.9) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.131579)
      (net 3 "Net-(C3-Pad2)"))
    (model ${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_10x12.6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer B.Cu) (tedit 5F68FEEE)
    (at 80 74.0875 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at -0.5875 1.5 90) (layer B.SilkS))
    (fp_text value "1.8 k" (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(R1-Pad1)"))
    (pad 2 smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer B.Cu) (tedit 5F68FEEE)
    (at 101 84.5 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at -0.5 -2) (layer B.SilkS))
    (fp_text value 360 (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -1 0 180) (size 1.2 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.208333)
      (net 2 /COM))
    (pad 2 smd roundrect (at 1 0 180) (size 1.2 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.208333)
      (net 3 "Net-(C3-Pad2)"))
    (model ${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer B.Cu) (tedit 5F68FEEE)
    (at 105 81 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 1.65 90) (layer B.SilkS))
    (fp_text value "560 k" (at 0 -1.65 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.208333)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.208333)
      (net 5 "Net-(R3-Pad2)"))
    (model ${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer B.Cu) (tedit 5F68FEEE)
    (at 105 97.5)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 1.65) (layer B.SilkS))
    (fp_text value "1.8 k" (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1 0) (size 1.2 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.208333)
      (net 5 "Net-(R3-Pad2)"))
    (pad 1 smd roundrect (at -1 0) (size 1.2 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.208333)
      (net 6 "Net-(R5-Pad1)"))
    (model ${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_MiniMELF_Handsoldering (layer B.Cu) (tedit 5905D919)
    (at 100 78 270)
    (descr "Diode Mini-MELF (SOD-80) Handsoldering")
    (tags "Diode Mini-MELF (SOD-80) Handsoldering")
    (attr smd)
    (fp_text reference VD2 (at -3 -2.5 90) (layer B.SilkS))
    (fp_text value "BZV55 C3V3" (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -2.75 0 270) (size 3.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2.75 0 270) (size 3.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C3-Pad2)"))
    (model ${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-89-3_Handsoldering (layer B.Cu) (tedit 5C33D6DD)
    (at 97.5 91 180)
    (descr "SOT-89-3 Handsoldering")
    (tags "SOT-89-3 Handsoldering")
    (attr smd)
    (fp_text reference VT1 (at 0.3 3.5) (layer B.SilkS))
    (fp_text value Q_PNP_BCE (at 0.3 -3.5) (layer B.Fab))
    (fp_text user %R (at 0.5 0 270) (layer B.Fab))
    (pad 1 smd rect (at -2.15 1.5 180) (size 2.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C3-Pad2)"))
    (pad 3 smd rect (at -2.15 -1.5 180) (size 2.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(R5-Pad1)"))
    (pad 2 smd custom (at -2.0625 0 180) (size 2.475 0.9) (layers B.Cu B.Paste B.Mask)
      (net 7 /VOUT) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 1.2375 0.8665) (xy 5.3625 0.8665) (xy 5.3625 -0.8665) (xy 1.2375 -0.8665)) (width 0))
      ))
    (model ${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-89-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_BarrelJack:BarrelJack_Horizontal (layer F.Cu) (tedit 5A1DBF6A)
    (at 66 75)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference XP1 (at -8.45 5.75) (layer F.SilkS))
    (fp_text value Barrel_Jack_Switch (at -6.2 -5.5) (layer F.Fab))
    (fp_text user %R (at -3 -2.95) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole roundrect (at -6 0) (size 3 3.5) (drill oval 1 3) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 2 /COM))
    (pad 3 thru_hole roundrect (at -3 4.7) (size 3.5 3.5) (drill oval 3 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(XP1-Pad3)"))
    (model ${KICAD6_3DMODEL_DIR}/Connector_BarrelJack.3dshapes/BarrelJack_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal (layer F.Cu) (tedit 5C13907B)
    (at 112.5 75 270)
    (descr http://www.farnell.com/datasheets/612848.pdf)
    (tags "BNC Amphenol Horizontal")
    (fp_text reference XS1 (at 0 4 270) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 6 90) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 thru_hole oval (at -5.08 -5.08 270) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 2 /COM))
    (pad 2 thru_hole oval (at 5.08 -5.08 270) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 2 /COM))
    (pad 1 thru_hole oval (at 0 0 270) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 7 /VOUT))
    (pad 2 thru_hole oval (at -2.54 0 270) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 2 /COM))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/BNC_Amphenol_B6252HB-NPP3G-50_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 50 125) (end 50 50) (layer Edge.Cuts) (width 0.5))
  (gr_line (start 125 125) (end 50 125) (layer Edge.Cuts) (width 0.5))
  (gr_line (start 125 50) (end 125 125) (layer Edge.Cuts) (width 0.5))
  (gr_line (start 50 50) (end 125 50) (layer Edge.Cuts) (width 0.5))
  (zone (net 2) (net_name /COM) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.45)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 125 125) (xy 50 125) (xy 50 50) (xy 125 50)
      )
    )
  )
)
